;*******************************************************************************
; Copyright 2001-2006 Broadcom Corporation.
;
; INF for NTamd64.6.0 Windows Longhorn Beta
;
; InfVersion   10.9.0.0i
;
;*******************************************************************************

[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
CatalogFile = b57nd60a.cat
Compatible  = 1
Provider    = %BRCM%
DriverVer=04/04/2007,10.9.0.0

[Manufacturer]
%BRCM% = Broadcom, NTamd64.6.0

      
[Broadcom.NTamd64.6.0]
%3C998SX%           =  3C998SX_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_16A8&SUBSYS_200110B7
%3C998T%            =  3C998T_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1648&SUBSYS_200010B7
%3C999T%            =  3C999T_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1648&SUBSYS_300010B7
%BCM5703%           =  BCM5703_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1647
%BCM5703%           =  BCM5703_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_16a7
%BCM5703%           =  BCM5703_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_16C7
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5703SW%         =  BCM5703SW_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5704%           =  BCM5704_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1648
%BCM5704S%          =  BCM5704S_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_16A8
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02e81014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02e91014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_16A8&SUBSYS_03331014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1654
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014
%BCM5705%           =  BCM5705_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1653
%BCM5705F%          =  BCM5705F_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_166e
%BCM5705F%          =  BCM5705F_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_166e&SUBSYS_3000103c
%BCM5705FHA%        =  BCM5705F_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_166e&SUBSYS_1700103c
%BCM5705FHB%        =  BCM5705F_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_166e&SUBSYS_1703103c
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1654&SUBSYS_12f810cf
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_165E&SUBSYS_127910cf
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165E
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165E&SUBSYS_0727152d
%BCM5705M%          =  BCM5705M_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_165D
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1668
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_166A&SUBSYS_03131014
%BCM5714%           =  BCM5780_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_166A
%BCM5714%           =  BCM5780_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_166A&SUBSYS_107F1734
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1678
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1678&SUBSYS_032a1014
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1678&SUBSYS_108C1734
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1669
%BCM5714S%          =  BCM5714SHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1669&SUBSYS_03281014
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_166B
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1679
%BCM5714S%          =  BCM5714SWol_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1679&SUBSYS_399710f1

%BCM5750A1%         =  BCM5750A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1%         =  BCM5750A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167D&SUBSYS_131510cf
%BCM5750A1%         =  BCM5750A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1%         =  BCM5750A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167D&SUBSYS_832a1033
%BCM5750A1%         =  BCM5750A1F3_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5750A1%         =  BCM5750A1F3_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1%         =  BCM5750A1F3_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1601
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD
%BCM5750A1%         =  BCM5750A1SPECIAL_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_81AA104D
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_108B1734
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_5047107b
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_5048107b
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_0280107b
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_0215107b
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_0460107b
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_0604107b
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_03301014
%BCM5750A1%         =  BCM5750A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1601&SUBSYS_202017AA
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1658
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1659
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1659&SUBSYS_02FE1014
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1659&SUBSYS_02C61014
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1676
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_00631025
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_10961734
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167C
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_16F7
%BCM5750A1%         =  BCM5750MHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_167D&SUBSYS_05771014
%BCM5750A1%         =  BCM5750MHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_167D&SUBSYS_208117AA
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01791028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1600&SUBSYS_01A71028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1600&SUBSYS_01A81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1600&SUBSYS_01AD1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C11028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1600&SUBSYS_01CF1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1600&SUBSYS_01C81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1600&SUBSYS_01C21028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1600&SUBSYS_01CC1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1600&SUBSYS_01D61028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1600&SUBSYS_01CE1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1600&SUBSYS_02011028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_019c1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_01E01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_1677&SUBSYS_02071028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_16F7&SUBSYS_01BF1028

%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_167A&SUBSYS_01da1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_167A&SUBSYS_01de1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_167A&SUBSYS_01e11028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,  PCI\VEN_14e4&DEV_167A&SUBSYS_01ec1028

%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167E
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167E&SUBSYS_01E41028
%BCM5750A1F%        =  BCM5750FHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014
%BCM5750A1STSP%     =  BCM5750A1STSP_LHinst.NTamd64.6.0,     PCI\VEN_14e4&DEV_1659&SUBSYS_3260103c
%BCM5750B0%         =  BCM5750B0MHAL_LHinst.NTamd64.6.0,     PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_10
%BCM5750B0F%        =  BCM5750B0MFHAL_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_10
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01

%BCM5754%           =  BCM5754A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A
%BCM5754%           =  BCM5754A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1672
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1672&SUBSYS_02021028

%BCM5755%           =  BCM5755A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1673
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1673&SUBSYS_01fa1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1673&SUBSYS_01f91028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1673&SUBSYS_02061028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1673&SUBSYS_01fe1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0, PCI\VEN_14e4&DEV_1673&SUBSYS_01ff1028

%BCM5755%           =  BCM5755A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167B       
%BCM5755%           =  BCM5755A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167B&SUBSYS_10B21734
%BCM5755%           =  BCM5755A1EStar_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_167B&SUBSYS_2808103c
%BCM5755%           =  BCM5755A1EStar_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_167B&SUBSYS_280A103c
%BCM5755%           =  BCM5755A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167B&SUBSYS_280C103c
%BCM5755%           =  BCM5755A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167B&SUBSYS_2817103c
%BCM5755%           =  BCM5755A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167B&SUBSYS_100C17AA
%BCM5755%           =  BCM5755A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167B&SUBSYS_100F17AA
%BCM5755%           =  BCM5755A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167B&SUBSYS_101017AA
%BCM5755%           =  BCM5755A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167B&SUBSYS_101117AA
%BCM5755%           =  BCM5755A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167B&SUBSYS_101317AA
%BCM5755%           =  BCM5755A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_167B&SUBSYS_866917AA

%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1696
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1696&SUBSYS_12bb103c
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1696&SUBSYS_12bc103c
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1696&SUBSYS_000c103c
%BCM5786%           =  BCM5787A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169A
%BCM5786%           =  BCM5787A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169A&SUBSYS_101517aa
%BCM5786%           =  BCM5787A1F3_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_169A&SUBSYS_13ee10cf

%BCM5787%           =  BCM5787A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169B
%BCM5787%           =  BCM5787A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_169B&SUBSYS_203017AA
%BCM5787%           =  BCM5787A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_169B&SUBSYS_100D17AA
%BCM5787%           =  BCM5787A1HAL_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_169B&SUBSYS_100E17AA
%BCM5787%           =  BCM5787A1F3_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_169B&SUBSYS_139810cf
%BCM5787%           =  BCM5787A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693
%BCM5787M%          =  BCM5787A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_30c0103c
%BCM5787M%          =  BCM5787A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_30c2103c
%BCM5787%           =  BCM5787MHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_203017AA
%BCM5787%           =  BCM5787MHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_20d517AA
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_386017AA
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_139910cf

%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88111033
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88121033
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88361033
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88421033
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88611033
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88621033
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88631033
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88741033
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_88831033

%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_011A1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_011B1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_011C1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_011D1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_011E1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_011F1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01211025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01221025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01231025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01241025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01251025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01261025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01271025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01281025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01291025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_012A1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_012B1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_012C1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_012D1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_012E1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_012F1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,    PCI\VEN_14e4&DEV_1693&SUBSYS_01301025

%BCM5787F%          =  BCM5750A1F_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167F
%BCM5787F%          =  BCM5750A1F_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167F&SUBSYS_30c0103C
%BCM5787F%          =  BCM5750A1F_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167F&SUBSYS_30c2103C

%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c
%BCM5788%           =  BCM5788F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169C&SUBSYS_123c10cf
%BCM5788%           =  BCM5788F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169C&SUBSYS_12f710cf
%BCM5788%           =  BCM5788F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169c&SUBSYS_82fa1033
%BCM5788%           =  BCM5788F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169c&SUBSYS_83011033
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_c016144d
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_101717aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_101817aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_101a17aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_101b17aa
%BCM5789%           =  BCM5789F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169d&SUBSYS_12ff10cf
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169d
%BCM5789%           =  BCM5789F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169d&SUBSYS_83101033
%BCM5789%           =  BCM5789F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169d&SUBSYS_83321033
%BCM5789%           =  BCM5789F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169d&SUBSYS_833a1033
%BCM5789%           =  BCM5789F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169d&SUBSYS_881b1033
%BCM5789%           =  BCM5789F1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169d&SUBSYS_881c1033
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169d&SUBSYS_0280107b
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169d&SUBSYS_100317AA
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169d&SUBSYS_100517AA
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169d&SUBSYS_060017FF
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_16DD
%BCM5750B0%         =  BCM5750B0M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FF
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_170D
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_170E
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_170E&SUBSYS_05451014

%BCM5906%           =  BCM5906_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1712
%BCM5906_ID4_FEA%   =  BCM5906Star_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1712&SUBSYS_2816103c
%BCM5906_ID4_FEB%   =  BCM5906Star_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1712&SUBSYS_170f103c

%BCM5906M%          =  BCM5906M_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1713
%BCM5906MH%         =  BCM5906M_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1713&SUBSYS_30c0103C
%BCM5906MH%         =  BCM5906M_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1713&SUBSYS_30c2103C
%BCM5906_ID4_FEA%   =  BCM5906Mstar_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1713&SUBSYS_2816103c
%BCM5906_ID4_FEB%   =  BCM5906Mstar_LHinst.NTamd64.6.0,      PCI\VEN_14e4&DEV_1713&SUBSYS_170f103c
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1713&SUBSYS_386117AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1713&SUBSYS_3C2C17AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1713&SUBSYS_400617AA
%BCM5906M%          =  BCM5906F3M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1713&SUBSYS_143410CF
%BCM5906M%          =  BCM5906F3M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1713&SUBSYS_171310CF
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1713&SUBSYS_01F31028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1713&SUBSYS_02271028
%OEM1_DEV4%			= OEM1_DEV4_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV4%			= OEM1_DEV4_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV4%			= OEM1_DEV4_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV4%			= OEM1_DEV4_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028

%OEM1_DEV5%			= OEM1_DEV5_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5%			= OEM1_DEV5_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_165E&SUBSYS_865d1028
%OEM1_DEV5%			= OEM1_DEV5_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV5%			= OEM1_DEV5_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_165E&SUBSYS_20031028
%OEM1_DEV6%			= OEM1_DEV6_LHinst.NTamd64.6.0,		   PCI\VEN_14e4&DEV_1653&SUBSYS_86531028


%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D&SUBSYS_0a0c103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D&SUBSYS_3095103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D&SUBSYS_3098103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167D&SUBSYS_3099103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_3095103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_3098103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_3099103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_309F103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_30ac103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_30ad103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_30a3103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_30a2103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16FD&SUBSYS_30b1103C
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_3014103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c&REV_00
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169C&SUBSYS_099c103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_308b103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_308e103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_3095103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_3098103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_3099103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_30aa103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_30a1103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_30b0103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169c&SUBSYS_3021103c
%OEM2_DEV1%         =  BCM5705M_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_165d&SUBSYS_00580E11
%OEM2_DEV1%         =  BCM5705M_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_165d&SUBSYS_005A0E11
%OEM3_DEV1%         =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165e&SUBSYS_0890103c
%OEM3_DEV1%         =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165e&SUBSYS_0a0c103c
%OEM3_DEV2%         =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165e&SUBSYS_0894103c
%OEM3_DEV3%         =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165e&SUBSYS_088c103c
%OEM3_DEV4%         =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165e&SUBSYS_08bc103c
%OEM3_DEV4%         =  BCM5705MA2_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_165e&SUBSYS_099c103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_3013103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_3015103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_12f2103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_3008103c
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_3002103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c&REV_00


;;------ MSI support ------
[BCM5750_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1HAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5780_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714S_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714SHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714SWol_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1STSP_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5789_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5789F1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750B0MHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750B0MFHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750B0M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1SPECIAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5754A1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5754A1M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1Estar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1HAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1HAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1F3_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1F3M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787MHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787MHALe_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750MHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1MBDFS_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1F_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750FHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1CLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1CLDeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1F3_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1F3M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5901_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5788_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5788F1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906MHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906F3M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906Star_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906Mstar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906MD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd
;;------ end of MSI support ----
[BCM5703_LHinst.NTamd64.6.0]
DelReg          = DelReg_Generic
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5703_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5704_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.WolS
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5704_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5705_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLMagic, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1HAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1HAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
DelReg          = DelReg_Generic, DelReg.Wol
DelReg          = DelReg_Generic, DelReg.WolMagic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5714_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5780_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSndJumboCombo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5780_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5714S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5714S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5714SWol_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsWOLTbi
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5714SWol_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714SHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo , ParamsWOLTbi
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5714SHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog




[BCM5750A1STSP_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1STSP_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5789_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo , DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5789_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5789F1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo , DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5789F1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750B0MHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750B0MHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750B0MFHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.ClockControl
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750B0MFHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog




[BCM5750B0M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750B0M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1SPECIAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xSPECIAL, ParamsCSPECIAL, ParamsWOL, ParamsWireSpeedSPECIAL, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1SPECIAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750A1M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5754A1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5754A1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo
AddReg          = LH_AddReg, BCM5750.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5754A1M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4


[BCM5754A1M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1Estar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WolS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1Estar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS


[BCM5755A1M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog
[BCM5755A1HAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS


[BCM5755A1HAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787A1HAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1HAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787A1F3_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.ClockControl
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787A1F3M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.ClockControl
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787A1M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1MBDFS_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4


[BCM5787A1MBDFS_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog




[BCM5787MHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787MHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787MHALe_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787MHALe_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750MHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750MHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.ClockControl
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1F_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750FHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.ClockControl
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750FHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1CLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg_CLNAHKD_1, DelReg.Jumbo
AddReg          = LH_AddReg, BCM5750.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1CLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1CLDeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg_CLNAHKD_1, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1CLDeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.ClockControl
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1F3_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750A1F3M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.ClockControl
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5750A1F3M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705M.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5705M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705F_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705F.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5705F_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705A2_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5705A2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5705A2_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705MA2_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5705MA2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5705MA2_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705MA2F2_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5705MA2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5705MA2F2_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5901_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5901.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5901_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5788_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5788_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5788F1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5788F1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5703S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5703S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5703SW_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5703SW_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5704S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5704S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5704SW_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5704SW_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[3C998T_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[3C998T_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[3C998SX_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[3C998SX_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[3C999T_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[3C999T_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[OEM1_DEV4_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, OEM1_DEV4.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[OEM1_DEV4_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[OEM1_DEV5_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, OEM1_DEV5.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[OEM1_DEV5_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[OEM1_DEV6_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, OEM1_DEV6.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[OEM1_DEV6_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5906_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5906_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5906M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5906M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5906MD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed, DelReg.Wol, DelReg.LAA, DelReg.TaskOffload
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, 5906MClnahkdXP.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified
[BCM5906MD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog
[BCM5906MHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5906MHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5906F3M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ClockControl, DelReg.LsoV1IPv4
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5906F3M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906Mstar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed, DelReg.WolS
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5906Mstar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5906Star_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.WireSpeed, DelReg.WolS
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 0          ; NdisPhysicalMediumUnspecified

[BCM5906Star_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog
;*******************************************************************************
; 32-bit Windows Longhorn common sections.
;*******************************************************************************

[LH_AddReg]
HKR, Ndi,            Service,    0, "b57nd60a"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Intr_coal]
HKR, Ndi\Params\*InterruptModeration,        ParamDesc, , %ParamDesc_InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,        default,   , "1"
HKR, Ndi\Params\*InterruptModeration,        type,      , "enum"
HKR, Ndi\Params\*InterruptModeration\enum,   0,         , %GenDisable%
HKR, Ndi\Params\*InterruptModeration\enum,   1,         , %GenEnable%

[MsiSupportStd]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties",	MSISupported, 0x00010001, 1

[LH_EventLog]
AddReg = LH_AddEventLogReg

[LH_AddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57nd60a.sys"
HKR, , TypesSupported  , 0x00010001, 7


[BRCM_LH_Service]
DisplayName    = %SvcDispName%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57nd60a.sys
LoadOrderGroup = NDIS

;*******************************************************************************
; Registry parameters.
;*******************************************************************************

[BCM5701.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5702.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5703.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5704.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705M.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705F.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705A2.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705MA2.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5901.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5788.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[OEM1_DEV4.Params]
HKR, , AdminSettingsLevel,		 0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *LsoV1IPv4,               0, "0"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV5.Params]
HKR, , AdminSettingsLevel,		 0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *LsoV1IPv4,               0, "1"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV6.Params]
HKR, , AdminSettingsLevel,		 0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *LsoV1IPv4,               0, "1"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[ClnahkdXP.Params]
HKR, , AdminSettingsLevel,		 0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *LsoV1IPv4,               0, "1"
HKR, , RxMtu,                    0, "1514"
HKR, , WireSpeed,                0, "1"
HKR, , *InterruptModeration,     0, "1"

[ParamsGSOv4]
HKR, Ndi\Params\*LsoV2IPv4,        ParamDesc, , %ParamDesc_GSOv4%
HKR, Ndi\Params\*LsoV2IPv4,        default,   , "1"
HKR, Ndi\Params\*LsoV2IPv4,        type,      , "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*LsoV2IPv4\enum,   "1",       , %GenEnable%

[ParamsGSOv6]
HKR, Ndi\Params\*LsoV2IPv6,        ParamDesc, , %ParamDesc_GSOv6%
HKR, Ndi\Params\*LsoV2IPv6,        default,   , "1"
HKR, Ndi\Params\*LsoV2IPv6,        type,      , "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*LsoV2IPv6\enum,   "1",       , %GenEnable%


[ParamsRSS]
HKR, Ndi\Params\*RSS,        ParamDesc, , %ParamDesc_RSS%
HKR, Ndi\Params\*RSS,        default,   , "1"
HKR, Ndi\Params\*RSS,        type,      , "enum"
HKR, Ndi\Params\*RSS\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*RSS\enum,   "1",       , %GenEnable%
[5906MClnahkdXP.Params]
HKR, , AdminSettingsLevel,		 0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *InterruptModeration,     0, "1"

[ParamsNt]
HKR, , AdminSettingsLevel,		 0, "2"

HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4,        ParamDesc, , %ParamDesc_TCPUDPChecksumOffloadIPv4%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4,        default,   , "3"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4,        type,      , "enum"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4\enum,   "1",       , %GenTxEnable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4\enum,   "2",       , %GenRxEnable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4\enum,   "3",       , %GenTxRxEnable%

[ParamsNtv6Tx]
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        ParamDesc, , %ParamDesc_TCPUDPChecksumOffloadIPv6%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        default,   , "1"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        type,      , "enum"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "1",       , %GenTxEnable%

[ParamsNtv6TxRx]
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        ParamDesc, , %ParamDesc_TCPUDPChecksumOffloadIPv6%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        default,   , "3"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        type,      , "enum"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "1",       , %GenTxEnable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "2",       , %GenRxEnable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "3",       , %GenTxRxEnable%

[ParamsNT8021p]
HKR, Ndi\Params\*PriorityVLANTag,  ParamDesc,  , "Priority & VLAN"
HKR, Ndi\Params\*PriorityVLANTag,      default,, "3"
HKR, Ndi\Params\*PriorityVLANTag,      type,   , "enum"
HKR, Ndi\Params\*PriorityVLANTag\enum, 0,      , "Priority & VLAN Disabled"
HKR, Ndi\Params\*PriorityVLANTag\enum, 1,      , "Priority Enabled"
HKR, Ndi\Params\*PriorityVLANTag\enum, 2,      , "VLAN Enabled"
HKR, Ndi\Params\*PriorityVLANTag\enum, 3,      , "Priority & VLAN Enabled"

HKR, Ndi\params\VlanID,     ParamDesc,       0, %VlanID%
HKR, Ndi\params\VlanID,     default,         0, "0"
HKR, Ndi\params\VlanID,     type,            0, "long"
HKR, Ndi\params\VlanID,     min,             0, "0"
HKR, Ndi\params\VlanID,     max,             0, "4095"
HKR, Ndi\params\VlanID,     step,            0, "1"
HKR, Ndi\params\VlanID,     base,            0, "10"

[ParamsNtW9x]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "2147483648"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\*FlowControl\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"


[ParamsNtW9xFJ]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "0"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\*FlowControl\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"



[ParamsNtW9xMOBILE]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "2147483648"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\*FlowControl\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2147483648, , %FlowControl_Auto%


[ParamsNtW9xSPECIAL]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "2147483648"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

[ParamsJumbo]
HKR, Ndi\Params\RxMtu, ParamDesc, , %JumboMtu%
HKR, Ndi\Params\RxMtu, default,   , "1500"
HKR, Ndi\Params\RxMtu, type,      , "dword"
HKR, Ndi\Params\RxMtu, min,       , "1500"
HKR, Ndi\Params\RxMtu, max,       , "9000"
HKR, Ndi\Params\RxMtu, step,      , "500"
HKR, Ndi\Params\RxMtu, base,      , "10"

[ParamsWireSpeed]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%


[ParamsWOLLink]
HKR, Ndi\Params\WakeOnLink,        ParamDesc, , %WakeOnLink%
HKR, Ndi\Params\WakeOnLink,        default,   , "0"
HKR, Ndi\Params\WakeOnLink,        type,      , "enum"
HKR, Ndi\Params\WakeOnLink\enum,   0,         , %WakeOnLink_Disable%
HKR, Ndi\Params\WakeOnLink\enum,   1,         , %WakeOnLink_Enable%



[ParamsWireSpeedSPECIAL]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%

[ParamsLogOptions]
HKR, Ndi\Params\LogLevelInfo,        ParamDesc, , %LogLevelInfo%
HKR, Ndi\Params\LogLevelInfo,        default,   , "0"
HKR, Ndi\Params\LogLevelInfo,        type,      , "enum"
HKR, Ndi\Params\LogLevelInfo\enum,   0,         , %LogLevelInfo_Disable%
HKR, Ndi\Params\LogLevelInfo\enum,   1,         , %LogLevelInfo_Enable%
HKR, Ndi\Params\LogLevelWarn,        ParamDesc, , %LogLevelWarn%
HKR, Ndi\Params\LogLevelWarn,        default,   , "0"
HKR, Ndi\Params\LogLevelWarn,        type,      , "enum"
HKR, Ndi\Params\LogLevelWarn\enum,   0,         , %LogLevelWarn_Disable%
HKR, Ndi\Params\LogLevelWarn\enum,   1,         , %LogLevelWarn_Enable%


[ParamsC]
HKR, Ndi\Params\*SpeedDuplex,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\*SpeedDuplex,      default,   , "0"
HKR, Ndi\Params\*SpeedDuplex,      type,      , "enum"
HKR, Ndi\Params\*SpeedDuplex\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 1,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 2,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\*SpeedDuplex\enum, 3,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 4,         , %Speed_Duplex_100Mb_Fd%

[ParamsCSPECIAL]
HKR, Ndi\Params\*SpeedDuplex,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\*SpeedDuplex,      default,   , "0"
HKR, Ndi\Params\*SpeedDuplex,      type,      , "enum"
HKR, Ndi\Params\*SpeedDuplex\enum, 0,         , %Speed_Duplex_Auto%

[ParamsC100]
HKR, Ndi\Params\*SpeedDuplex,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\*SpeedDuplex,      default,   , "0"
HKR, Ndi\Params\*SpeedDuplex,      type,      , "enum"
HKR, Ndi\Params\*SpeedDuplex\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 1,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 2,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\*SpeedDuplex\enum, 3,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 4,         , %Speed_Duplex_100Mb_Fd%


[ParamsWOL]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%

[ParamsWOLeStar]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "256"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,       , %WolSpeed_LowestAvail%

HKR, , WolSpeed, 0, "256"

[eStar]
HKR, , WolSpeed, 0, "256"

[ParamsM]
HKR, , ClockControl,          0, "1"

[ParamsWOLTbi]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, , TbiWol,                   0, "1"

[ParamsLgSnd]
;; Vista
HKR, Ndi\Params\*LsoV1IPv4,        ParamDesc, , %ParamDesc_LSOv4%
HKR, Ndi\Params\*LsoV1IPv4,        default,   , "1"
HKR, Ndi\Params\*LsoV1IPv4,        type,      , "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*LsoV1IPv4\enum,   "1",       , %GenEnable%

[ParamsWOLNS]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

[ParamsFlow]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "2147483648"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\*FlowControl\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2147483648, , %FlowControl_Auto%


[ParamsLgSndJumboCombo]
HKR, , *LsoV1IPv4,                   0, "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    ParamDesc, , %TaskOffload_LargeSend_Jumbo%
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    default,   , "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 0,        , %TaskOffload_LargeSend_Disable_Both%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 1,        , %TaskOffload_LargeSend_Enable_JumboDisable%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 2,        , %TaskOffload_LargeSend_Disable_JumboEnable3000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 3,        , %TaskOffload_LargeSend_Disable_JumboEnable4500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 4,        , %TaskOffload_LargeSend_Disable_JumboEnable6000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 5,        , %TaskOffload_LargeSend_Disable_JumboEnable7500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 6,        , %TaskOffload_LargeSend_Disable_JumboEnable9000%

[ParamsWOLMagic]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%

;[ParamsWOL10M]
;HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
;HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
;HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
;HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
;HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
;HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
;HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

;HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
;HKR, Ndi\Params\WolSpeed,       default,   , "1"
;HKR, Ndi\Params\WolSpeed,       type,      , "enum"
;HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
;HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
;HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%


;*******************************************************************************
; DriverInfo section.
;*******************************************************************************

[DriverInfo]


;*******************************************************************************
; Keys to remove.
;*******************************************************************************

[DelReg_Generic]
;; Vista
HKR, , UserTaskOffloadCapDisable
HKR, ,          LargeSendOffload
HKR, Ndi\Params\LargeSendOffload

HKR, ,          InterruptModeration
HKR, Ndi\Params\InterruptModeration

HKR, ,          AdminSettingsLevel
HKR, Ndi\Params\AdminSettingsLevel

HKR, ,          RSS
HKR, Ndi\Params\RSS

HKR, ,          TaskOffloadCap
HKR, Ndi\Params\TaskOffloadCap

HKR, ,          *TCPChksumOffv4
HKR, Ndi\Params\*TCPChksumOffv4
HKR, ,          *UDPChksumOffv4
HKR, Ndi\Params\*UDPChksumOffv4
HKR, ,          *IPChksumOffv4
HKR, Ndi\Params\*IPChksumOffv4

HKR, ,          *TCPChksumOffv6
HKR, Ndi\Params\*TCPChksumOffv6
HKR, ,          *UDPChksumOffv6
HKR, Ndi\Params\*UDPChksumOffv6

HKR, ,          *TCPChecksumOffloadIPv4
HKR, Ndi\Params\*TCPChecksumOffloadIPv4
HKR, ,          *UDPChecksumOffloadIPv4
HKR, Ndi\Params\*UDPChecksumOffloadIPv4
HKR, ,          *IPChecksumOffloadIPv4
HKR, Ndi\Params\*IPChecksumOffloadIPv4

HKR, ,          *TCPChecksumOffloadIPv6
HKR, Ndi\Params\*TCPChecksumOffloadIPv6
HKR, ,          *UDPChecksumOffloadIPv6
HKR, Ndi\Params\*UDPChecksumOffloadIPv6

HKR, ,          *LSOv4
HKR, Ndi\Params\*LSOv4
HKR, ,          *GSOv4
HKR, Ndi\Params\*GSOv4
HKR, ,          *GSOv6
HKR, Ndi\Params\*GSOv6

HKR, ,          FlowControlCap
HKR, Ndi\Params\FlowControlCap
HKR, Ndi\Params\RequestedMediaType
HKR, Ndi\Params\*SpeedDuplex
HKR, Ndi\Params\Enable8021p
HKR, NDI\params\*NetworkAddress

[DelReg_CLNAHKD]
HKR, Ndi\Params\*InterruptModeration
HKR, ,          WolSpeed
HKR, Ndi\Params\WolSpeed
HKR, ,          WakeOnLink
HKR, Ndi\Params\WakeOnLink
HKR, ,          LogLevelInfo
HKR, Ndi\Params\LogLevelInfo
HKR, ,          *RSS
HKR, Ndi\Params\*RSS

[DelReg_CLNAHKD_1]
HKR, ,          *LsoV2IPv6
HKR, Ndi\Params\*LsoV2IPv6
HKR, ,          *LsoV2IPv4
HKR, Ndi\Params\*LsoV2IPv4
HKR, ,          *TCPUDPChecksumOffloadIPv6
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6

[DelReg.RequestedMediaType]
HKR, Ndi\Params\RequestedMediaType
HKR, Ndi\Params\*SpeedDuplex
HKR, Ndi\Params\Enable8021p

[DelReg.Wol]
HKR, Ndi\Params\WolSpeed
HKR, Ndi\Params\WakeUpModeCap

[DelReg.WolS]
HKR, Ndi\Params\WolSpeed

[DelReg.WolMagic]
HKR, Ndi\Params\WakeUpModeCap
HKR, Ndi\Params\WolSpeed

[DelReg.Jumbo]
HKR, Ndi\Params\RxMtu

[DelReg.LgSnd]
HKR, Ndi\Params\LargeSendOffload

[DelReg.LsoV1IPv4]
HKR, Ndi\Params\*LsoV1IPv4
HKR, ,          *LsoV1IPv4

[DelReg.WireSpeed]
HKR, Ndi\Params\WireSpeed

[DelReg.ClockControl]
HKR, ,ClockControl

[DelReg.LAA]
HKR, Ndi\params\*NetworkAddress
HKR, , *NetworkAddress
HKR, Ndi\params\NetworkAddress
HKR, , NetworkAddress

[DelReg.TaskOffload]
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 11
CopyFile_Binary = 12

[SourceDisksNames]
1 = %DISK_DESC%,,,

[SourceDisksFiles]
b57nd60a.sys = 1

[CopyFile_Binary]
b57nd60a.sys,,,1


;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
BRCM                = "Broadcom"
SvcDispName         = "Broadcom NetXtreme Gigabit Ethernet - NDIS 6.0"
DISK_DESC           = "Broadcom NetXtreme Installation Media"

BCM5700             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5701             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5702             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5703             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705F            = "Broadcom 570x 10/100 Integrated Controller"
BCM5750             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1F          = "Broadcom NetXtreme Fast Ethernet"
BCM5751A1           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5714             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5714S            = "Broadcom NetXtreme Gigabit Fiber"

BCM5786             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787F            = "Broadcom NetLink (TM) Fast Ethernet"
BCM5787M            = "Broadcom NetLink Gigabit Ethernet"
BCM5755             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5754             = "Broadcom NetXtreme Gigabit Ethernet"

BCM5750A1STSP       = "Embedded Broadcom NetXtreme 5721 PCI-E Gigabit NIC"

BCM5750B0           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750B0F          = "Broadcom NetXtreme Fast Ethernet"

BCM5901             = "Broadcom NetXtreme Fast Ethernet"
BCM5782             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5788             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5789             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5700FB           = "Broadcom NetXtreme Gigabit Fiber"
BCM5700FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5701FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5703S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5703SW           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5704SW           = "Broadcom NetXtreme Gigabit Ethernet"

3C998T              = "3Com Dual Port 10/100/1000 PCI-X Server NIC"
3C998SX             = "3Com Dual Port 1000-SX PCI-X Server NIC"
3C999T              = "3Com Quad Port 10/100/1000 PCI-X Server NIC"

OEM1_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV4           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV5           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"
OEM2_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV4           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV5           = "Broadcom 570x 10/100 Integrated Controller"
OEM3_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV6A1       = "Broadcom NetXtreme Gigabit Ethernet"

BCM5750A1DSF      = "Broadcom NetXtreme 5751 Gigabit Controller"
BCM5750A1DSSF    = "Broadcom NetXtreme 5721 Gigabit Controller"
BCM5750A1DDT      = "Broadcom NetXtreme 57xx Gigabit Controller"
BCM5750A1CLNAHKD =  "Broadcom NetXtreme 57xx Gigabit Controller"

BCM5906             = "Broadcom NetLink (TM) Fast Ethernet"
BCM5906MH           = "Broadcom 590x 10/100 Ethernet"
BCM5906M            = "Broadcom NetLink (TM) Fast Ethernet"
OEM1_DEV7           = "Broadcom 570x Gigabit Integrated Controller"

BCM5705FHA            = "Broadcom NetXtreme FE-A"
BCM5705FHB            = "Broadcom NetXtreme FE-B"

BCM5906_ID4_FEA      = "Broadcom NetLink FE-A"
BCM5906_ID4_FEB      = "Broadcom NetLink FE-B"

JumboMtu = "Jumbo Mtu"

FlowControl             = "Flow Control"
FlowControl_Disable     = "Disable"
FlowControl_Rx_Pause    = "Rx PAUSE"
FlowControl_Tx_Pause    = "Tx PAUSE"
FlowControl_Rx_Tx_Pause = "Rx/Tx PAUSE"
FlowControl_Auto        = "Auto"

Speed_Duplex          = "Speed & Duplex"
Speed_Duplex_Auto     = "Auto"
Speed_Duplex_10Mb_Hd  = "10 Mb Half"
Speed_Duplex_10Mb_Fd  = "10 Mb Full"
Speed_Duplex_100Mb_Hd = "100 Mb Half"
Speed_Duplex_100Mb_Fd = "100 Mb Full"
Speed_Duplex_1000Mb_Fd = "1000 Mb Full"

QOS_8021p         = "802.1p QOS"
QOS_8021p_Disable = "Disable"
QOS_8021p_Enable  = "Enable"

WireSpeed         = "Ethernet@WireSpeed"
WireSpeed_Disable = "Disable"
WireSpeed_Enable  = "Enable"

WakeOnLink         = "Wake On Link"
WakeOnLink_Disable = "Disable"
WakeOnLink_Enable  = "Enable"

;; Vista
ParamDesc_RSS = "Receive Side Scaling"
ParamDesc_InterruptModeration = "Interrupt Moderation"
ParamDesc_IPChksumOffv4  = "IPv4 Checksum Offload"
ParamDesc_TCPChksumOffv4 = "TCP Checksum Offload (IPv4)"
ParamDesc_UDPChksumOffv4 = "UDP Checksum Offload (IPv4)"
ParamDesc_TCPChksumOffv6 = "TCP Checksum Offload (IPv6)"
ParamDesc_UDPChksumOffv6 = "UDP Checksum Offload (IPv6)"
ParamDesc_TCPUDPChecksumOffloadIPv4 = "TCP/UDP Checksum Offload (IPv4)"
ParamDesc_TCPUDPChecksumOffloadIPv6 = "TCP/UDP Checksum Offload (IPv6)"
ParamDesc_LSOv4          = "Large Send Offload (IPv4)"
ParamDesc_GSOv4          = "Large Send Offload v2 (IPv4)"
ParamDesc_GSOv6          = "Large Send Offload v2 (IPv6)"
GenTxEnable = "Tx Enabled"
GenRxEnable = "Rx Enabled"
GenTxRxEnable = "Rx & Tx Enabled"
GenEnable="Enable"
GenDisable="Disable"


TaskOffload              = "Checksum Offload"
TaskOffload_None         = "None"
TaskOffload_Rx_Chksum    = "Rx TCP/IP Checksum"
TaskOffload_Tx_Chksum    = "Tx TCP/IP Checksum"
TaskOffload_Rx_Tx_Chksum = "Tx/Rx TCP/IP Checksum"


TaskOffload_LargeSend           = "Large Send Offload"
TaskOffload_LargeSend_Disable   = "Disable"
TaskOffload_LargeSend_Enable    = "Enable"

TaskOffload_LargeSend_Jumbo                           = "LSO & Jumbo Frames"
TaskOffload_LargeSend_Disable_Both                = "Both Disabled"
TaskOffload_LargeSend_Enable_JumboDisable   = "LSO Enabled,Jumbo Off"
TaskOffload_LargeSend_Disable_JumboEnable3000   = "LSO Off,Jumbo 3000"
TaskOffload_LargeSend_Disable_JumboEnable4500   = "LSO Off,Jumbo 4500"
TaskOffload_LargeSend_Disable_JumboEnable6000   = "LSO Off,Jumbo 6000"
TaskOffload_LargeSend_Disable_JumboEnable7500   = "LSO Off,Jumbo 7500"
TaskOffload_LargeSend_Disable_JumboEnable9000   = "LSO Off,Jumbo 9000"


WakeUpMode         = "Wake Up Capabilities"
WakeUpMode_None    = "None"
WakeUpMode_Magic   = "Magic Packet"
WakeUpMode_Pattern = "Wake Up Frame"
WakeUpMode_Both    = "Both"

WolSpeed       = "WOL Speed"
WolSpeed_Auto  = "Auto"
WolSpeed_10mb  = "10 Mb"
WolSpeed_100mb = "100 Mb"
WolSpeed_1000mb = "1000 Mb"
WolSpeed_LowestAvail = "Lowest Speed Advertised"

NetworkAddress           = "Network Address"


LogLevelInfo    = "Log Information Messages"
LogLevelWarn  = "Log Warning Messages"
LogLevelInfo_Disable  =  "Disable"
LogLevelInfo_Enable  =  "Enable"
LogLevelWarn_Disable  =  "Disable"
LogLevelWarn_Enable  =  "Enable"

VlanID = "VLAN ID"
