***************************************************************************
		    Fast Ethernet Controller Provider Inc.        
		       PCI 10/100 Fast Ethernet Adapter                    

	         NetWare ODI Client Driver For DOS Workstation
	         ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

	   Copyright (C) 1999 Fast Ethernet Controller Provider Inc.        
			     All rights reserved.
***************************************************************************

This file is a description of the files contained in the \NETWARE\DOSODI 
subdirectory of this diskette, and of their usage. For more information 
please refer to "NOVELL NetWare ODI Shell for DOS" manual.

Installation Procedure
======================
Before you start with the installation process, make sure that the adapter
is properly installed and configured. Make sure that your NetWare operating
system is properly installed.

Should there already be Netware client programs such as: LSL.COM, IPXODI, 
and VLM.EXE in your system, you can use the following procedures to setup 
your system.

  1. Copy the A:\NETWARE\DOSODI\FASTNIC.COM  file to the Netware client  
     directory which contains NET.CFG, LSL.COM, IPXODI.COM, and VLM.EXE
     with related *.VLM files.

  2. Update the NET.CFG file. You can refer to the NET.CFG sample.

  3. Make sure to add LASTDRIVE=Z in your CONFIG.SYS file.

  4. Enter the following commands to connect to your Novell server:
		LSL
		FASTNIC  
		IPXODI
		VLM
		F:
		LOGIN <user_name>


  ** NOTE **
     Multiple LAN Adapters in a system:
      If you want to install a mutiple LAN adapter in your system, you have
      to use "SLOT" keyword in NET.CFG to select which adapter to use with
      your netware client.



Configuration Files
===================
  File Name:		NET.CFG
  
  Sample of configuration file:
----------------------------------------------------------------------------
Link Driver FastNIC  
    FRAME Ethernet_802.2
    FRAME Ethernet_802.3
    FRAME Ethernet_SNAP
    FRAME Ethernet_II

;	No_Early_Rx_Interrupt_Enable	; Certification, please remove the
					; first ";" of this line
;       FORCE_MEDIA
;       Connection_Type	= 10MFD	; 10M 10MFD 100M 100MFD, default is AUTO
        TX_THRESHOLD	= 0	; 0..3,	4=Store and forward, default=0
        RX_THRESHOLD	= 1	; 0..2,	2=Store and forward, default=1
        CAL		= 2	; 0..3,	default = 2
        PBL		= 10	; 0,1,2,4,8,10,20, default = 10
        Rx_Buffer_Size	= 100	; Hex number, 100-600
;       Slot  1
        RX_FIFO_SIZE	= 2	; 0..2, 0 ~ 2:2K, 3:1K; 0 is default

NetWare DOS Requester
        FIRST NETWORK DRIVE = F
        NETWARE PROTOCOL = NDS BIND
;       MAX IPG = 0
;       PBURST READ WINDOW SIZE=45
;       PBURST WRITE WINDOW SIZE=45

----------------------------------------------------------------------------
** Note **	
  Its PCI cycle may be slower on some mechine. At this time, you should 
  eable store and forward function in NET.CFG.

All trademarks and brand names mentioned belong to their respective owners.