;; Realtek RTL8139/810x/8169/8110 all in one NDIS Driver
;;
;; Copyright 2003, Realtek Semiconductor Corporation
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                               
CatalogFile.NT    = netrtl.cat                        ;;for WHQL certified
DriverVer      = 12/02/2004,5.620.1202.2004

[Manufacturer]
%Realtek%   = Realtek, NT.5.1

[ControlFlags]
ExcludeFromSelect = PCI\VEN_10EC&DEV_8139
ExcludeFromSelect = PCI\VEN_10EC&DEV_8169
;ExcludeFromSelect = PCI\VEN_10EC&DEV_8168

[Realtek]
; DisplayName            Section            DeviceID
; -----------            -------            --------
;%RTL8168.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8168
%RTL8169.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8169
%RTL8139.DeviceDesc%    = RTL8139.ndi,      PCI\VEN_10EC&DEV_8139&REV_10
%RTL8139P.DeviceDesc%   = RTL8139P.ndi,     PCI\VEN_10EC&DEV_8139&REV_20
;%RTL8168.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC
%RTL8169.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8139.DeviceDesc%    = RTL8139.ndi,      PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_10
%RTL8139P.DeviceDesc%   = RTL8139P.ndi,     PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_20
%RTL8139.DeviceDesc%    = RTL8139_TOS.ndi,  PCI\VEN_10EC&DEV_8139&SUBSYS_813610EC

[Realtek.NT.5.1]; This section will only be installed by Windows XP
;%RTL8168.DeviceDesc%	= RTL8169x.ndi,	    PCI\VEN_10EC&DEV_8168
%RTL8169.DeviceDesc%	= RTL8169x.ndi,	    PCI\VEN_10EC&DEV_8169
%RTL8139.DeviceDesc%	= RTL8139x.ndi,     PCI\VEN_10EC&DEV_8139&REV_10
%RTL8139P.DeviceDesc%	= RTL8139Px.ndi,    PCI\VEN_10EC&DEV_8139&REV_20
;%RTL8168.DeviceDesc%	= RTL8169x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC
%RTL8169.DeviceDesc%	= RTL8169x.ndi,     PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8139.DeviceDesc%	= RTL8139x.ndi,     PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_10
%RTL8139P.DeviceDesc%	= RTL8139Px.ndi,    PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_20
%RTL8139.DeviceDesc%	= RTL8139_TOSx.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_813610EC

;;****************************************************************************
;; Windows 98/ME
;;****************************************************************************
[rtl8139.ndi]
DriverVer       = 12/02/2004,620
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8139P.ndi]
DriverVer       = 12/02/2004,620
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8169.ndi]
DriverVer       = 12/02/2004,620
AddReg          = rtl8169.id.reg, RTLnic.all.reg, RTL8169.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

[RTL8139_TOS.ndi]
DriverVer       = 12/02/2004,620
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL8139TOS.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;; Windows 2000
;;****************************************************************************
[RTL8139.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8139P.ndi.NT]
DelReg          = CpPreParams.DelReg
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL39.common.reg, RTL39p.only.reg, RTL39p.w2k.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139P.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8169.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL8169.common.reg, RTL8169.W2K.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8169.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8139_TOS.ndi.NT]
DelReg          = PreParams.DelReg           
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL8139TOS.common.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139_TOS.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
Rtlnic.sys,,,2

[Rtlnic.CopyFiles9x]
Rtlnic.sys,,,2

;;****************************************************************************
;; Windows XP
;;****************************************************************************
;----------------
; RTL8139 Family
;----------------
[RTL8139x.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139x.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[RTL8139_TOSx.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL8139TOS.common.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139_TOSx.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

;-----------
; RTL8139c+
;-----------
[RTL8139Px.ndi.NT]
DelReg          = CpPreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL39.common.reg, RTL39p.only.reg, RTL39p.w2k.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139Px.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

;---------
; RTL8169
;---------
[RTL8169x.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL8169.common.reg, RTL8169.W2K.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8169x.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[Rtlnic.CopyFilesXP]
Rtlnicxp.sys,,,2

;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8139.id.reg]
HKR,,                 MediaType,          0,    1
HKR,,                 AdapterType,        0,    5
HKR,,                 BusType,            0,    5
HKR,,                 DevLoader,          0,    "*ndis"
HKR,,                 DeviceVxDs,         0,    "Rtlnic.sys"
HKR,,                 EnumPropPages,      0,    "netdi.dll,EnumPropPages"
HKR,NDIS,             MajorNdisVersion,   1,    03
HKR,NDIS,             MinorNdisVersion,   1,    0A
HKR,NDIS,             LogDriverName,      0,    "RTL8023"
HKR,Ndi,              DeviceID,           0,    "PCI\VEN_10EC&DEV_8139"
HKR,Ndi\Install,      ndis3,              0,    "rtl139.ndis5"
HKR,Ndi\Interfaces,   DefLower,            ,    "ethernet"
HKR,Ndi\Interfaces,   LowerRange,          ,    "ethernet"
HKR,Ndi\Interfaces,   DefUpper,            ,    "ndis3"
HKR,Ndi\Interfaces,   UpperRange,          ,    "ndis3"

[rtl8169.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtlnic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTL8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8169"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;;****************************************************************************
;; common parameters
;;****************************************************************************
[RTLnic.all.reg]
HKR,Ndi\params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	type,		0, "edit"
HKR,Ndi\params\NetworkAddress,	default,	0, "000000000000"
HKR,Ndi\params\NetworkAddress,	LimitText,	0, "12"
HKR,Ndi\params\NetworkAddress,	UpperCase,	0, "1"
HKR,Ndi\params\NetworkAddress,	Optional,	0, "1"

[RTL39.common.reg]
HKR,Ndi\params\DuplexMode,        ParamDesc,   0, %SpeedDuplexMode%
HKR,Ndi\params\DuplexMode,        type,        0, "enum"
HKR,Ndi\params\DuplexMode,        default,     0, "1"
HKR,Ndi\params\DuplexMode\enum,   1,           0, %auto_nego%
HKR,Ndi\params\DuplexMode\enum,   2,           0, %sd10half%
HKR,Ndi\params\DuplexMode\enum,   3,           0, %sd10full%
HKR,Ndi\params\DuplexMode\enum,   4,           0, %sd100half%
HKR,Ndi\params\DuplexMode\enum,   5,           0, %sd100full%

HKR,Ndi\params\OptimalPerf,      ParamDesc,  0, %OptimalPerf%
HKR,Ndi\params\OptimalPerf,      default,    0, "0"
HKR,Ndi\params\OptimalPerf,      type,       0, "enum"
HKR,Ndi\params\OptimalPerf\enum, "1",        0, "Enable"
HKR,Ndi\params\OptimalPerf\enum, "0",        0, "Disable"

HKR,Ndi\params\WakeUpFrame,	ParamDesc,	0, %WOLCapability%
HKR,Ndi\params\WakeUpFrame,	default,	0, "1"
HKR,Ndi\params\WakeUpFrame,	type,		0, "enum"
HKR,Ndi\params\WakeUpFrame\enum,"0",		0, "Disable"
HKR,Ndi\params\WakeUpFrame\enum,"1",		0, "Enable"
HKR,,WakeUpFrame, 0, "1"

HKR,Ndi\params\LinkUp,           ParamDesc, 0, "WakeUp on Link Change"
HKR,Ndi\params\LinkUp,           default,   0, "0"
HKR,Ndi\params\LinkUp,           type,      0, "enum"
HKR,Ndi\params\LinkUp\enum,      "1",       0, "Enable"
HKR,Ndi\params\LinkUp\enum,      "0",       0, "Disable"

HKR,Ndi\params\EnableLDPS,       ParamDesc, 0, "Link Down Power Saving"
HKR,Ndi\params\EnableLDPS,       default,   0, "0"
HKR,Ndi\params\EnableLDPS,       type,      0, "enum"
HKR,Ndi\params\EnableLDPS\enum,  "1",       0, "Enable"
HKR,Ndi\params\EnableLDPS\enum,  "0",       0, "Disable"

[RTL39.only.reg]
HKR,Ndi\params\RxBufLen,	 ParamDesc, 0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,	 type,      0, "enum"
HKR,Ndi\params\RxBufLen,	 default,   0, "3"
HKR,Ndi\params\RxBufLen\enum,	 "0",       0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,	 "1",	    0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,	 "2",	    0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,	 "3",	    0, "64K bytes"

HKR,Ndi\params\RTPME,            ParamDesc, 0, "WakeUp using APM Mode"
HKR,Ndi\params\RTPME,            default,   0, "0"
HKR,Ndi\params\RTPME,            type,      0, "enum"
HKR,Ndi\params\RTPME\enum,       "1",       0, "Enable"
HKR,Ndi\params\RTPME\enum,       "0",       0, "Disable"

[RTL39p.only.reg]
HKR,Ndi\Params\NumCoalesce,       ParamDesc,  0, "Number of Tx Coalesce Buffer"
HKR,Ndi\Params\NumCoalesce,       Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,       Default,    0, "16"
HKR,Ndi\Params\NumCoalesce,       Min,        0, "0"
HKR,Ndi\Params\NumCoalesce,       Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,       Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,       Base,       0, "10"

[PreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[CpPreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\RTPME
HKR,,RTPME
HKR,Ndi\Params\RxBufLen
HKR,,RxBufLen
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[GigPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid

[RTL39p.w2k.reg]
HKR,Ndi\params\Offload,           ParamDesc,  0, "Task Offload"
HKR,Ndi\params\Offload,           default,    0, "1"
HKR,Ndi\params\Offload,           type,       0, "enum"
HKR,Ndi\params\Offload\enum,      "0",        0, "All Disable"
HKR,Ndi\params\Offload\enum,      "1",        0, "Checksum"
HKR,Ndi\params\Offload\enum,      "2",        0, "Chksum & TCP_Segment"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

[RTL8139TOS.common.reg]
HKR,Ndi\params\RxBufLen,          ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,          type,       0, "enum"
HKR,Ndi\params\RxBufLen,          default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,     "0",        0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,     "1",        0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,     "2",        0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,     "3",        0, "64K bytes"

HKR,Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR,Ndi\params\LinkUp,            default,    0, "0"
HKR,Ndi\params\LinkUp,            type,       0, "enum"
HKR,Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR,Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR,Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"         
HKR,Ndi\params\WakeUpFrame,       default,    0, "1"                          
HKR,Ndi\params\WakeUpFrame,       type,       0, "enum"                       
HKR,Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"                     
HKR,Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"                    

HKR,Ndi\params\RTPME,             ParamDesc,  0, "WakeUp using APM Mode"      
HKR,Ndi\params\RTPME,             default,    0, "0"                          
HKR,Ndi\params\RTPME,             type,       0, "enum"                      
HKR,Ndi\params\RTPME\enum,        "1",        0, "Enable"                     
HKR,Ndi\params\RTPME\enum,        "0",        0, "Disable"                   

HKR,Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR,Ndi\params\EnableLDPS,        default,    0, "1"
HKR,Ndi\params\EnableLDPS,        type,       0, "enum"
HKR,Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"
HKR,Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"

HKR,Ndi\params\TxMaxDMABurst,     ParamDesc,  0, "Transmit DMA burst size"  
HKR,Ndi\params\TxMaxDMABurst,     type,       0, "enum"                           
HKR,Ndi\params\TxMaxDMABurst,     default,    0, "6"                           
HKR,Ndi\params\TxMaxDMABurst\enum,0,          0, "16 bytes"                  
HKR,Ndi\params\TxMaxDMABurst\enum,1,          0, "32 bytes"        
HKR,Ndi\params\TxMaxDMABurst\enum,2,          0, "64 bytes"         
HKR,Ndi\params\TxMaxDMABurst\enum,3,          0, "128 bytes"         
HKR,Ndi\params\TxMaxDMABurst\enum,4,          0, "256 bytes"        
HKR,Ndi\params\TxMaxDMABurst\enum,5,          0, "512 bytes"            
HKR,Ndi\params\TxMaxDMABurst\enum,6,          0, "1024 bytes"             
HKR,Ndi\params\TxMaxDMABurst\enum,7,          0, "2048 bytes"             

HKR,Ndi\params\RxMaxDMABurst,     ParamDesc,  0, "Receive DMA burst size"  
HKR,Ndi\params\RxMaxDMABurst,     type,       0, "enum"
HKR,Ndi\params\RxMaxDMABurst,     default,    0, "6"                      
HKR,Ndi\params\RxMaxDMABurst\enum,0,          0, "16 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,1,          0, "32 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum,2,          0, "64 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum,3,          0, "128 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,4,          0, "256 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,5,          0, "512 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,6,          0, "1024 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,7,          0, "unlimitted"               

HKR,Ndi\params\EarlyRxThreshold,  ParamDesc,  0, "Receive FIFO threshold"   
HKR,Ndi\params\EarlyRxThreshold,  type,       0, "enum"
HKR,Ndi\params\EarlyRxThreshold,  default,    0, "2"
HKR,Ndi\params\EarlyRxThreshold\enum,0,       0, "16 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,1,       0, "32 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,2,       0, "64 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,3,       0, "128 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,4,       0, "256 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,5,       0, "512 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,6,       0, "1024 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,7,       0, "No threshold"

HKR,,EnableLDPS,        0,   "1"
HKR,,WakeUpFrame,       0,   "1"          
HKR,,RTPME,             0,   "0"         
HKR,,LinkUp,            0,   "0"
HKR,,RxBufLen,          0,   "3"
HKR,,EarlyRxThreshold,  0,   "2"
HKR,,RxMaxDMABurst,     0,   "6"
HKR,,TxMaxDMABurst,     0,   "6" 

[RTL8169.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%

;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
HKR,Ndi\params\Jumboframe\enum,   "1",        0, "2KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "2",        0, "3KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "3",        0, "4KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "4",        0, "5KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "5",        0, "6KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "6",        0, "7KB MTU"

HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, "Disable"
HKR,Ndi\params\FlowControl\enum, "1",        0, "Enable"
HKR,,FlowControl,0,"1" 

[RTL8169.W2K.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, "Disable"
HKR,Ndi\params\CksOffload\enum,   "1",        0, "Tx/Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "3",        0, "Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "4",        0, "Tx Checksum"

HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "1",        0, "Enable"
HKR,Ndi\params\Largesend\enum,    "0",        0, "Disable"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"

;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"

HKR,,CksOffload,0,"1" 
HKR,,Largesend,0,"1" 

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8023.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtlnic.sys
LoadOrderGroup  = NDIS

[RTL8023xp.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8023xp"

[rtsntxp.Service]
DisplayName     = %Rtlnicxp.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtlnicxp.sys
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
Rtlnic.CopyFilesXP         = 12
Rtlnic.CopyFiles9x         = 11
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
Rtlnic.sys   = 1
Rtlnicxp.sys  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek			= "TP-LINK TECHNOLOGIES CO., LTD."
VLanTagging		= "802.1Q/1p VLAN Tagging"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Offload Checksum"
LargesendOffload	= "Offload TCP_LargeSend"
SpeedDuplexMode		= "Link Speed/Duplex Mode"
auto_nego		= "Auto Negotiation"
sd10half		= "10Mbps/Half Duplex"
sd10full		= "10Mbps/Full Duplex"
sd100half		= "100Mbps/Half Duplex"
sd100full		= "100Mbps/Full Duplex"
sd1000full		= "1000Mbps/Full Duplex"
NetworkAddress		= "Network Address"
JumboFrame		= "Jumbo Frame"
;TxDescNumber		= "Number of Tx Descriptor"
;RxDescNumber		= "Number of Rx Descriptor"
;TxHPQDescNumber	= "Number of High Priority Tx Descriptor"
WOLCapability		= "WakeUp on ARP/PING"
WOLLinkChange		= "WakeUp on Link Change"
LDPSCapability		= "Link Down Power Saving"
OptimalPerf		= "Optimal Performance"
FlowControl		= "Flow Control"

;;Source disk name
DISKNAME = "TP-LINK TF-3239 Series Fast Ethernet Adapter Driver Diskette"

;RTL8168.DeviceDesc        = "Realtek RTL8168 PCI-E Gigabit Ethernet NIC"
RTL8169.DeviceDesc        = "TP-LINK TG-3269 Gigabit Ethernet Adapter"
RTL8139.DeviceDesc        = "TP-LINK TF-3239 Series Fast Ethernet Adapter"
RTL8139P.DeviceDesc       = "Realtek RTL8139C+ Fast Ethernet NIC"

;;NT service name
Rtlnic.Service.DispName    = "TP-LINK TF-3239 Series Fast Ethernet Adapter NDIS NT Driver"
Rtlnicxp.Service.DispName    = "TP-LINK TF-3239 Series Fast Ethernet Adapter NDIS NT Driver"
