   Windows 98, Windows 98 SE, Windows2000, Windows ME, Windows XP

   Introduction:
   -------------
   This document describes the procedure to install Windows 98/98 SE
   Windows 2000 Windows ME and Windows XP driver for TP-LINK TF-3239
   Series Fast Ethernet Adapter.

   Location of Windows 98/98 SE Driver :   \win98\Rtlnic4.sys
   Location of Windows 2000 and Windows XP Driver     :   \win2000&winxp\Rtlnic.sys
   Location of Windows ME Driver       :   \winme\Rtlnic.sys

   Installing driver for Win98/Win98 SE/Windows2000/Windows ME/Windows XP:
   -------------------------------------------------------------------
      Before you start with the installation process, make sure that your
      adapter should be properly installed in your PCI bus slot.
      Executing Win98/Win98 SE/Windows2000/Windows ME/Windows XP, it will
      auto-detect your system configuration and find the adapter hardware.
      ( If Win98/Win98 SE/Windows2000/Windows ME/Windows XP does not prompt
      that it detects the PCI Ethernet adapter,there must be something wrong with
      the TP-LINK TF-3239 Series Fast Ethernet Adapter or your system enviroment.)

      1. Ask you to select which driver you want to install, select "Driver
         from disk provided by hardware manufacturer".

      2. Insert the TP-LINK TF-3239 Series Fast Ethernet Adapter Driver  
         Diskette into drive A and specify the setup file pathname 
             A:\WIN98 (for Windows 98/98 SE) or
             A:\WIN2000&WINXP  (for Windows 2000 and Windows XP)
             A:\WinMe (for Windows ME)
                               
      3. Win98/Win98 SE/Windows2000/Windows ME/Windows XP will appear some
         messages to insert Win98/Win98 SE/Windows2000/Windows ME/Windows XP
         system disk to complete setup step.

      4. Win98/Win98 SE/Windows2000/Windows ME/Windows XP will finish the other 
         installation procedure automatically, then you restart the system.

