;****************************************************************************
;                                                                           *
;       Novell NetWare Server Driver Description File for RTSSRV.LAN        *
;                                                                           *
;****************************************************************************

VER: 1.00
SYN: 1.00

DR RTSSRV
{
    DES:    $RTSSRV_1
    HELP:   $RTSSRV_2
    PAR:    2.00
    PROD:    'PCI.10EC.8139.*.*.*','PCI.10EC.8138.*.*.*'

;@# SPROD:  'REALTEK ~ RTL8139/810X Family Fast Ethernet PCI driver'
;@# ALIAS:  RTSSRV.LAN
;@# CLIENT: RTSSRV.LAN

    FILE:   RTSSRV.LAN
    TIME:   15

    PR SLOT
    {
        DES:    $RTSSRV_3
        HELP:   $RTSSRV_4

        TYP:   DEC
        VAL:    1-65535
        DEF:    UND
        OUT:    'SLOT=%s'
    }

    FR FrameSelect
    {
        CD:     $RTSSRV_5
        CH:     $RTSSRV_6
        CD:     $RTSSRV_7
        CH:     $RTSSRV_8
        CD:     $RTSSRV_9
        CH:     $RTSSRV_10
        CD:     $RTSSRV_11
        CH:     $RTSSRV_12
        DEF:    1,2,3,4
    }

    PR NODE OPT
    {
        DES:    $RTSSRV_13
        TYP:   HEX
        VAL:    1-FFFFFFFFFFFE
        DEF:    UND
        OUT:    'NODE=%s'
    }

     PR MEDIUMTYPE   OPT
    {
        DES:    $RTSSRV_14
        HELP:   $RTSSRV_15
        TYP:   STR
        VAL:    AUTO , 100FULL, 100HALF, 10FULL, 10HALF
        DEF:   UND
        OUT:    'MEDIUMTYPE=%s'
    }
}


DLANG:    4
;English
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    6
;French
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    7
;German
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board is installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    8
;Italian
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board is installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    14
;Spanish
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    12
;Portuquese
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    9
;Japanese
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    10
;Korean
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    1
;Chinese (Simplified)
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    16
;Chinese (Traditional)
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    13
;Russian
    $RTSSRV_1 = "Realtek RTL8139/810X Family Fast Ethernet PCI driver"
    $RTSSRV_2 = "This driver supports PCI bus devices"
    $RTSSRV_3 = "Slot"
    $RTSSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTSSRV_5 = "802.2"
    $RTSSRV_6 = "ethernet_802.2"
    $RTSSRV_7 = "802.3"
    $RTSSRV_8 = "ethernet_802.3"
    $RTSSRV_9 = "SNAP"
    $RTSSRV_10 = "ethernet_snap"
    $RTSSRV_11 = "ethernet II"
    $RTSSRV_12 = "ethernet_II"
    $RTSSRV_13 = "Node Address"
    $RTSSRV_14 = "MediumType Select"
    $RTSSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"
