
;
; FastNIC.INF - Windows 95 ODI driver installation information file
;              for PCI 10/100 Fast Ethernet Adapter                    
;
; Copyright (C) 1998, Fast Ethernet Controller Provider. All Rights Reserved.     

[version]
InfVersion=00.01.11
signature=$CHICAGO$
Class=Net
provider=%V_N%

;****************************************************************************
; Manufacturer Section
;****************************************************************************
[Manufacturer]
%V_FastNIC%=FastNIC  

[ControlFlags]
ExcludeFromSelect = PCI\VEN_1317&DEV_0981
ExcludeFromSelect = PCI\VEN_1317&DEV_0985  
ExcludeFromSelect = PCI\VEN_1317&DEV_1985
ExcludeFromSelect = PCI\VEN_1317&DEV_9511
ExcludeFromSelect = PCI\VEN_1317&DEV_9513

;****************************************************************************
; Manufacturer Name Section
;****************************************************************************
[FastNIC] 
%PCI\VEN_1317&DEV_0981.DeviceDesc%=FastNIC.ndi,        PCI\VEN_1317&DEV_0981  
%PCI\VEN_1317&DEV_0985.DeviceDesc%=CentaurFastNIC.ndi,   PCI\VEN_1317&DEV_0985  
%PCI\VEN_1317&DEV_9511.DeviceDesc%=CentaurFastNIC.SW.ndi,   PCI\VEN_1317&DEV_9511  
%PCI\VEN_1317&DEV_9513.DeviceDesc%=CentaurFastNIC.HW.ndi,   PCI\VEN_1317&DEV_9513  
%PCI\VEN_1317&DEV_1985.DeviceDesc%=CentaurCFastNIC.ndi,   PCI\VEN_1317&DEV_1985  

;****************************************************************************
; INF Install Section
;****************************************************************************
[FastNIC.ndi]  
AddReg=FastNICID.ndi.reg,FastNIC.ndi.reg,FastNIC.pci.reg     

[CentaurFastNIC.ndi]  
AddReg=CentaurFastNICID.ndi.reg,FastNIC.ndi.reg,FastNIC.pci.reg     

[CentaurFastNIC.SW.ndi] 
AddReg=CentaurFastNICID.SW.ndi.reg,FastNIC.ndi.reg,FastNIC.pci.reg     

[CentaurFastNIC.HW.ndi] 
AddReg=CentaurFastNICID.HW.ndi.reg,FastNIC.ndi.reg,FastNIC.pci.reg     


[CentaurCFastNIC.ndi] 
AddReg=CentaurCFastNICID.ndi.reg,FastNIC.ndi.reg,FastNIC.pci.reg    

;****************************************************************************
; .REG (Device IDs)
;****************************************************************************
[FastNICID.ndi.reg]  
HKR,Ndi,DeviceID,,"PCI\VEN_1317&DEV_0981"
HKR,,AdapterCFID,,09811317

[CentaurFastNICID.ndi.reg]  
HKR,Ndi,DeviceID,,"PCI\VEN_1317&DEV_0985"
HKR,,AdapterCFID,,09851317

[CentaurFastNICID.SW.ndi.reg]  
HKR,Ndi,DeviceID,,"PCI\VEN_1317&DEV_9511"
HKR,,AdapterCFID,,95111317

[CentaurFastNICID.HW.ndi.reg]  
HKR,Ndi,DeviceID,,"PCI\VEN_1317&DEV_9513"
HKR,,AdapterCFID,,95131317

[CentaurCFastNICID.ndi.reg]  
HKR,Ndi,DeviceID,,"PCI\VEN_1317&DEV_1985"
HKR,,AdapterCFID,,19851317

[FastNIC.ndi.reg]  
; key,subkey,valuname,type,value
HKR,,DevLoader,,*odiload
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"

; Ndi section
HKR,Ndi,NdiInstaller,,"odipage.dll,odiNdiproc"

; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"odinsup,NovellODI32"
HKR,Ndi\Interfaces,UpperRange,,"odinsup,NovellODI32"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"

; Install section
HKR,Ndi\Install,"16 Bit",,"FastNIC.odi16.Install"  
HKR,Ndi\Install,"32 Bit",,"FastNIC.odi32.Install"  

; Remove section
HKR,Ndi\Remove,"16 Bit",,"FastNIC.odi16.Remove"  

; ODI 16 Bit info
HKR,"ODI\16 Bit",ModulePath,,"%24%%DRIVER_32_PATH%"
HKR,"ODI\16 Bit",Modules,,"LSLC32.NLM,PC32MLID.LAN"
HKR,"ODI\16 Bit",DriverPath,,"%24%%DRIVER_16_PATH%"
HKR,"ODI\16 Bit",NetcfgPath,,"%24%%DRIVER_16_PATH%"
HKR,"ODI\16 Bit",NetcfgFileName,,"net.cfg"
HKR,"ODI\16 Bit",FileName,,"FastNIC.com"  
HKR,"ODI\16 Bit",LinkDriver,,"FastNIC"  

; ODI 32 Bit Info
HKR,"ODI\32 Bit",ModulePath,,"%24%%DRIVER_32_PATH%"
HKR,"ODI\32 Bit",Modules,,"LSLC32.NLM,CMSM.NLM,ETHERTSM.NLM"
HKR,"ODI\32 Bit",DriverPath,,"%24%%DRIVER_32_PATH%"
HKR,"ODI\32 Bit",FileName,,"FastNIC.lan"  


;****************************************************************************
; Install Section
;****************************************************************************
[FastNIC.odi16.Install]  
CopyFiles=FastNIC.odi16.CopyFiles  
UpdateAutoBat=FastNIC.odi16.autobat  

[FastNIC.odi32.Install]  
CopyFiles=FastNIC.odi32.CopyFiles  
UpdateAutoBat=FastNIC.odi32.autobat  

[FastNIC.odi16.autobat]  
CmdDelete=LSL
CmdDelete=NE1500T
CmdDelete=ODIHLP
CmdAdd=LSL.COM,  "-c=%24%%DRIVER_16_PATH%NET.CFG"
CmdAdd=N16ODI.COM
CmdAdd=NESL.COM
CmdAdd=FastNIC.com  

[FastNIC.odi32.autobat]  
CmdDelete=LSL
CmdDelete=N16ODI
CmdDelete=NESL
CmdDelete=FastNIC  
CmdDelete=ODIHLP

;****************************************************************************
; Remove Section
;****************************************************************************
[FastNIC.odi16.Remove]  
UpdateAutoBat=odi16.AutoBatRemove

[odi16.AutoBatRemove]
CmdDelete=LSL
CmdDelete=N16ODI
CmdDelete=NESL
CmdDelete=FastNIC  

;****************************************************************************
; Common Params
;****************************************************************************
[FastNIC.pci.reg]  

; General Ethernet Frame-Type params
;------------------------------------
; First Logical Board
;---------------------
HKR,Ndi\params\Frame1,ParamDesc,,"1. Frame Type"
HKR,Ndi\params\Frame1,default,,1
HKR,Ndi\params\Frame1,type,,enum
HKR,Ndi\params\Frame1,optional,,0
HKR,Ndi\params\Frame1\enum,1,,"Ethernet_802.2"
HKR,Ndi\params\Frame1\enum,2,,"Ethernet_SNAP"
HKR,Ndi\params\Frame1\enum,3,,"Ethernet_II"
HKR,Ndi\params\Frame1\enum,4,,"Ethernet_802.3"

; Second Logical Board
;----------------------
HKR,Ndi\params\Frame2,ParamDesc,,"2. Frame Type"
HKR,Ndi\params\Frame2,default,,2
HKR,Ndi\params\Frame2,type,,enum
HKR,Ndi\params\Frame2,optional,,0
HKR,Ndi\params\Frame2\enum,1,,"Ethernet_802.2"
HKR,Ndi\params\Frame2\enum,2,,"Ethernet_SNAP"
HKR,Ndi\params\Frame2\enum,3,,"Ethernet_II"
HKR,Ndi\params\Frame2\enum,4,,"Ethernet_802.3"
HKR,Ndi\params\Frame2\enum,5,,"Not used"

; Third Logical Board
;---------------------
HKR,Ndi\params\Frame3,ParamDesc,,"3. Frame Type"
HKR,Ndi\params\Frame3,default,,3
HKR,Ndi\params\Frame3,type,,enum
HKR,Ndi\params\Frame3,optional,,0
HKR,Ndi\params\Frame3\enum,1,,"Ethernet_802.2"
HKR,Ndi\params\Frame3\enum,2,,"Ethernet_SNAP"
HKR,Ndi\params\Frame3\enum,3,,"Ethernet_II"
HKR,Ndi\params\Frame3\enum,4,,"Ethernet_802.3"
HKR,Ndi\params\Frame3\enum,5,,"Not used"

; Fourth Logical Board
;----------------------
HKR,Ndi\params\Frame4,ParamDesc,,"4. Frame Type"
HKR,Ndi\params\Frame4,default,,4
HKR,Ndi\params\Frame4,type,,enum
HKR,Ndi\params\Frame4,optional,,0
HKR,Ndi\params\Frame4\enum,1,,"Ethernet_802.2"
HKR,Ndi\params\Frame4\enum,2,,"Ethernet_SNAP"
HKR,Ndi\params\Frame4\enum,3,,"Ethernet_II"
HKR,Ndi\params\Frame4\enum,4,,"Ethernet_802.3"
HKR,Ndi\params\Frame4\enum,5,,"Not used"

; Node Address Override
;-----------------------
HKR,Ndi\params\"Node Address",ParamDesc,,"Node Address Override"
HKR,Ndi\params\"Node Address",type,,edit
HKR,Ndi\params\"Node Address",LimitText,,18
HKR,Ndi\params\"Node Address",UpperCase,,1
HKR,Ndi\params\"Node Address",default,,""
HKR,Ndi\params\"Node Address",flag,1,20,00,00,00
HKR,Ndi\params\"Node Address",optional,,1

; PCI Slot Number
;-----------------
HKR,Ndi\params\Slot,ParamDesc,,"Slot"
HKR,Ndi\params\Slot,default,,1
HKR,Ndi\params\Slot,type,,int
HKR,Ndi\params\Slot,min,,1
HKR,Ndi\params\Slot,max,,65535
HKR,Ndi\params\Slot,step,,1
HKR,Ndi\params\Slot,optional,,1
HKR,Ndi\params\Slot,HIN,,##
;HKR,Ndi\params\Slot,flag,1,20,00,00,00

; AutoDetect Media
;------------------
HKR,Ndi\params\AUTO,ParamDesc,,"AutoDetect Media"
HKR,Ndi\params\AUTO,default,,1
HKR,Ndi\params\AUTO,type,,enum
HKR,Ndi\params\AUTO\enum,1,,"ON"
HKR,Ndi\params\AUTO,flag,1,20,00,00,00
HKR,Ndi\params\AUTO,optional,,1

; 100BaseTx Full-Duplex Connection
;----------------------------------
HKR,Ndi\params\100-FD,ParamDesc,,"100BaseTx Full-Duplex"
HKR,Ndi\params\100-FD,default,,1
HKR,Ndi\params\100-FD,type,,enum
HKR,Ndi\params\100-FD\enum,1,,"ON"
HKR,Ndi\params\100-FD,flag,1,20,00,00,00
HKR,Ndi\params\100-FD,optional,,1

; 100BaseTx Half-Duplex Connection
;----------------------------------
HKR,Ndi\params\100-HD,ParamDesc,,"100BaseTx Half-Duplex"
HKR,Ndi\params\100-HD,default,,1
HKR,Ndi\params\100-HD,type,,enum
HKR,Ndi\params\100-HD\enum,1,,"ON"
HKR,Ndi\params\100-HD,flag,1,20,00,00,00
HKR,Ndi\params\100-HD,optional,,1

; 10BaseT Full-Duplex Connection
;--------------------------------
HKR,Ndi\params\10-FD,ParamDesc,,"10BaseT Full-Duplex"
HKR,Ndi\params\10-FD,default,,1
HKR,Ndi\params\10-FD,type,,enum
HKR,Ndi\params\10-FD\enum,1,,"ON"
HKR,Ndi\params\10-FD,flag,1,20,00,00,00
HKR,Ndi\params\10-FD,optional,,1

; 10BaseT Half-Duplex Connection
;--------------------------------
HKR,Ndi\params\10-HD,ParamDesc,,"10BaseT Half-Duplex"
HKR,Ndi\params\10-HD,default,,1
HKR,Ndi\params\10-HD,type,,enum
HKR,Ndi\params\10-HD\enum,1,,"ON"
HKR,Ndi\params\10-HD,flag,1,20,00,00,00
HKR,Ndi\params\10-HD,optional,,1

; Help section
HKR,Ndi,HelpText,,%ODIMLID_HELP%

;****************************************************************************
; File to be copied
;****************************************************************************
[FastNIC.odi32.CopyFiles]  
FastNIC.lan  

[FastNIC.odi16.CopyFiles]  
FastNIC.com  
LSL.com,,,5
N16ODI.COM,,,5
NESL.COM,,,5
;LSL.msg,,,5
;NESL.msg,,,5

;****************************************************************************
; Source Disk Names & Source Disk Files
;****************************************************************************
[SourceDisksNames]
50 = "PCI 10/100 Fast Ethernet Adapter Driver Diskette","",0                    

[SourceDisksFiles]
FastNIC.lan = 50,,10000  
FastNIC.COM = 50,,10000  
LSL.COM = 50
N16ODI.COM = 50
NESL.COM = 50
;LSL.msg = 50
;NESL.msg = 50

;****************************************************************************
; Destination Directories
;****************************************************************************
[DestinatioNdirs]
DefaultDestDir          = 11    ; LDID_SYS
FastNIC.odi32.CopyFiles  = 24,novell\client32  
FastNIC.odi16.CopyFiles  = 24,novell\nwclient  

;****************************************************************************
; Localizable Strings
;****************************************************************************
[strings]
; Provider
V_N="Novell"

; Manufacturers
V_FastNIC="FastNIC"  

;Paths to drivers
DRIVER_32_PATH="novell\client32\"
DRIVER_16_PATH="novell\nwclient\"

; FastNIC PCI Devices  
PCI\VEN_1317&DEV_0981.DeviceDesc="PCI 10/100 Fast Ethernet Adapter (32-Bit ODI)"                   
PCI\VEN_1317&DEV_0985.DeviceDesc="PCI 10/100 Fast Ethernet Adapter (32-Bit ODI)"                   
PCI\VEN_1317&DEV_9511.DeviceDesc="PCI 10/100 Fast Ethernet Adapter (32-Bit ODI)"                   
PCI\VEN_1317&DEV_9513.DeviceDesc="PCI 10/100 Fast Ethernet Adapter (32-Bit ODI)"                   
PCI\VEN_1317&DEV_1985.DeviceDesc="PCI 10/100 Fast Ethernet Adapter (32-Bit ODI)"                   

; Context help
ODIMLID_HELP="The FastNIC ODI Driver supports either 16-bits or 32-bits networking components."  


