****************************************************************************
		    TP-LINK TECHNOLOGIES CO., LTD.      
		       TP-LINK TF-3283 10/100M Fast Ethernet Adapter                   

	     NDIS 5 Miniport Driver For Windows 2000 Installation
	     ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

	   Copyright (C) 2000 TP-LINK TECHNOLOGIES CO., LTD.     
			     All rights reserved.
****************************************************************************

The driver conforms to the Network Driver Interface Specification (NDIS)5.0,
and used with Microsoft Windows OS.


Contents
--------
    A) Install NDIS5.0 Miniport driver to Microsoft Windows 2000
    B) Configure NDIS5.0 Miniport driver to Microsoft Windows 2000
	

A)Install NDIS5.0 Miniport driver to Microsoft Windows 2000
===========================================================
  1. Plug the TP-LINK TF-3283 10/100M Fast Ethernet Adapter into one of the Master PCI                   
     slots of your PCI platform.

  2. Turn on the power of PC then boot into Windows 2000.

  3. Windows 2000 will prompt "PCI Ethernet Controller" in "New Hardware 
     Found" dialog box.

  4. Select "Search for suitable driver for your device(Recommand)" from 
     "Found New Hardware Wizard" dialog box, then click "Next" button.

  5. Select "Specify a location" from "Found New Hardware Wizard" dialog box
     , then click "Next" button.

  6. Insert the TP-LINK TF-3283 10/100M Fast Ethernet Adapter Driver Diskette in your                   
     floppy drive.

  7. Enter the driver pathname, i.e. A:\win2000 (or B:\), then click "OK" 
     button from "Found New Hardware Wizard" dialog box.

  8. "Found New Hardware Wizard" dialog box will find inf file.
     i.e. A:\WIN2000\FASTNIC.INF, then click "Next" button.  

  9. Windows 2000 will prompt; "TP-LINK TF-3283 10/100M Fast Ethernet Adapter" in "Found                   
     New Hardware Wizard" dialog box, then click "Finsh" button.

 10. Windows 2000 will prompt "New Connection" Wizard diag box, then click 
     "Next" button.

 11. You can Modify or Add your LAN protocol or LAN Service... form "LAN
     Wizard", and click "Next" button to continue.

 12. Type a name you want for this connection form "LAN Wizard" diag box,
     and click "Finsh" button.

 13. Remove the TP-LINK TF-3283 10/100M Fast Ethernet Adapter Driver Diskette from your                    
     floppy drive.

 

B) Configuring NDIS5.0 Miniport driver to Microsoft Windows 2000
================================================================
  1. Click the "My Computer" icon in the Main Program Group.

  2. Click the "Control Panel" icon from My Computer window.

  3. Click the "Network and Dial-up Connections" icon from the Control 
     Panel window.

  4. Select "TP-LINK TF-3283 10/100M Fast Ethernet Adapter" item from "Network" dialog                    
     box, then click "Properties" button.

  5. Press "Configure" key.

  6. Click "Advanced" button from "TP-LINK TF-3283 10/100M Fast Ethernet Adapter Properties"                    
     dialog box.

  7. Select the Media Type value (AutoDetect, 10BaseT, 10BaseT Full_Duplex,
     100BaseTX, 100BaseTX Full_Duplex) from "Value" item, then click OK 
     button from "ADMtek ADM9511 10/100Mbps Fast Ethernet Adapter Properties" 
     dialog box.

  8. Click OK button from "Network" dialog box.




Trademarks:
Microsoft Windows 2000 is a trademark of Microsoft Corporation.

