InS_StArT
FastNIC.COM  
1.0
^PCI 10/100 Fast Ethernet Adapter   ,FastNIC.COM,IE0                       
?This driver supports only PCI machine
$OIE0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*OIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIE0(Connection_Type)Connection Type
?NOTE: The default Line speed will be selected on driver's load according to the board.
@AUTO
10M
10MFD
100M
100MFD
InS_EnD
