; yk60x64.inf created 07-Feb-2007
;
; Marvell Yukon Ethernet Controller 
;
; (C)Copyright 2002-2007 Marvell(R).
; 
; All rights reserved.
;
; INF File for NDIS6.0 Miniport Driver for Windows Vista x64 YK60X64.sys v9.16.4.3

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %Marvell%
CatalogFile	= yk60x64.CAT
DriverVer       = 02/07/2007, 9.16.4.3

[Manufacturer]
%Marvell%	= Marvell, NTamd64.6.0

[ControlFlags]

ExcludeFromSelect	= *


;-----------------------------------------------------------------------------
;
;       Windows 2000
;
;-----------------------------------------------------------------------------
[Marvell]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows XP
;
;-----------------------------------------------------------------------------
[Marvell.NT.5.1]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows Server 2003
;
;-----------------------------------------------------------------------------
[Marvell.NT.5.2]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows Vista
;
;-----------------------------------------------------------------------------

[Marvell.NTAMD64.6.0]
%AT-2916.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_29161259
%AT-2973.DeviceDesc% = SLYukFibGig_01.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_29731259
%AT-2973_1.DeviceDesc% = SLYuk2FibGig_02.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_29731259
%AT-2974.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_29741259
%AT-2974_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_29741259
%AT-2978.DeviceDesc% = SLYuk2FibGig_02.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_29781259
%RDK-8001.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_01211148
%RDK-8002.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_02211148
%RDK-8003.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_03211148
%RDK-8004.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_04211148
%RDK-8006.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_06211148
%RDK-8007.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_07211148
%RDK-8008.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_08211148
%RDK-8009.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_09211148
%RDK-8011.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_11211148
%RDK-8012.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_12211148
%SK-9521-V2.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_32211148
%SK-9521.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_95211148
%SK-9821-V2.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50211148
%SK-9841-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50411148
%SK-9843-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50431148
%SK-9851-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50511148
%SK-9861-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50611148
%SK-9871-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50711148
%SKYukon2-2220.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_22201148
%SKYukon2-8220.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_82201148
%SKYukon2-9C21.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21C01148
%SKYukon2-9E21.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21001148
%SKYukon2-9E21D.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21D01148
%SKYukon2-9E22.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_22001148
%SKYukon2-9E81.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_81001148
%SKYukon2-9E82.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_82001148
%SKYukon2-9E91.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_91001148
%SKYukon2-9E92.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_92001148
%SKYukon2-9I22.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_22101148
%SKYukon2-9P22.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_22101148
%SKYukon2-9P82.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_82101148
%SKYukon2-9S21.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_21001148
%SKYukon2-9S22.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_22001148
%SKYukon2-9S81.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_81001148
%SKYukon2-9S82.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_82001148
%SKYukon2-9S91.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_91001148
%SKYukon2-9S92.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_92001148
%Yukon-1700.DeviceDesc% = SLYukCopGig_01.ndi, PCI\VEN_10B7&DEV_1700&SUBSYS_002010B7
%Yukon-1700_1.DeviceDesc% = SLYukCopGig_01.ndi, PCI\VEN_10B7&DEV_1700&SUBSYS_001010B7
%Yukon-4001.DeviceDesc% = SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4001&SUBSYS_40011186
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_00851025
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_00881025
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_012111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_032111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0F381019
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_102111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_173C1043
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1C0317F2
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_502111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_952111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_E0001458
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_004715D4
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0C19105B
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0CC5105B
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0CCF105B
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1406147B
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_2803270F
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_80011019
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_811A1043
%Yukon-4320.DeviceDesc% = SLYukCopGig_03.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_90251695
%Yukon-4340.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4340&SUBSYS_212111AB
%Yukon-4340.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_11AB&DEV_4344&SUBSYS_218111AB
%Yukon-4340.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_11AB&DEV_4344&SUBSYS_219111AB
%Yukon-4341.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341&SUBSYS_222211AB
%Yukon-4341.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341&SUBSYS_3015107B
%Yukon-4341.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345&SUBSYS_228211AB
%Yukon-4341.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345&SUBSYS_229211AB
%Yukon-4342.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4342&SUBSYS_612111AB
%Yukon-4342.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_11AB&DEV_4346&SUBSYS_618111AB
%Yukon-4342.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_11AB&DEV_4346&SUBSYS_619111AB
%Yukon-4343.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_3015107B
%Yukon-4343.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_622211AB
%Yukon-4343.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_81DA1043
%Yukon-4343.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_E0001458
%Yukon-4343.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_628211AB
%Yukon-4343.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_629211AB
%Yukon-4343.DeviceDesc% = DLYuk2FibGig_01.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_001A1170
%Yukon-4346.DeviceDesc% = SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4346&SUBSYS_43461186
%Yukon-4350.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_352111AB
%Yukon-4350.DeviceDesc% = SLYuk2CopFast_05.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_00BA11AB
%Yukon-4350.DeviceDesc% = SLYuk2CopFast_17.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_00011179
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00018086
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_362111AB
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_01.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_3015107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_01.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_3031107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_01.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_3032107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_01.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_4009107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_01.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_4038107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_01.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_4039107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_01.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_5052107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_01.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_5053107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_03.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0300107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_03.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0365107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_03.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0506107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_11111071
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_80361019
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_902B1695
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_05.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001214C0
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_05.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00BA11AB
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_05.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_833810F7
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_07.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_81E6104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_07.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_8203104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_07.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_8205104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_07.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_820F104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_07.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_8212104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_07.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_9005104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_07.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_9017104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0733152D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0748152D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_AC1213D1
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_10.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_C027144D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_11.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_203D161F
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000D1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000E1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000F1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00111854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00121854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00141854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00151854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00161854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00171854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00181854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001A1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001B1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001C1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001E1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00201854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00211854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00221854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00231854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00241854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00281854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_002A1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_002B1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_002D1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00301854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_12.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00311854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_17.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00011179
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_17.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_FF001179
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_17.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_FF101179
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_02.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_001214C0
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_02.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_00241854
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_02.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_00BA11AB
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_02.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_01011025
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_02.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0366107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_02.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_F50117FF
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_1C0317F2
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_80381019
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_902D1695
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_E9001631
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_06.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0317107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_06.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0318107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_06.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0367107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_06.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0507107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_06.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_06201558
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_06.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0753152D
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_06.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0754152D
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_06.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_666617AA
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_08.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_2054161F
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_13.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_01101025
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_15.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_FF101179
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_303017AA
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_80391019
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_04.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_E9001631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_00BA11AB
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_0CE7105B
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_B048144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C1021631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C1031631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C1041631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_09.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C1051631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_10.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C031144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_10.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C034144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_10.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C510144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_14.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_30CD103C
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_16.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01041854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_16.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01051854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_16.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01061854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_16.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01071854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_16.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01081854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_16.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01091854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_17.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_FF101179
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_17.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_FF131179
%Yukon-4356.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4356&SUBSYS_2A35103C
%Yukon-4356.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4356&SUBSYS_2A36103C
%Yukon-4356.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4356&SUBSYS_2A37103C
%Yukon-4356.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4356&SUBSYS_2A46103C
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_00861025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_00871025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_008D1025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_008E1025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0C36105B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_522111AB
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_80521849
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_E0001940
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3015107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3031107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3032107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4009107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4038107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4039107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_5052107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_5053107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0509A0A0
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_052C1462
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_110115BD
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_81341043
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_E0001458
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_06.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0300107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_06.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0506107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_15.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_01231025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_15.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_01241025
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_30638086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34398086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343A8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343B8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343C8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343D8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343E8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34508086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34518086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34528086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34538086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34588086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34598086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345A8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345B8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345C8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345D8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345E8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345F8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34608086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34618086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34628086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34638086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34648086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34658086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34668086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34678086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_502111AB
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_50218086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_3015107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_3031107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_3032107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_4009107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_4038107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_4039107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_5052107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_5053107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_06.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_0300107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_06.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_0506107B
%Yukon-4362.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00461737
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0CA9105B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0CAA105B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0CAB105B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0CAC105B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3197109F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_532111AB
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_62501462
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80011854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80031854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80531849
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_B039144D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2401297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2411297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2421297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_E0001940
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3015107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3031107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3032107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_4009107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_4038107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_4039107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_5052107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_03.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_5053107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00031290
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_01111071
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0506A0A0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_058C1462
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_061DA0A0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_061EA0A0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_100315BD
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_110215BD
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2801270F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2A0D103C
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2C0817F2
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80531019
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81421043
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_90291695
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_A43010FD
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2431297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2441297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_E0001458
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001214C0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00BA11AB
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_038A1558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05601558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05701558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_058517FF
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_11D51043
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_204E161F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_61001584
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_833810F7
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_06.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0300107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_06.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0506107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81E6104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81E8104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81E9104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81FE104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_8205104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000217C0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_04A01558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05901558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05911558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05921558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0733152D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0748152D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_10B717C0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_AC1113D1
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_12.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_203C161F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_12.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_203D161F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_12.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_204A161F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000B1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000C1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00101854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00131854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00191854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001D1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001F1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00241854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00291854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_002C1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_002F1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_13.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00321854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_16.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00011179
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_16.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_FF001179
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_16.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_FF101179
%Yukon-4362_2.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_AB1214EA
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_902F1695
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_00241854
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_006C1025
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_00BA11AB
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_05711558
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_059017FF
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_61001584
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_833810F7
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_07.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_10C11734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_07.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_10D71734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_07.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_139A10CF
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_07.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_202317C0
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_81E6104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_81FE104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_8208104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_8210104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9008104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_900E104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9014104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9016104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_08.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9018104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_09.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_01101025
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_10.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C02F144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_10.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C031144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_10.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C033144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_10.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C034144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_10.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C509144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0317107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0318107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0507107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0753152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0754152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0761152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0762152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0763152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_2C201059
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_30D4103C
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_666617AA
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C1031631
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C1041631
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_11.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C1051631
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_12.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_2054161F
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_14.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_00791854
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_14.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_007A1854
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_16.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_FF101179
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_16.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_FF131179
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_17.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_820B104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_17.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_900F104D
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_562111AB
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_D6028086
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C75105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7A1053
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7A105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7B105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7C105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7D105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7E105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0CBF105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0CCA105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0CE7105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0D10105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0DF9105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0E09105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_14951043
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_1C0417F2
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_300319DB
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_326C1462
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_73261462
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_80561019
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_81F81043
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_82791043
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_90321695
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_E0001458
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_E9001631
%Yukon-4366.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4366&SUBSYS_2A35103C
%Yukon-4366.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4366&SUBSYS_2A36103C
%Yukon-4369.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4369&SUBSYS_00BA11AB
%Yukon-4369.DeviceDesc% = SLYuk2CopGig_04.ndi, PCI\VEN_11AB&DEV_4369&SUBSYS_80561019
%Yukon-4B00.DeviceDesc% = SLYuk2CopGig_01.ndi, PCI\VEN_1186&DEV_4B00&SUBSYS_4B001186
%Yukon-4B01.DeviceDesc% = SLYukCopGig.ndi, PCI\VEN_1186&DEV_4B01&SUBSYS_4B011186
%Yukon-4B02.DeviceDesc% = SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4B02&SUBSYS_4B021186
%Yukon-4B03.DeviceDesc% = SLYuk2CopGig.ndi, PCI\VEN_1186&DEV_4B03&SUBSYS_4B031186
%Yukon-4C00.DeviceDesc% = SLYukCopGig.ndi, PCI\VEN_1186&DEV_4C00&SUBSYS_4C001186
%Yukon-Generic.DeviceDesc% = SLYukCopGig_02.ndi, PCI\VEN_11AB&DEV_4320
%Yukon-Generic_1.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4340
%Yukon-Generic_1.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_11AB&DEV_4344
%Yukon-Generic_10.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4363
%Yukon-Generic_11.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4364
%Yukon-Generic_12.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_436A
%Yukon-Generic_12.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_436A&SUBSYS_00BA11AB
%Yukon-Generic_13.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4342
%Yukon-Generic_13.DeviceDesc% = SLYuk2FibGig_01.ndi, PCI\VEN_11AB&DEV_4346
%Yukon-Generic_14.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343
%Yukon-Generic_14.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347
%Yukon-Generic_15.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4367
%Yukon-Generic_16.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4356
%Yukon-Generic_17.DeviceDesc% = SLYuk2CopGig_05.ndi, PCI\VEN_11AB&DEV_4368
%Yukon-Generic_18.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4366
%Yukon-Generic_19.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4369
%Yukon-Generic_2.DeviceDesc% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341
%Yukon-Generic_2.DeviceDesc% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345
%Yukon-Generic_3.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4350
%Yukon-Generic_4.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4351
%Yukon-Generic_5.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4352
%Yukon-Generic_6.DeviceDesc% = SLYuk2CopFast_00.ndi, PCI\VEN_11AB&DEV_4353
%Yukon-Generic_7.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4361
%Yukon-Generic_8.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4360
%Yukon-Generic_9.DeviceDesc% = SLYuk2CopGig_02.ndi, PCI\VEN_11AB&DEV_4362


;-------------------------------------------------------------------------------
; (1)

[SLYuk2CopFast_00.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_00.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (2)

[SLYuk2CopFast_01.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLMagicPkt.params, yk60x64.DefaultWfSON.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_01.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (3)

[SLYuk2CopFast_02.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMaxRed.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_02.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (4)

[SLYuk2CopFast_03.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLMagicPkt.params, yk60x64.DefaultWfSON.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_03.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (5)

[SLYuk2CopFast_04.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_04.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (6)

[SLYuk2CopFast_05.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_05.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (7)

[SLYuk2CopFast_06.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMaxRed.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_06.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (8)

[SLYuk2CopFast_07.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLW10.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_07.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (9)

[SLYuk2CopFast_08.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMaxRed.params, yk60x64.WoLNoLnkCh.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_08.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (10)

[SLYuk2CopFast_09.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_09.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (11)

[SLYuk2CopFast_10.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatSmart.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_10.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (12)

[SLYuk2CopFast_11.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLNoLnkCh.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_11.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (13)

[SLYuk2CopFast_12.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatSmart.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSON.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_12.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (14)

[SLYuk2CopFast_13.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMaxRed.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_13.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (15)

[SLYuk2CopFast_14.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSON.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_14.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (16)

[SLYuk2CopFast_15.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegmLSOff.params, yk60x64.TxRxLE.params, yk60x64.BatMaxRed.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSON.params, yk60x64.HwFeaDev.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_15.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (17)

[SLYuk2CopFast_16.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSON.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_16.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (18)

[SLYuk2CopFast_17.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.FastFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegmLSOff.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLMagicPkt.params, yk60x64.DefaultWfSOFF.params, yk60x64.HwFeaDev.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopFast_17.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (19)

[SLYuk2CopGig.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SingleLink.params, yk60x64.TxRxLE.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (20)

[SLYuk2CopGig_01.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLStd.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_01.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (21)

[SLYuk2CopGig_02.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_02.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (22)

[SLYuk2CopGig_03.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLMagicPkt.params, yk60x64.DefaultWfSON.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_03.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (23)

[SLYuk2CopGig_04.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_04.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (24)

[SLYuk2CopGig_05.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_05.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (25)

[SLYuk2CopGig_06.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLMagicPkt.params, yk60x64.DefaultWfSON.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_06.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (26)

[SLYuk2CopGig_07.ndi]
AddReg		= yk60x64.reg, yk60x64.commonMsgLogOff.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLinkFCOff.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLWfSForcedCombine.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_07.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (27)

[SLYuk2CopGig_08.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLW10.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_08.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (28)

[SLYuk2CopGig_09.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_09.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (29)

[SLYuk2CopGig_10.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatSmart.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_10.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (30)

[SLYuk2CopGig_11.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_11.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (31)

[SLYuk2CopGig_12.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLNoLnkCh.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_12.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (32)

[SLYuk2CopGig_13.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatSmart.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSON.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_13.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (33)

[SLYuk2CopGig_14.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WfSON.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSON.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_14.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (34)

[SLYuk2CopGig_15.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLW10.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSON.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_15.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (35)

[SLYuk2CopGig_16.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegmLSOff.params, yk60x64.TxRxLE.params, yk60x64.BatMax.params, yk60x64.WoLMagicPkt.params, yk60x64.DefaultWfSOFF.params, yk60x64.HwFeaDev.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_16.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (36)

[SLYuk2CopGig_17.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.BatSmart.params, yk60x64.SmartBatDefaults.params, yk60x64.WoLW10.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig_17.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (37)

[DLYuk2CopGig.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_DL, yk60x64.GigFrSize.params, yk60x64.DLSpeedDuplex.params, yk60x64.DualLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLDL.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[DLYuk2CopGig.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (38)

[SLYuk2FibGig.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SingleLink.params, yk60x64.TxRxLE.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2FibGig.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (39)

[SLYuk2FibGig_01.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2FibGig_01.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (40)

[SLYuk2FibGig_02.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2FibGig_02.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (41)

[DLYuk2FibGig.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_DL, yk60x64.GigFrSize.params, yk60x64.DualLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[DLYuk2FibGig.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (42)

[DLYuk2FibGig_01.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_DL, yk60x64.GigFrSize.params, yk60x64.DualLink.params, yk60x64.TCPSegm.params, yk60x64.TxRxLE.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[DLYuk2FibGig_01.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (43)

[SLYukCopGig.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TxRxBuff.params, yk60x64.WoLStd.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYukCopGig.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (44)

[SLYukCopGig_01.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TxRxBuff.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSON.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYukCopGig_01.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (45)

[SLYukCopGig_02.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TxRxBuff.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYukCopGig_02.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (46)

[SLYukCopGig_03.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TxRxBuff.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params, yk60x64.FAN.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYukCopGig_03.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (47)

[SLYukFibGig.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SingleLink.params, yk60x64.TxRxBuff.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYukFibGig.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (48)

[SLYukFibGig_01.ndi]
AddReg		= yk60x64.reg, yk60x64.common.params, yk60x64.YKVS_SL, yk60x64.GigFrSize.params, yk60x64.SLSpeedDuplex.params, yk60x64.SingleLink.params, yk60x64.TxRxBuff.params, yk60x64.WoLStd.params, yk60x64.DefaultWfSOFF.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk60x64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYukFibGig_01.ndi.Services]
AddService	= yukonx64, 2, yukonx64.Service, common.EventLog



;-----------------------------------------------------------------------------
;
; General Driver Parameters
;
;-----------------------------------------------------------------------------
[yk60x64.common.params]


HKR, Ndi\Params\MessageLog,		ParamDesc,	0, %LogMsg%
HKR, Ndi\Params\MessageLog,		Type,		0, "enum"
HKR, Ndi\Params\MessageLog\enum,	"4",			0, %Non%
HKR, Ndi\Params\MessageLog\enum,	"3",			0, %Err%
HKR, Ndi\Params\MessageLog\enum,	"2",			0, %Wrn%
HKR, Ndi\Params\MessageLog\enum,	"1",			0, %Sta%
HKR, Ndi\Params\MessageLog\enum,	"0",			0, %All%
HKR, Ndi\Params\MessageLog,		Default,		0, "1"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\NetworkAddress,	ParamDesc,	0, %NetAddress%
HKR, Ndi\Params\NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,	Default,		0, ""
HKR, Ndi\Params\NetworkAddress,	Optional,		0, "1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, %IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, "enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, "1"


HKR, Ndi\Params\FixedIntMod,	ParamDesc,	0, %MaxIrq%
HKR, Ndi\Params\FixedIntMod,	Type,		0, "int"
HKR, Ndi\Params\FixedIntMod,	Base,		0, "10"
HKR, Ndi\Params\FixedIntMod,	Min,			0, "1000"
HKR, Ndi\Params\FixedIntMod,	Max,			0, "30000"
HKR, Ndi\Params\FixedIntMod,	Step,		0, "1"
HKR, Ndi\Params\FixedIntMod,	Default,		0, "5000"

;-----------------------------------------------------------------------------
;
; General Driver Parameters with changes
;
;-----------------------------------------------------------------------------
[yk60x64.commonMsgLogOff.params]


HKR, Ndi\Params\MessageLog,		ParamDesc,	0, %LogMsg%
HKR, Ndi\Params\MessageLog,		Type,		0, "enum"
HKR, Ndi\Params\MessageLog\enum,	"4",			0, %Non%
HKR, Ndi\Params\MessageLog\enum,	"3",			0, %Err%
HKR, Ndi\Params\MessageLog\enum,	"2",			0, %Wrn%
HKR, Ndi\Params\MessageLog\enum,	"1",			0, %Sta%
HKR, Ndi\Params\MessageLog\enum,	"0",			0, %All%
HKR, Ndi\Params\MessageLog,		Default,		0, "4"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,		ParamDesc,	0, %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*NetworkAddress,	ParamDesc,	0, %NetAddress%
HKR, Ndi\Params\*NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\*NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\*NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\*NetworkAddress,	Default,	0, ""
HKR, Ndi\Params\*NetworkAddress,	Optional,	0, "1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, %IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, "enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, "1"


;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX buffers (V1 and V2)
;
;-----------------------------------------------------------------------------
[yk60x64.TxRxBuff.params]

HKR, Ndi\Params\*ReceiveBuffers,	ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,	Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,	Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,	Min,		0, "3"
HKR, Ndi\Params\*ReceiveBuffers,	Max,		0, "500"
HKR, Ndi\Params\*ReceiveBuffers,	Step,		0, "1"
HKR, Ndi\Params\*ReceiveBuffers,	Default,	0, "50"

HKR, Ndi\Params\*TransmitBuffers,ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,Min,		0, "4"
HKR, Ndi\Params\*TransmitBuffers,Max,		0, "200"
HKR, Ndi\Params\*TransmitBuffers,Step,		0, "1"
HKR, Ndi\Params\*TransmitBuffers,Default,	0, "50"
;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX LE (Y2)
;
;-----------------------------------------------------------------------------
[yk60x64.TxRxLE.params]

HKR, Ndi\Params\*ReceiveBuffers,	ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,	Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,	Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,	Min,		0, "256"
HKR, Ndi\Params\*ReceiveBuffers,	Max,		0, "512"
HKR, Ndi\Params\*ReceiveBuffers,	Step,		0, "128"
HKR, Ndi\Params\*ReceiveBuffers,	Default,	0, "256"

HKR, Ndi\Params\*TransmitBuffers,	ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,	Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,	Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,	Min,		0, "256"
HKR, Ndi\Params\*TransmitBuffers,	Max,		0, "512"
HKR, Ndi\Params\*TransmitBuffers,	Step,		0, "128"
HKR, Ndi\Params\*TransmitBuffers,	Default,	0, "256"
;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100/1000 chip)
;
;-----------------------------------------------------------------------------
[yk60x64.GigFrSize.params]

HKR, Ndi\params\*JumboPacket,	ParamDesc,	0, %JumboPacket%
HKR, Ndi\params\*JumboPacket,	Type,		0, "enum"
HKR, Ndi\params\*JumboPacket\enum,	"0",	0, "1514"
HKR, Ndi\params\*JumboPacket\enum,	"1",	0, "4088"
HKR, Ndi\params\*JumboPacket\enum,	"2",	0, "9014"
HKR, Ndi\params\*JumboPacket,	Default,	0, "1514"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100 chip)
;
;-----------------------------------------------------------------------------
[yk60x64.FastFrSize.params]
HKR,, *JumboPacket,, "1514"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for battery powered Adapters
;
;----------------------------------------------------------------------------
[yk60x64.BatMax.params]

HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",		0, %SmartSpeed%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",		0, %MaxSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Default,	0, "4"

HKR, Ndi\Params\BatteryModeLinkDetection,		ParamDesc,	0, %BatLinkDet%
HKR, Ndi\Params\BatteryModeLinkDetection,		Type,		0, "enum"
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"0",		0, %NoPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"1",		0, %MaxPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"4",		0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection,		Default,	0, "4"

HKR,, BatteryCheckInterval,, "20000"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for reduced battery powered Adapters
;
;-----------------------------------------------------------------------------
[yk60x64.BatMaxRed.params]

HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",		0, %SmartSpeed%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",		0, %MaxSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Default,	0, "4"

HKR, Ndi\Params\BatteryModeLinkDetection,		ParamDesc,	0, %BatLinkDet%
HKR, Ndi\Params\BatteryModeLinkDetection,		Type,		0, "enum"
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"0",		0, %NoPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"4",		0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection,		Default,	0, "4"

HKR,, BatteryCheckInterval,, "20000"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for battery powered Adapters
;
;-----------------------------------------------------------------------------
[yk60x64.BatSmart.params]

HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",		0, %SmartSpeed%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",		0, %MaxSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Default,	0, "3"

HKR, Ndi\Params\BatteryModeLinkDetection,		ParamDesc,	0, %BatLinkDet%
HKR, Ndi\Params\BatteryModeLinkDetection,		Type,		0, "enum"
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"0",		0, %NoPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"1",		0, %MaxPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"4",		0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection,		Default,	0, "1"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan
;
;-----------------------------------------------------------------------------
[yk60x64.WoLStd.params]

HKR, Ndi\Params\WakeUpModeCap_A,		ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"28",		0, %LinkChange%
HKR, Ndi\Params\WakeUpModeCap_A,		Default,	0, "27"

[yk60x64.DefaultWfSOFF.params]

HKR, Ndi\Params\WakeFromShutdown,		ParamDesc,	0, %WakeFromShut%
HKR, Ndi\Params\WakeFromShutdown,		Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",		0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",		0, %Off%
HKR, Ndi\Params\WakeFromShutdown,		Default,	0, "0"

HKR,, WakeFromShutdown,, "0" 
 
[yk60x64.DefaultWfSON.params]

HKR, Ndi\Params\WakeFromShutdown,		ParamDesc,	0, %WakeFromShut%
HKR, Ndi\Params\WakeFromShutdown,		Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",		0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",		0, %Off%
HKR, Ndi\Params\WakeFromShutdown,		Default,	0, "1"

HKR,, WakeFromShutdown,, "1" 

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan dual port adapters
;
;-----------------------------------------------------------------------------
[yk60x64.WoLDL.params]

HKR, Ndi\Params\WakeUpModeCap_A,		ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap_A,		Default,	0, "25"

HKR, Ndi\Params\WakeFromShutdown,		ParamDesc,	0, %WakeFromShut%
HKR, Ndi\Params\WakeFromShutdown,		Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",		0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",		0, %Off%
HKR, Ndi\Params\WakeFromShutdown,		Default,	0, "0"

HKR,, WakeFromShutdown,, "0" 
HKR,, WakeUpModeCap_A,, "25"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan variant 1
;
;-----------------------------------------------------------------------------
[yk60x64.WoLWfSForcedCombine.params]

HKR, Ndi\Params\WakeUpModeCap_A,		ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"28",		0, %LinkChange%
HKR, Ndi\Params\WakeUpModeCap_A,		Default,	0, "27"

HKR,, WakeFromShutdown,, "1" 
HKR,, WakeFromShutdownMode,, "17"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan variant 2
;
;-----------------------------------------------------------------------------
[yk60x64.WoLNoLnkCh.params]

HKR, Ndi\Params\WakeUpModeCap_A,		ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap_A,		Default,	0, "27"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan variant 3
;
;-----------------------------------------------------------------------------
[yk60x64.WoLMagicPkt.params]

HKR, Ndi\Params\WakeUpModeCap_A,		ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap_A,		Default,	0, "25"


[yk60x64.WfSON.params]

HKR,, WakeFromShutdown,, "1" 

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters
;
;-----------------------------------------------------------------------------
[yk60x64.WoLW10.params]

HKR,, WakeUpSpeed,, "2"
;-----------------------------------------------------------------------------
;
; Additional Driver Parameters HwFeaDev
;
;-----------------------------------------------------------------------------
[yk60x64.HwFeaDev.params]

HKR,, HwFeaOnMask,,	"16777216"
HKR,, HwFeaOffMask,,	"0"
HKR,, HwDevOnMask,,	"0"
HKR,, HwDevOffMask,,	"0"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Auto-neg.
;
;-----------------------------------------------------------------------------
[yk60x64.FAN.params]

HKR,, HwFeaOnMask,,	"67108864"
HKR,, HwFeaOffMask,,	"0"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for forced Batterymode defaults.
;
;-----------------------------------------------------------------------------
[yk60x64.SmartBatDefaults.params]

HKR,, BatterySpeedSettings,, "3" 
HKR,, BatteryModeLinkDetection,, "1" 

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TCP segmentation
;
;-----------------------------------------------------------------------------
[yk60x64.TcpSegm.params]

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, %LSOv1%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, "1"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TCP segmentation with default value set to Off.
;
;-----------------------------------------------------------------------------
[yk60x64.TcpSegmLSOff.params]

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, %LSOv1%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, "0"

HKR,, TcpLargeSend,,  "0"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Single Link Adapters
;
;-----------------------------------------------------------------------------
[yk60x64.SingleLink.params]

HKR, Ndi\Params\*PriorityVLANTag,		ParamDesc,	0, %PriorityVLAN%
HKR, Ndi\Params\*PriorityVLANTag,		Type,		0, "enum"
HKR, Ndi\Params\*PriorityVLANTag\enum,		"3",		0, %PrioVlanEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"2",		0, %VlanEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"1",		0, %PrioEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"0",		0, %PrioVLANDis%
HKR, Ndi\Params\*PriorityVLANTag,		Default,	0, "0"

HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowCtrl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "3"

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Single Link Adapters (FlowControl OFF)
;
;-----------------------------------------------------------------------------
[yk60x64.SingleLinkFCOff.params]

HKR, Ndi\Params\*PriorityVLANTag,		ParamDesc,	0, %PriorityVLAN%
HKR, Ndi\Params\*PriorityVLANTag,		Type,		0, "enum"
HKR, Ndi\Params\*PriorityVLANTag\enum,		"3",		0, %PrioVlanEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"2",		0, %VlanEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"1",		0, %PrioEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"0",		0, %PrioVLANDis%
HKR, Ndi\Params\*PriorityVLANTag,		Default,	0, "0"

HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowCtrl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "0"

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"

;-----------------------------------------------------------------------------
;
; Additional driver parameter to set the port speed and capabilities
;
;-----------------------------------------------------------------------------
[yk60x64.SLSpeedDuplex.params]

HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "0"
HKR,Ndi\Params\*SpeedDuplex\enum, "0",        0, %Autosense%
HKR,Ndi\Params\*SpeedDuplex\enum, "1",        0, %10MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "2",        0, %10MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%

HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowCtrl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "3"
;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Dual Link Adapters
;
;-----------------------------------------------------------------------------
[yk60x64.DualLink.params]

HKR, Ndi\Params\PriorityVLANTag,		ParamDesc,	0, %PriorityVLAN%
HKR, Ndi\Params\PriorityVLANTag,		Type,		0, "enum"
HKR, Ndi\Params\PriorityVLANTag\enum,		"3",		0, %PrioVlanEna%
HKR, Ndi\Params\PriorityVLANTag\enum,		"2",		0, %VlanEna%
HKR, Ndi\Params\PriorityVLANTag\enum,		"1",		0, %PrioEna%
HKR, Ndi\Params\PriorityVLANTag\enum,		"0",		0, %PrioVLANDis%
HKR, Ndi\Params\*PriorityVLANTag,		Default,	0, "0"



HKR, Ndi\Params\RlmtMode,		ParamDesc,	0, %RLMT%
HKR, Ndi\Params\RlmtMode,		Type,		0, "enum"
HKR, Ndi\Params\RlmtMode\enum,	"1",		0, %Link%
HKR, Ndi\Params\RlmtMode\enum,	"3",		0, %OtherPort%
HKR, Ndi\Params\RlmtMode\enum,	"7",		0, %Segment%
HKR, Ndi\Params\RlmtMode,		Default,	0, "1"

HKR, Ndi\Params\PreferredPort,		ParamDesc,	0, %Preferred%
HKR, Ndi\Params\PreferredPort,		Type,		0, "enum"
HKR, Ndi\Params\PreferredPort\enum,	"1",		0, %A%
HKR, Ndi\Params\PreferredPort\enum,	"2",		0, %B%
HKR, Ndi\Params\PreferredPort,		Default,	0, "1"


HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"
HKR,, RlmtChgBCPrio,, "0"

;-----------------------------------------------------------------------------
;
; Additional driver parameter to set the port speed and capabilities
;
;-----------------------------------------------------------------------------
[yk60x64.DLSpeedDuplex.params]

HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "0"
HKR,Ndi\Params\*SpeedDuplex\enum, "0",        0, %Autosense%
HKR,Ndi\Params\*SpeedDuplex\enum, "1",        0, %10MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "2",        0, %10MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%
;-----------------------------------------------------------------------------
;
; General Registry Entries
;
;-----------------------------------------------------------------------------
[yk60x64.reg]

HKR, Ndi\Interfaces, UpperRange,, "ndis5"

HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "yukonx64"

;-----------------------------------------------------------------------------
;
; Special Registry Entrries
;
;-----------------------------------------------------------------------------
[yk60x64.YKVS_SL]

;Key used by notify object
HKR,, YKVS,, "762751"

;-----------------------------------------------------------------------------
;
; Special Registry Entrries
;
;-----------------------------------------------------------------------------
[yk60x64.YKVS_DL]

;Key used by notify object
HKR,, YKVS,, "762752"




;-----------------------------------------------------------------------------
;
; Service
;
;-----------------------------------------------------------------------------
[yukonx64.Service]
DisplayName	= %yk60x64.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\yk60x64.sys
LoadOrderGroup = NDIS


;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.EventLog]
AddReg = common.AddEventLog.reg

;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\yk60x64.sys"
HKR,, TypesSupported,	0x00010001, 7


;-----------------------------------------------------------------------------
;
; Source Files
;
;-----------------------------------------------------------------------------
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
yk60x64.sys	= 1,,

[yk60x64.CopyFiles]
yk60x64.sys,,,2


;-----------------------------------------------------------------------------
;
; Destination Directories
;
;-----------------------------------------------------------------------------
[DestinationDirs]

DefaultDestDir = 12
yk60x64.CopyFiles	= 12

;-----------------------------------------------------------------------------
;
; Localizable Strings
;
;-----------------------------------------------------------------------------
[Strings]

Marvell = "TP-LINK"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Jumbo Packet"
ReceiveBuffers = "Receive Buffers"
TransmitBuffers = "Transmit Buffers"
IPChksumOffv4 = "IPv4 Checksum Offload"
TCPChksumOffv4 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 = "UDP Checksum Offload (IPv6)"
LSOv1 = "Large Send Offload (IPv4)"
LSOv2IP4 = "Large Send Offload v2 (IPv4)"
LSOv2IP6 = "Large Send Offload v2 (IPv6)"
PriorityVLAN = "Priority & VLAN"
RSS = "Receive Side Scaling"
TXEna = "Tx Enabled"
RXEna = "Rx Enabled"
TXRXEna = "Tx & Rx Enabled"
PrioVlanDis = "Priority and VLAN Disabled"
PrioEna = "Priority Enabled"
VlanEna = "VLAN Enabled"
PrioVlanEna = "Priority & VLAN Enabled"

NetAddress   = "Network Address"
WakeUpCaps   = "Wake Up Capabilities"
IntMod = "Interrupt Moderation"
MaxIrq = "Max IRQ per Sec"
LogMsg = "Log Status Messages"
RLMT  = "RLMT Mode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Preferred Port"
On = "On"
Off = "Off"
Enabled = "Enabled"
Disabled = "Disabled"
Non = "None"
Err = "Errors"
Wrn = "Warnings"
Sta = "Status Messages"
All = "All Messages"
A = "A"
B = "B"
Autosense = "Auto Negotiation"
10MHD = "10 Mbps Half Duplex"
10MFD = "10 Mbps Full Duplex"
100MHD = "100 Mbps Half Duplex"
100MFD = "100 Mbps Full Duplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Link Change"
SpeedDuplex = "Speed & Duplex"
FlowCtrl = "FlowControl"
WakeFromShut = "Wake From Shutdown"
BatSpeed = "BatterySpeedSettings"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
;-----------------------------------------------------------------------------
DriverDisk = "TP-LINK TG-3201 Ethernet Controller Installation Disk"

AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


;-----------------------------------------------------------------------------

; Chinese (Taiwan)
[Strings.0404]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "特大包"
ReceiveBuffers = "接收緩衝"
TransmitBuffers = "傳輸緩衝"
IPChksumOffv4 = "卸載IPv4檢查和"
TCPChksumOffv4 = "卸載TCP檢查和(IPv4)"
TCPChksumOffv6 = "卸載TCP檢查和(IPv6)"
UDPChksumOffv4 = "卸載UDP檢查和(IPv4)"
UDPChksumOffv6 = "卸載UDP檢查和(IPv6)"
LSOv1 = "卸載超大發送(IPv4)"
LSOv2IP4 = "卸載超大發送v2(IPv4)"
LSOv2IP6 = "卸載超大發送v2(IPv6)"
PriorityVLAN = "802.1p優先權和VLAN"
RSS = "受端負載調節"
TXEna = "啟用Tx"
RXEna = "啟用Rx"
TXRXEna = "啟用Tx和Rx"
PrioVlanDis = "禁用優先權和VLAN"
PrioEna = "啟用優先權"
VlanEna = "啟用VLAN"
PrioVlanEna = "啟用優先權和VLAN"
NetAddress   = "網路位址"
WakeUpCaps   = "喚醒功能"
IntMod = "中斷模式"
MaxIrq = "最大 IRQ數量"
LogMsg = "日誌狀態訊息"
RLMT  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "偏好埠"
On = "開啟"
Off = "關閉"
Enabled = "啟用"
Disabled = "禁用"
Non = "無"
Err = "錯誤"
Wrn = "警告"
Sta = "狀態訊息"
All = "所有訊息"
A = "A"
B = "B"
Autosense = "自動感應"
10MHD = "10Mbps 半雙工"
10MFD = "10Mbps 全雙工"
100MHD = "100Mbps 半雙工"
100MFD = "100Mbps 全雙工"
MagicPacket = "Magic Packet喚醒模式"
PatternMatch = "Pattern Match喚醒模式"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Link Change喚醒模式"
SpeedDuplex = "速度和雙工"
FlowCtrl = "流量控制"
WakeFromShut = "從關閉狀態下喚醒"
BatSpeed = "電池狀態傳輸速度"
SmartSpeed = "智慧降速節能"
MaxSpeed = "全速"
BatLinkDet = "電池狀態鏈接偵測"
NoPwrSave = "無節能"
MaxPwrSave = "最大節能"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Greek
[Strings.0408]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Μεγάλο πακέτο"
ReceiveBuffers = "Προσωρινές μνήμες λήψης"
TransmitBuffers = "Προσωρινές μνήμες μετάδοσης"
IPChksumOffv4 = "ΠΔv4 άθρ.ελέγχου εκτός φορτ."
TCPChksumOffv4 = "ΠΕΜ άθρ.ελέγ.εκτός φορτ.(ΠΔv4)"
TCPChksumOffv6 = "ΠΕΜ άθρ.ελέγ.εκτός φορτ.(ΠΔv6)"
UDPChksumOffv4 = "ΠΔΧ άθρ.ελέγ.εκτός φορτ.(ΠΔv4)"
UDPChksumOffv6 = "ΠΔΧ άθρ.ελέγ.εκτός φορτ.(ΠΔv6)"
LSOv1 = "Μεγ. αποστ.εκτός φορτ.(ΠΔv4)"
LSOv2IP4 = "Μεγ.αποστ. εκτός φορτ.v2(ΠΔv4)"
LSOv2IP6 = "Μεγ.αποστ. εκτός φορτ.v2(ΠΔv6)"
PriorityVLAN = "802.1p Προτεραιότητα & VLAN"
RSS = "Κλιμάκωση όψης λήψης"
TXEna = "Αποστολή ενεργός"
RXEna = "Λήψη ενεργός"
TXRXEna = "Αποστολή & Λήψη ενεργός"
PrioVlanDis = "Προτερ. & VLAN ανενεργός"
PrioEna = "Προταιρεότητα ενεργός"
VlanEna = "VLAN ενεργός"
PrioVlanEna = "Προτερ. & VLAN ανενεργός"
NetAddress   = "Διεύθυνση δικτύου"
WakeUpCaps   = "Ικανότητες διέγερσης"
IntMod = "Μετρίαση διακοπών"
MaxIrq = "Μέγ. IRQ ανά sec"
LogMsg = "Μηνύματα  κατάστασης σύνδεσης"
RLMT  = "Λειτουργία RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Προτιμούμενη θύρα"
On = "On"
Off = "Off"
Enabled = "Ενεργοποιημένο"
Disabled = "Απενεργοποιημένο"
Non = "Κανένα"
Err = "Σφάλματα"
Wrn = "Προειδοποιήσεις"
Sta = "Μηνύματα κατάστασης"
All = "Όλα τα μηνύματα"
A = "A"
B = "B"
Autosense = "Αυτόματη ανίχνευση"
10MHD = "10Mbps ημιαμφίδρομος"
10MFD = "10Mbps αμφίδρομος"
100MHD = "100Mbps ημιαμφίδρομος"
100MFD = "100Mbps αμφίδρομος"
MagicPacket = "Μαγικό πακέτο"
PatternMatch = "Προσαρμογή σε πρότυπο"
MagPackPattMatch = "Μαγ. πακέτο&Προσρ. πρότ."
LinkChange = "Αλλαγή σύνδεσης"
SpeedDuplex = "Ταχύτητα & Αμφίδρομα"
FlowCtrl = "Έλεγχος ροής"
WakeFromShut = "Διέγερση από διακοπή"
BatSpeed = "Ρυθμίσεις ταχύτ. μπαταρίας"
SmartSpeed = "Μειωμένη ταχύτητα"
MaxSpeed = "Μέγιστη ταχύτητα"
BatLinkDet = "Ανίχνευση σύνδεσης λειτ. μπατ."
NoPwrSave = "Καμία οικονομία ενέργειας"
MaxPwrSave = "Μέγ. οικονομία ενέργειας"
EnDetPwrSave = "Ανίχνευση ενέργειας+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Dutch (Netherlands)
[Strings.0413]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Jumbo Packet"
ReceiveBuffers = "Ontvang Buffers"
TransmitBuffers = "Overdracht Buffers"
IPChksumOffv4 = "IPv4 Controletotaal Offload"
TCPChksumOffv4 = "TCP Controletotaal Offload (IPv4)"
TCPChksumOffv6 = "TCP Controletotaal Offload (IPv6)"
UDPChksumOffv4 = "UDP Controletotaal Offload (IPv4)"
UDPChksumOffv6 = "UDP Controletotaal Offload (IPv6)"
LSOv1 = "Groot Zend Offload (IPv4)"
LSOv2IP4 = "Groot Zend Offload v2 (IPv4)"
LSOv2IP6 = "Groot  Offload v2 (IPv6)"
PriorityVLAN = "802.1p Prioriteit & VLAN"
RSS = "Ontvang Side Scaling"
TXEna = "Tx ingeschakeld"
RXEna = "Rx ingeschakeld"
TXRXEna = "Tx & Rx ingeschakeld"
PrioVlanDis = "Prioriteit & VLAN uitgeschakeld"
PrioEna = "Prioriteit ingeschakeld"
VlanEna = "VLAN ingeschakeld"
PrioVlanEna = "Prioriteit & VLAN ingeschakeld"
NetAddress   = "Netwerkadres"
WakeUpCaps   = "Wake-up-vermogens"
IntMod = "Interrupt Moderatie"
MaxIrq = "Max IRQ per sec"
LogMsg = "Log-status meldingen"
RLMT  = "RlmtMode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Voorkeurspoort"
On = "Aan"
Off = "Uit"
Enabled = "Ingeschakeld"
Disabled = "Uitgeschakeld"
Non = "Geen"
Err = "Fouten"
Wrn = "Waarschuwingen"
Sta = "Statusberichten"
All = "Alle berichten"
A = "A"
B = "B"
Autosense = "Auto-sense"
10MHD = "10Mbps half duplex"
10MFD = "10Mbps full duplex"
100MHD = "100Mbps half duplex"
100MFD = "100Mbps full duplex"
MagicPacket = "Magic packet"
PatternMatch = "Pattern match"
MagPackPattMatch = "Magic packet & pattern match"
LinkChange = "Link verandering"
SpeedDuplex = "Speed & duplex"
FlowCtrl = "Flowcontrol"
WakeFromShut = "Wake from shutdown"
BatSpeed = "AccuSnelheidInstellingen"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "AccuModusLinkDetectie"
NoPwrSave = "Geen energiebesparing"
MaxPwrSave = "MaximumEnergiesparen"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Chinese (PRC)
[Strings.0804]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "特大包"
ReceiveBuffers = "接收缓冲"
TransmitBuffers = "传送缓冲"
IPChksumOffv4 = "卸载 IPv4 检查和"
TCPChksumOffv4 = "卸载 TCP 检查和 (IPv4)"
TCPChksumOffv6 = "卸载 TCP 检查和 (IPv6)"
UDPChksumOffv4 = "卸载 UDP 检查和 (IPv4)"
UDPChksumOffv6 = "卸载 UDP 检查和 (IPv6)"
LSOv1 = "卸载超大发送 (IPv4)"
LSOv2IP4 = "卸载超大发送 v2 (IPv4)"
LSOv2IP6 = "卸载超大发送 v2 (IPv6)"
PriorityVLAN = "802.1p 优先级和 VLAN"
RSS = "受端负载调节"
TXEna = "启用 Tx"
RXEna = "启用 Rx"
TXRXEna = "启用Tx 和 Rx"
PrioVlanDis = "禁用优先级和 VLAN"
PrioEna = "启用优先级"
VlanEna = "启用VLAN"
PrioVlanEna = "启用优先级和 VLAN"
NetAddress   = "网络地址"
WakeUpCaps   = "唤醒功能"
IntMod = "中断模式"
MaxIrq = "最大 IRQ数量"
LogMsg = "日志状态信息"
RLMT  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "首选端口"
On = "开"
Off = "关"
Enabled = "启用"
Disabled = "禁用"
Non = "无"
Err = "错误"
Wrn = "警告"
Sta = "状态信息"
All = "所有信息"
A = "A"
B = "B"
Autosense = "自动感应"
10MHD = "10Mbps 半双工"
10MFD = "10Mbps 全双工"
100MHD = "100Mbps 半双工"
100MFD = "100Mbps 全双工"
MagicPacket = "Magic Packet唤醒模式"
PatternMatch = "Pattern Match唤醒模式"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Link Change唤醒模式"
SpeedDuplex = "速度和双工"
FlowCtrl = "流控制"
WakeFromShut = "从关闭状态下唤醒"
BatSpeed = "电池状态传输速度"
SmartSpeed = "智慧降速节能"
MaxSpeed = "全速"
BatLinkDet = "电池状态链接侦测"
NoPwrSave = "无节能"
MaxPwrSave = "最大节能"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; German (Standard)
[Strings.0407]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Jumbo-Paket"
ReceiveBuffers = "Empfangspuffer"
TransmitBuffers = "Übertragungspuffer"
IPChksumOffv4 = "Verlagerung IPv4-Prüfsumme"
TCPChksumOffv4 = "Verlagerung TCP-Prüfsumme (IPv4)"
TCPChksumOffv6 = "Verlagerung TCP-Prüfsumme (IPv6)"
UDPChksumOffv4 = "Verlagerung UDP-Prüfsumme (IPv4)"
UDPChksumOffv6 = "Verlagerung UDP-Prüfsumme (IPv6)"
LSOv1 = "Übernahme TCP-Segment. (IPv4)"
LSOv2IP4 = "Übernahme TCP-Segment. V2 (IPv4)"
LSOv2IP6 = "Übernahme TCP-Segment. V2 (IPv6)"
PriorityVLAN = "802.1p Priorität & VLAN"
RSS = "Receive Side Scaling"
TXEna = "Tx aktiviert"
RXEna = "Rx aktiviert"
TXRXEna = "Tx & Rx aktiviert"
PrioVlanDis = "Priorität & VLAN deaktiviert"
PrioEna = "Priorität aktiviert"
VlanEna = "VLAN aktiviert"
PrioVlanEna = "Priorität & VLAN aktiviert"
NetAddress   = "Netzwerkadresse"
WakeUpCaps   = "Wake-up-Funktionen"
IntMod = "Interrupt-Moderation"
MaxIrq = "Max. IRQ pro Sek."
LogMsg = "Statusmeldungen protokollieren"
RLMT  = "RLMT-Modus"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Bevorzugter Port"
On = "Ein"
Off = "Aus"
Enabled = "Aktiviert"
Disabled = "Deaktiviert"
Non = "Keine"
Err = "Fehler"
Wrn = "Warnungen"
Sta = "Statusmeldungen"
All = "Alle Meldungen"
A = "A"
B = "B"
Autosense = "Automatische Erkennung"
10MHD = "10 Mbit/s Halbduplex"
10MFD = "10 Mbit/s Vollduplex"
100MHD = "100 Mbit/s Halbduplex"
100MFD = "100 Mbit/s Vollduplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Änderung des Linkstatus"
SpeedDuplex = "Geschwindigkeit und Duplexmodus"
FlowCtrl = "Datenflusskontrolle"
WakeFromShut = "Wake-up aus abgeschaltetem Zust."
BatSpeed = "Batteriemodus-Geschwindigkeit"
SmartSpeed = "Energiespar-Geschwindigkeit"
MaxSpeed = "Höchstgeschwindigkeit"
BatLinkDet = "Linkerkennung im Batteriemodus"
NoPwrSave = "Keine Energieeinsparung"
MaxPwrSave = "Maximale Energieeinsparung"
EnDetPwrSave = "EnergyDetect+™"










;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Spanish (Spain, Traditional Sort)
[Strings.040A]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Paquete Jumbo"
ReceiveBuffers = "Recibir búferes"
TransmitBuffers = "Transmitir búferes"
IPChksumOffv4 = "Desc. suma comp.IPv4"
TCPChksumOffv4 = "Desc. suma comp. TCP (IPv4)"
TCPChksumOffv6 = "Desc. suma comp. TCP (IPv6)"
UDPChksumOffv4 = "Desc. suma comp. UDP (IPv4)"
UDPChksumOffv6 = "Desc. suma comp. UDP (IPv6)"
LSOv1 = "Desc. envío grande (IPv4)"
LSOv2IP4 = "Desc. envío grande v2 (IPv4)"
LSOv2IP6 = "Desc. envío grande v2 (IPv6)"
PriorityVLAN = "802.1p prioridad y VLAN"
RSS = "Escala del lado de la recep."
TXEna = "Tx activado"
RXEna = "Rx activado"
TXRXEna = "Tx y Rx activados"
PrioVlanDis = "Prioridad y VLAN desactivados"
PrioEna = "Prioridad activada"
VlanEna = "VLAN activado"
PrioVlanEna = "Prioridad y VLAN activados"
NetAddress   = "Dirección de red"
WakeUpCaps   = "Capacidades de reactivación"
IntMod = "Moderación de interrupción"
MaxIrq = "IRQ máx. por seg."
LogMsg = "Mensajes de estado del registro"
RLMT  = "Modo RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Puerto preferido"
On = "Encendido"
Off = "Apagado"
Enabled = "Activado"
Disabled = "Desactivado"
Non = "Ninguna"
Err = "Errores"
Wrn = "Advertencias"
Sta = "Mensajes de estado"
All = "Todos los mensajes"
A = "A"
B = "B"
Autosense = "Orientación automática"
10MHD = "Dúplex media 10Mbps"
10MFD = "Dúplex completa 10Mbps"
100MHD = "Dúplex media 100Mbps"
100MFD = "Dúplex completa 100Mbps"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Cambio de enlace"
SpeedDuplex = "Velocidad y dúplex del enlace"
FlowCtrl = "Control de flujo"
WakeFromShut = "Wake From Shutdown"
BatSpeed = "BatterySpeedSettings"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; French (Standard)
[Strings.040C]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Paquet géant"
ReceiveBuffers = "Tampons de réception"
TransmitBuffers = "Tampons de transmission"
IPChksumOffv4 = "DéchargTotal de contrôle IPv4"
TCPChksumOffv4 = "DéchargTotalContrôle TCP(IPv4)"
TCPChksumOffv6 = "DéchargTotalContrôle TCP(IPv6)"
UDPChksumOffv4 = "DéchargTotalContrôle UDP(IPv4)"
UDPChksumOffv6 = "DéchargTotalContrôle UDP(IPv6)"
LSOv1 = "DéchargeEnvoiImportant (IPv4)"
LSOv2IP4 = "DéchargeEnvoiImportant v2 IPv4"
LSOv2IP6 = "DéchargeEnvoiImportant v2 IPv6"
PriorityVLAN = "Priorité 802.1p & VLAN"
RSS = "Distribution côté Rx"
TXEna = "Tx activée"
RXEna = "Rx activée"
TXRXEna = "Tx & Rx activées"
PrioVlanDis = "Priorité & VLAN désactivés"
PrioEna = "Priorité activée"
VlanEna = "VLAN activé"
PrioVlanEna = "Priorité & VLAN activés"

NetAddress   = "Adresse réseau"
WakeUpCaps   = "Capacités de réveil"
IntMod = "Modération de l'interruption"
MaxIrq = "IRQ max. par seconde"
LogMsg = "Messages d'état du journal"
RLMT  = "Mode RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Port préféré"
On = "Actif"
Off = "Inactif"
Enabled = "Activé(e)"
Disabled = "Désactivé(e)"
Non = "Aucun"
Err = "Erreurs"
Wrn = "Avertissements"
Sta = "Messages d'état"
All = "Tous les messages"
A = "A"
B = "B"
Autosense = "Détection automatique"
10MHD = "10 Mbits/s Semi-duplex"
10MFD = "10 Mbits/s Duplex intégral"
100MHD = "100 Mbits/s Semi-duplex"
100MFD = "100 Mbits/s Duplex intégral"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Changement du lien"
SpeedDuplex = "Vitesse de liaison et duplex"
FlowCtrl = "Contrôle de flux"
WakeFromShut = "Reveil de l'état arreté"
BatSpeed = "Vitesse en mode batterie"
SmartSpeed = "Reduction d'énergie"
MaxSpeed = "Pleine vitesse"
BatLinkDet = "Détection en mode batterie"
NoPwrSave = "Pas des économies d'énergie"
MaxPwrSave = "Économies d'énergie maximales"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Italian (Standard)
[Strings.0410]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pacchetto jumbo"
ReceiveBuffers = "Buffer di ricezione"
TransmitBuffers = "Buffer di trasmissione"
IPChksumOffv4 = "Checksum Offload IPv4"
TCPChksumOffv4 = "Checksum Offload TCP (IPv4)"
TCPChksumOffv6 = "Checksum Offload TCP (IPv6)"
UDPChksumOffv4 = "Checksum Offload UDP (IPv4)"
UDPChksumOffv6 = "Checksum Offload UDP (IPv6)"
LSOv1 = "Large Send Offload (IPv4)"
LSOv2IP4 = "Large Send Offload v2 (IPv4)"
LSOv2IP6 = "Large Send Offload v2 (IPv6)"
PriorityVLAN = "Priorità & VLAN 802.1p"
RSS = "Receive Side Scaling"
TXEna = "Tx abilitato"
RXEna = "Rx abilitato"
TXRXEna = "Tx & Rx abilitati"
PrioVlanDis = "Priorità & VLAN disabil."
PrioEna = "Priorità abilitata"
VlanEna = "VLAN abilitato"
PrioVlanEna = "Priorità & VLAN abilitati"
NetAddress   = "Indirizzo di rete"
WakeUpCaps   = "Funzioni Wake Up "
IntMod = "Moderazione interrupt"
MaxIrq = "Max IRQ per sec"
LogMsg = "Messaggi di stato registro"
RLMT  = "Modalità RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Porta preferita"
On = "Attivato"
Off = "Disattivato"
Enabled = "Attivato"
Disabled = "Disattivato"
Non = "Nessuno"
Err = "Errori"
Wrn = "Avvertenze"
Sta = "Messaggi di stato"
All = "Tutti i messaggi"
A = "A"
B = "B"
Autosense = "Autoriconoscimento"
10MHD = "10Mbps half duplex"
10MFD = "10Mbps full duplex"
100MHD = "100Mbps half duplex"
100MFD = "100Mbps full duplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Cambio collegamento"
SpeedDuplex = "Velocità di collegamento e duplex"
FlowCtrl = "Controllo del flusso"
WakeFromShut = "Wake From Shutdown"
BatSpeed = "BatterySpeedSettings"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Japanese
[Strings.0411]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "ジャンボ パケット"
ReceiveBuffers = "受信バッファ"
TransmitBuffers = "送信バッファ"
IPChksumOffv4 = "IPv4チェックサム オフロード"
TCPChksumOffv4 = "TCPチェックサム オフロード(IPv4)"
TCPChksumOffv6 = "TCPチェックサム オフロード(IPv6)"
UDPChksumOffv4 = "UDPチェックサム オフロード(IPv4)"
UDPChksumOffv6 = "UDPチェックサム オフロード(IPv6)"
LSOv1 = "大量送信オフロード (IPv4)"
LSOv2IP4 = "大量送信オフロード v2 (IPv4)"
LSOv2IP6 = "大量送信オフロード v2 (IPv6)"
PriorityVLAN = "802.1p 優先度オン & VLAN"
RSS = "RSS"
TXEna = "Tx 有効化"
RXEna = "Rx 有効化"
TXRXEna = "Tx & Rx 有効化"
PrioVlanDis = "優先度 & VLAN 無効化"
PrioEna = "優先度有効化"
VlanEna = "VLAN 有効化"
PrioVlanEna = "優先度 & VLAN 有効化"
NetAddress   = "ネットワークアドレス"
WakeUpCaps   = "ウェイク アップ機能"
IntMod = "割り込み節度"
MaxIrq = "毎秒最大 IRQ"
LogMsg = "ログ ステータス メッセージ"
RLMT  = "RLMTモード"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "優先ポート"
On = "オン"
Off = "オフ"
Enabled = "オン"
Disabled = "オフ"
Non = "なし"
Err = "エラー"
Wrn = "警告"
Sta = "ステータス メッセージ"
All = "全てのメッセージ"
A = "A"
B = "B"
Autosense = "自動感知"
10MHD = "10Mbps 半二重"
10MFD = "10Mbps 全二重"
100MHD = "100Mbps 半二重"
100MFD = "100Mbps 全二重"
MagicPacket = "マジック パケット"
PatternMatch = "パターン マッチ"
MagPackPattMatch = "マジック パケットとパターン マッチ"
LinkChange = "リンクの変更"
SpeedDuplex = "リンク速度とデュプレックス"
FlowCtrl = "フロー制御"
WakeFromShut = "シャットダウンからのウェイクアップ"
BatSpeed = "バッテリ速度設定"
SmartSpeed = "スマート速度制御"
MaxSpeed = "最大速度"
BatLinkDet = "バッテリ モード リンク検出"
NoPwrSave = "省エネなし"
MaxPwrSave = "最大省エネ"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Korean
[Strings.0412]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "점보 패킷"
ReceiveBuffers = "수신 버퍼"
TransmitBuffers = "송신 버퍼"
IPChksumOffv4 = "IPv4 검사합계 오프로드"
TCPChksumOffv4 = "TCP검사합계오프로드(IPv4)"
TCPChksumOffv6 = "TCP검사합계오프로드(IPv6)"
UDPChksumOffv4 = "UDP검사합계오프로드(IPv4)"
UDPChksumOffv6 = "UDP검사합계오프로드(IPv6)"
LSOv1 = "대량송신 오프로드(IPv4)"
LSOv2IP4 = "대량송신오프로드v2(IPv4)"
LSOv2IP6 = "대량송신오프로드v2(IPv6)"
PriorityVLAN = "802.1p우선순위&VLAN"
RSS = "수신 성능 확장 구조"
TXEna = "Tx 사용"
RXEna = "Rx 사용"
TXRXEna = "Tx & Rx 사용"
PrioVlanDis = "우선순위&VLAN미사용"
PrioEna = "우선순위 사용"
VlanEna = "VLAN 사용"
PrioVlanEna = "우선순위&VLAN 사용"
NetAddress   = "네트워크 주소"
WakeUpCaps   = "시스템 켜기 기능"
IntMod = "인터럽트 완화"
MaxIrq = "초당 최대 IRQ"
LogMsg = "로그 상태 메시지"
RLMT  = "RLMT 모드"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "기본 설정 포트"
On = "켜기"
Off = "끄기"
Enabled = "활성화됨"
Disabled = "활성 해제됨"
Non = "없음"
Err = "오류"
Wrn = "경고"
Sta = "상태 메시지"
All = "모든 메시지"
A = "A"
B = "B"
Autosense = "자동 감지"
10MHD = "10Mbps 반이중"
10MFD = "10Mbps 전이중"
100MHD = "100Mbps 반이중"
100MFD = "100Mbps 전이중"
MagicPacket = "매직 패킷"
PatternMatch = "패턴 일치"
MagPackPattMatch = "매직 패킷 및 패턴 일치"
LinkChange = "링크 변경"
SpeedDuplex = "링크 속도 및 이중성"
FlowCtrl = "흐름 제어"
WakeFromShut = "종료 상태에서 깨우기"
BatSpeed = "배터리속도설정"
SmartSpeed = "스마트감속"
MaxSpeed = "최대속도"
BatLinkDet = "배터리모델링크감지"
NoPwrSave = "절전안함"
MaxPwrSave = "최대절전"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Polish
[Strings.0415]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pakiet Jumbo"
ReceiveBuffers = "Bufory odbioru"
TransmitBuffers = "Bufory nadawcze"
IPChksumOffv4 = "IPv4 ob. sumy kon."
TCPChksumOffv4 = "ob. sumy kon. pak. TCP (IPv4)"
TCPChksumOffv6 = "ob. sumy kon. pak. TCP (IPv6)"
UDPChksumOffv4 = "ob. sumy kon. pak. UDP (IPv4)"
UDPChksumOffv6 = "ob. sumy kon. pak. UDP (IPv6)"
LSOv1 = "obs. wys. du. il da.(IPv4)"
LSOv2IP4 = "obs. wys. du. il da. v2 (IPv4)"
LSOv2IP6 = "obs. wys. du. il da. v2 (IPv6)"
PriorityVLAN = "802.1p Priorytet & VLAN"
RSS = "roz. ru. przy. do wiel. ukł."
TXEna = "Bufory nadawcze wł."
RXEna = "Bufory odbiorcze wł."
TXRXEna = "Buf. nad. & odb. wł."
PrioVlanDis = "Priorytet & VLAN wył."
PrioEna = "Priorytet wł."
VlanEna = "VLAN Włączony"
PrioVlanEna = "Priorytet & VLAN wł."
NetAddress   = "Adres sieciowy"
WakeUpCaps   = "Funkcje budzenia"
IntMod = "Moderacja przerwania"
MaxIrq = "Maks. IRQ na sek."
LogMsg = "Zapisywanie komunikatów o stat."
RLMT  = "RLMT Mode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Preferowany port"
On = "Włączone"
Off = "Wyłączone"
Enabled = "Włączony"
Disabled = "Wyłączony"
Non = "Żadne"
Err = "Błędy"
Wrn = "Ostrzeżenia"
Sta = "Komunikaty o stanie"
All = "Wszystkie komunikaty"
A = "A"
B = "B"
Autosense = "Automatyczne wykrywanie"
10MHD = "10 Mbps Półdupleks"
10MFD = "10 Mbps Pełen dupleks"
100MHD = "100 Mbps Półdupleks"
100MFD = "100 Mbps Pełen dupleks"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Zmiana łącza"
SpeedDuplex = "Szybkość i Dupleks"
FlowCtrl = "Kontrola przepływu danych"
WakeFromShut = "Uaktywnianie z Wyłączenia"
BatSpeed = "Szybkość w trybie bateryjnym"
SmartSpeed = "Zmniejszona szybkość łącza"
MaxSpeed = "Maksymalna szybkość łącza"
BatLinkDet = "Wykrywanie łącza w trybie bat."
NoPwrSave = "Bez oszczędności energii"
MaxPwrSave = "Maks. oszczędność energii"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Portuguese (Brazil)
[Strings.0416]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pacote Jumbo"
ReceiveBuffers = "Buffers de Recepção"
TransmitBuffers = "Buffers de Transmissão"
IPChksumOffv4 = "Descarga Soma de Verif. IPv4"
TCPChksumOffv4 = "Desc. Soma Verif. TCP (IPv4)"
TCPChksumOffv6 = "Desc. Soma Verif. TCP (IPv6)"
UDPChksumOffv4 = "Desc. Soma Verif. UDP (IPv4)"
UDPChksumOffv6 = "Desc. Soma Verif. UDP (IPv6)"
LSOv1 = "Grande Desc. Envio (IPv4)"
LSOv2IP4 = "Grande Desc. Envio v2 (IPv4)"
LSOv2IP6 = "Grande Desc. Envio v2 (IPv6)"
PriorityVLAN = "802.1p Prior. & VLAN"
RSS = "Escalamento Lado Receptor"
TXEna = "Tx habilitado"
RXEna = "Rx habilitado"
TXRXEna = "Tx & Rx habilitado"
PrioVlanDis = "Prior. & VLAN desabil."
PrioEna = "Prioridade habilitada"
VlanEna = "VLAN habilitado"
PrioVlanEna = "Prioridade & VLAN habil."

NetAddress   = "Endereço de Rede"
WakeUpCaps   = "Capacidades de Despertar"
IntMod = "Moderação de Interrupção"
MaxIrq = "IRQ Máx por Seg"
LogMsg = "Registrar Mensagens de Estado"
RLMT  = "Modo RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Porta Preferida"
On = "Ligado"
Off = "Desligado"
Enabled = "Ativado"
Disabled = "Desativado"
Non = "Nenhum"
Err = "Erros"
Wrn = "Avisos"
Sta = "Mensagens de Estado"
All = "Todas as Mensagens"
A = "A"
B = "B"
Autosense = "Autodetecção"
10MHD = "Semi Dúplex 10Mbps"
10MFD = "Dúplex Completo 10Mbps"
100MHD = "Semi Dúplex 100Mbps"
100MFD = "Dúplex Completo100Mbps"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Troca de Vínculo"
SpeedDuplex = "Velocidade de link e duplex"
FlowCtrl = "Controle de Fluxo"
WakeFromShut = "Wake From Shutdown"
BatSpeed = "BatterySpeedSettings"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"


; Russian
[Strings.0419]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Большой пакет"
ReceiveBuffers = "Буферы приема"
TransmitBuffers = "Буферы передачи"
IPChksumOffv4 = "Разг.контр.суммы IPv4"
TCPChksumOffv4 = "Разг.контр.суммы TCP (IPv4)"
TCPChksumOffv6 = "Разг.контр.суммы TCP (IPv6)"
UDPChksumOffv4 = "Разг.контр.суммы UDP (IPv4)"
UDPChksumOffv6 = "Разг.контр.суммы UDP (IPv6)"
LSOv1 = "Разг.больш.передач (IPv4)"
LSOv2IP4 = "Разг.больш.передач v2 (IPv4)"
LSOv2IP6 = "Разг.больш.передач v2 (IPv6)"
PriorityVLAN = "802.1p приоритет и VLAN"
RSS = "Масшт. на стор. приемника"
TXEna = "Tx включен"
RXEna = "Rx включен"
TXRXEna = "Tx & Rx включен"
PrioVlanDis = "Приоритет и VLAN откл."
PrioEna = "Приоритет включен"
VlanEna = "VLAN включен"
PrioVlanEna = "Приоритет и VLAN вкл."
NetAddress   = "Сетевой адрес"
WakeUpCaps   = "Возможности пробуждения"
IntMod = "Управление прерываниями"
MaxIrq = "Макс. IRQ - шт/сек."
LogMsg = "Записывать статус. сообщения"
RLMT  = "Режим RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Предпочтительный порт"
On = "Вкл."
Off = "Выкл."
Enabled = "Включать" 
Disabled = "Отключать"
Non = "Нет"
Err = "Ошибки"
Wrn = "Предупреждения"
Sta = "Статусные сообщения"
All = "Все сообщения"
A = "A"
B = "B"
Autosense = "Автоопределение"
10MHD = "10Мбит/с полудуплекс"
10MFD = "10Мбит/с полный дуплекс"
100MHD = "100Мбит/с полудуплекс"
100MFD = "100Мбит/с полный дуплекс"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Измен. статуса соединения"
SpeedDuplex = "Скорость и дуплекс"
FlowCtrl = "Управление потоком данных"
WakeFromShut = "Просыпаться от выключение"
BatSpeed = "Cкорость передачи от батареи"
SmartSpeed = "Уменьшение скорости"
MaxSpeed = "Макс. скорость передачи"
BatLinkDet = "Обнаружение канала от батареи"
NoPwrSave = "Без экономии энергии"
MaxPwrSave = "Mакс. экономии энергии"
EnDetPwrSave = "EnergyDetect+™"

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2916.DeviceDesc = "Allied Telesyn AT-2916T"
AT-2973.DeviceDesc = "Allied Telesyn AT-2971SX/SC-001"
AT-2973_1.DeviceDesc = "Allied Telesyn AT-2971SX Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesyn AT-2971T-001"
AT-2974_1.DeviceDesc = "Allied Telesyn AT-2971T Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesyn AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4B03.DeviceDesc = "D-Link DGE-550T Gigabit Ethernet Adapter V.B1"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
Yukon-Generic.DeviceDesc = "TP-LINK TG-3201 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
yk60x64.DriverDesc	= "NDIS6.0 Miniport Driver for Marvell Yukon Ethernet Controller"
