****************************************************************************
		    TP-LINK TECHNOLOGIES CO., LTD.     
		       TP-LINK TFF-3283 10/100M Fast Ethernet Adapter                   

	   NDIS 5 Miniport Driver For Windows 98/98_SE Installation 
	   ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

	   Copyright (C) 2000 Fast Ethernet Controller Provider Inc.     
			     All rights reserved.
****************************************************************************

The driver conforms to the Network Driver Interface Specification (NDIS)5.0,
and used with Microsoft Windows OS.




Contents
--------
    A) Install NDIS5.0 Miniport driver to Microsoft Windows 98/98_SE
    B) Configure NDIS5.0 Miniport driver to Microsoft Windows 98/98_SE

	

A) Installing NDIS 5 Miniport driver to Microsoft Windows 98/98_SE
==================================================================

  1. Plug the TP-LINK TFF-3283 10/100M Fast Ethernet Adapter into one of the Master PCI                   
     slots of your PCI platform.

  2. Turn ON the power of PC then boot into Windows 98/98_SE.

  3. Windows 98/98_SE will prompt "PCI Ethernet Controller" in "New Hardware 
     Found" dialog box and "Update Device Driver Wizard" dialog box.

  4. Click "Next" button when "Search for the best driver for your device"
     [Recommended] is on.

  5. Insert the TP-LINK TFF-3283 10/100M Fast Ethernet Adapter Driver Diskette in your                   
     floppy drive.

  6. Disable the "Floppy disk drives" check box. Click "Specify a location",
     type "A:\WIN98" and then click "Next" button.

  7. Windows 98/98_SE will prompt "TP-LINK TFF-3283 10/100M Fast Ethernet Adapter" in "Add                   
     New Hardware Wizard" dialog box.

  8. Click "Next" button and Windows starts to copy files from Windows
     98/98_SE CD-ROM to your hard disk.

  9. Click "Finish" button from "Add New Hardware Wizard" dialog box.

 10. Remove the Adapter Driver Diskette from your floppy drive.

 11. Restart your computer to implement the network function.



B) Configuring NDIS5.0 Miniport driver to Microsoft Windows 98/98_SE
====================================================================
  1. Click the "My Computer" icon in the Main Program Group.

  2. Click the "Control Panel" icon from My Computer window.

  3. Click the "Network" icon from the Control Panel window.

  4. Select "TP-LINK TFF-3283 10/100M Fast Ethernet Adapter" item from "Network" dialog box,                    
     then click "Properties" button.

  5. Click "Advanced" button from "TP-LINK TFF-3283 10/100M Fast Ethernet Adapter Properties"                   
     dialog box.

  6. Select the Media Type value (AutoDetect, 10BaseT, 10BaseT Full_Duplex,
     100BaseTX, 100BaseTX Full_Duplex) from "Value" item, then click OK 
     button from "TP-LINK TFF-3283 10/100M Fast Ethernet Adapter Properties" dialog box.                   

  7. Click OK button from "Network" dialog box.

  8. Restart your computer for the new configuration to take effect.




Trademarks:
Microsoft Windows 98 and 98_SE is a trademark of Microsoft Corporation.

