****************************************************************************
		    TP-LINK TECHNOLOGIES CO., LTD.      
		       TP-LINK TF-3283 10/100M Fast Ethernet Adapter                     

	      NDIS 5 Miniport Driver For Windows ME Installation
	      ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

	   Copyright (C) 2000 TP-LINK TECHNOLOGIES CO., LTD.     
			     All rights reserved.
****************************************************************************

The driver conforms to the Network Driver Interface Specification (NDIS)5.0,
and used with Microsoft Windows OS.


Contents
--------
    A) Install NDIS5.0 Miniport driver to Microsoft Windows ME
    B) Configure NDIS5.0 Miniport driver to Microsoft Windows ME

	
A) Installing NDIS 5 Miniport driver to Microsoft Windows ME
============================================================

  1. Plug the TP-LINK TF-3283 10/100M Fast Ethernet Adapter into one of the Master PCI                   
     slots of your PCI platform.

  2. Turn ON the power of PC then boot into Windows ME.

  3. Windows ME will prompt "PCI Ethernet Controller" in "New Hardware Found" 
     dialog box and "Update Device Driver Wizard" dialog box.

  4. Click "Next" button when "Search for the best driver for your device"
     [Recommended] is on.

  5. Insert the TP-LINK TF-3283 10/100M Fast Ethernet Adapter Driver Diskette in your                   
     floppy drive.

  6. Disable the "Floppy disk drives" check box. Click "Specify a location",
     type "A:\WINME" and then click "Next" button.

  7. Windows ME will prompt "TP-LINK TF-3283 10/100M Fast Ethernet Adapter" in "Add New                   
     Hardware Wizard" dialog box.

  8. Click "Next" button and Windows starts to copy files from Windows ME 
     CD-ROM to your hard disk.

  9. Click "Finish" button from "Add New Hardware Wizard" dialog box.

 10. Remove the Adapter Driver Diskette from your floppy drive.

 11. Restart your computer to implement the network function.



B) Configuring NDIS5.0 Miniport driver to Microsoft Windows ME
==============================================================
  1. Click the "My Computer" icon in the Main Program Group.

  2. Click the "Control Panel" icon from My Computer window.

  3. Click the "Network" icon from the Control Panel window.

  4. Select "TP-LINK TF-3283 10/100M Fast Ethernet Adapter" item from "Network" dialog box,                   
     then click "Properties" button.

  5. Click "Advanced" button from "TP-LINK TF-3283 10/100M Fast Ethernet Adapter Properties"                   
     dialog box.

  6. Select the Media Type value (AutoDetect, 10BaseT, 10BaseT Full_Duplex,
     100BaseTX, 100BaseTX Full_Duplex) from "Value" item, then click OK 
     button from "TP-LINK TF-3283 10/100M Fast Ethernet Adapter Properties" dialog box.                   

  7. Click OK button from "Network" dialog box.

  8. Restart your computer for the new configuration to take effect.




Trademarks:
Microsoft Windows ME is a trademark of Microsoft Corporation.

