Installing the NDIS2 driver for CardBus card is the same as for PCI card, 
in addition to the following steps:


After install driver in Microsoft Client or Windows 3.11

1. Check config.sys and remove the argument "NOEMS" of EMM386.sys
2. Copy rtpci.exe and rtbios.com to any directory. 
   Example     c:\wfw311
3. In autoexec.bat, add two lines of command, "rtpci /md000 /i11" 
   and "rtbios" in front of "net start" and "net initialize".  
   Example:
	If only "net start" exists,
    		
		:
		:
		c:\wfw311\rtpci.exe /md000 /i11   
		c:\wfw311\rtbios.com
		c:\wfw311\net start
		:
		:
	
	or if "net initialize" exists, 
    		
		:
		:
		c:\wfw311\rtpci.exe /md000 /i11   
		c:\wfw311\rtbios.com
		c:\wfw311\net initialize
		:
		:
 
4. Restart the computer.           