;*******************************************************************************
; Module Description:
;
; InfVersion   10.26.0.0.D
;
;*******************************************************************************

[Identification]
    OptionType = NetAdapter


[Options]
    B57NT4


[PlatformsSupported]
    PCI


[LanguagesSupported]
    ENG, English


[RequestedMediaTypeB57NT4]
    "Auto",                                 0
    "10 Mb Half",                           3
    "10 Mb Full",                           4
    "100 Mb Half",                          5
    "100 Mb Full",                          6


[FlowControlCapB57NT4]
    "Disable",                              0
    "Rx Pause",                             1
    "Tx Pause",                             2
    "Rx/Tx Pause",                          3
    "Auto",                                 2147483648


[RxMtuB57NT4]
    "1500",                                 1500
    "2000",                                 2000
    "2500",                                 2500
    "3000",                                 3000
    "3500",                                 3500
    "4000",                                 4000
    "4500",                                 4500
    "5000",                                 5000
    "5500",                                 5500
    "6000",                                 6000
    "6500",                                 6500
    "7000",                                 7000
    "7500",                                 7500
    "8000",                                 8000
    "8500",                                 8500
    "9000",                                 9000


[OptionsTextENG]
    B57NT4 = "Gigabit Ethernet Controller"


[FileConstants]
    UtilityInf      = "UTILITY.INF"
    SubroutineInf   = "SUBROUTN.INF"

    MAXIMUM_ALLOWED = 33554432
    NoTitle         = 0

    Manufacturer        = "Broadcom"
    ProductMajorVersion = "10"
    ProductMinorVersion = "26"
    ProductVersion      = $(ProductMajorVersion)"."$(ProductMinorVersion)

    NetEventDll              = "%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\drivers\B57NT4.sys"
    ProductSoftwareImagePath = "\SystemRoot\System32\drivers\B57NT4.sys"
    B57dtectDll              = "b57dtect.dll"

    MiniportProductName              = "B57NT4"
    MiniportProductKeyName           = $(!NTN_SoftwareBase)"\"$(Manufacturer)+
                                       "\"$(MiniportProductName)+
                                       "\CurrentVersion"
    MiniportSoftwareType             = "driver"

    MiniportNetRuleSoftwareUse       = $(MiniportSoftwareType)
    MiniportNetRuleSoftwareClass     = {"B57NT4Driver basic"}
    MiniportNetRuleSoftwareType      = "B57NT4Sys ndisDriver B57NT4Driver"
    MiniportNetRuleSoftwareBindForm  = """B57NT4Sys"" yes no container"
    MiniportNetRuleSoftwareBindable  = {"B57NT4Driver B57NT4Adapter non "+
                                        "exclusive 100"}

    MiniportNetRuleHardwareType      = "B57NT4 B57NT4Adapter"
    MiniportNetRuleHardwareBindForm  = " yes yes container"
    MiniportNetRuleHardwareClass     = {"B57NT4Adapter basic"}

    ServiceKeyName                   = "SYSTEM\CurrentControlSet\Services"

    NetworkCardKeyName               = $(!NTN_SoftwareBase)"\Microsoft\"+
        "Windows NT\CurrentVersion\NetworkCards"

    B57NT4HelpId                     = 100
    B57NT4HelpFile                   = "b57nt4.hlp"

    IBM_HPP_ServiceKey               = "SYSTEM\CurrentControlSet\Services\"+
        "HotSrv\SupportedDevices\14E4-1644-14E4-1644"
    CPQ_HPP_Key                      = "SOFTWARE\Compaq\Cpqrcmc\ClassDLLs\"+
        "NicMiniPort"


[FileConstantsENG]
    FunctionB57NT4Title = "Broadcom NetXtreme Gigabit Ethernet"

    MiniportProductSoftwareTitle       = $(FunctionB57NT4Title)
    MiniportProductSoftwareDisplayName = "Broadcom NetXtreme Gigabit Ethernet"

    MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Ethernet"
    MiniportB57NT4Description   = "Broadcom NetXtreme Gigabit Ethernet NDIS 4.0 Driver "+
        "Version "$(ProductVersion)"."

    MessageBoxTitle = "Gigabit Ethernet Driver"

    MsgShellErrorTitle  = "Error: "$(Function$(OptionId)Title)
    MsgShellErrorText   = "Shell Code Error."
    MsgRegistryKeyDoesNotExist = "Open registry key failed."
    MsgNoAdapterFound = "Network card is not present in the system."
    MsgDowngrade = "Cannot downgrade to an older driver.  To downgrade, "+
        "you must uninstall first and then re-install the older driver."
    MsgUpdateDone = "Driver update will take effect on the next reboot."
    MsgCannotFindB57dtectDll = "Cannot load B57dtect.dll file."
    MsgUntestedServicePack = "The Gigabit driver has not been tested on "+
        "this Service Pack release.  We recommend that you apply Service "+
        "Pack 4 or greater upon completion of the driver installation.  "+
        "Would you like to continue?"


[DialogConstantsENG]
    Help        = "&Help"
    Exit        = "C&ancel"
    OK          = "&OK"
    HelpContext = ""
    Continue    = "&Continue"
    Cancel      = "C&ancel"


[RequestedMediaTypeDlgENG]
    DlgText     = "Select the line speed and duplex mode to connect "+
                  "to the network.  The recommended selection is 'Auto' "+
                  "which sets up the adapter to auto detect the optimal "+
                  "connection."
    DlgTemplate = "WD"
    DlgType     = "Combination"
    Caption     = "Configurable Driver Parameters."
    Combo1Label = "&Speed && Duplex:"
    Combo1List  = $(ConnectionList)
    Combo1Out   = $(ConnectionValue)
    Combo2Label = "&Flow Control:"
    Combo2List  = $(FlowControlCapList)
    Combo2Out   = $(FlowControlCapValue)
    Combo3Label = "&Jumbo Mtu:"
    Combo3List  = $(RxMtuList)
    Combo3Out   = $(RxMtuValue)
    ComboListItemsIn  = { Combo1List, Combo2List, Combo3List }
    ComboListItemsOut = { Combo1Out, Combo2Out, Combo3Out }
    EditTextLim = ""
    CBOptionsGreyed = {}
    MinHelpId = 100
    MaxHelpId = 1000
    HelpContext = $($(OptionId)HelpId)

[RequestedMediaTypeADlgENG]
    DlgText     = "Select the line speed and duplex mode to connect "+
                  "to the network.  The recommended selection is 'Auto' "+
                  "which sets up the adapter to auto detect the optimal "+
                  "connection."
    DlgTemplate = "NE2000"
    DlgType     = "Combination"
    Caption     = "Configurable Driver Parameters."
    Label1 = "&Speed && Duplex:"
    Label2 = "&Flow Control:"
;    Combo1Label = "&Speed && Duplex:"
    Combo1List  = $(ConnectionList)
    Combo1Out   = $(ConnectionValue)
;    Combo2Label = "&Flow Control:"
    Combo2List  = $(FlowControlCapList)
    Combo2Out   = $(FlowControlCapValue)
    ComboListItemsIn  = { Combo1List, Combo2List } 
    ComboListItemsOut = { Combo1Out, Combo2Out } 
    EditTextLim = ""
    CBOptionsGreyed = {}
    MinHelpId = 100
    MaxHelpId = 1000
    HelpContext = $($(OptionId)HelpId)


[DebugControl]
    !DebugOutputControl = 0


[CurrentDate]
    Now = {} ? $(!LIBHANDLE) GetSystemDate


[Source Media Descriptions]
    1 = "Broadcom NetXtreme Installation Media", TAGFILE = b57nt4.sys


[Files-B57NT4Driver]
    1, b57nt4.sys, SIZE=999


[Files-B57NT4Help]
    1, b57nt4.hlp, SIZE=999


[Files-Other]
    1, b57dtect.dll, SIZE=65



;*******************************************************************************
; Description:
;    
; Input:
;    None.
;
; Output:
;    None.
;*******************************************************************************
[ShowShellErrorMessage]
    read-syms DebugControl
    debug-output "### ShowShellErrorMessage"

    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)

    set DlgType      = "MessageBox"
    set STF_MB_TITLE = $(MsgShellErrorTitle)
    set STF_MB_TEXT  = $(MsgShellErrorText)
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1

    ui start "Error Message"

    return



;*******************************************************************************
; Description:
;    
; Input:
;    $($0) = "WARNING", "FATAL", "NONFATAL", or "STATUS"
;    $($1) = Registery fatal text code.
;
; Output:
;    STATUS_FAILED
;    STATUS_SUCCESSFUL
;*******************************************************************************
[ShowRegistryErrorMessage]
    read-syms DebugControl
    debug-output "### ShowRegistryErrorMessage"

    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)

    set Severity = $($0)
    set RegStrCode = $($1)

    shell $(UtilityInf) RegistryErrorString $(RegStrCode)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        shell "" ShowShellErrorMessage
        return STATUS_FAILED
    endif

    set RegText = $($R0)

    shell $(SubroutineInf) SetupMessage $(!STF_LANGUAGE) $(Severity) $(RegText)

    return STATUS_SUCCESSFUL



;*******************************************************************************
; Description:
;    Displays shell error message.
;    
; Input:
;    $($0) = "WARNING", "FATAL", "NONFATAL", or "STATUS"
;    $($1) = Fatal text string.
;
; Output:
;    None.
;*******************************************************************************
[ShowErrorMessage]
    read-syms DebugControl
    debug-output "### ShowErrorMessage"

    read-syms FileConstants

    shell $(SubroutineInf) SetupMessage $(!STF_LANGUAGE) $($0) $($1)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        shell "" ShowShellErrorMessage
    endif

    return



;*******************************************************************************
; Description:
;    
; Input:
;
; Output:
;*******************************************************************************
[Install-Help]
    debug-output "### Install-Help"

    set STF_VITAL = ""
    set STF_OVERWRITE = "ALWAYS"

    AddSectionFilesToCopyList Files-$(OptionId)Help $(SrcDir) +
        $(!STF_WINDOWSSYSPATH)

    set !STF_OVERWRITE = TRUE
    set !STF_NCPA_FLUSH_COPYLIST = TRUE

    CopyFilesInCopyList

    exit



;*******************************************************************************
; Description:
;    
; Input:
;
; Output:
;*******************************************************************************
[Install-Update]
    debug-output "### Install-Update"

    set STF_VITAL     = ""
    set STF_OVERWRITE = "VERIFYSOURCEOLDER"

    AddSectionFilesToCopyList Files-$(OptionId)Driver $(SrcDir) +
        $(!STF_WINDOWSSYSPATH)\drivers
    AddSectionFilesToCopyList Files-$(OptionId)Help $(SrcDir) +
        $(!STF_WINDOWSSYSPATH)
    AddSectionFilesToCopyList Files-Other $(SrcDir) $(!STF_WINDOWSSYSPATH)

    set !STF_NCPA_FLUSH_COPYLIST = TRUE

    CopyFilesInCopyList

    exit



;*******************************************************************************
; Description:
;    
; Input:
;    None.
;
; Output:
;    None.
;*******************************************************************************
[Install-Option]
    debug-output "### Install-Option"

    ; Copy files.
    set STF_VITAL = ""
    ifstr(i) $(AddCopy) == "YES"
        debug-output "Add driver file to copy list."
        AddSectionFilesToCopyList Files-$(OptionId)Driver $(SrcDir) +
            $(!STF_WINDOWSSYSPATH)\drivers
    endif

    ifstr(i) $(DoCopy) == "YES"
        debug-output "copy files in copy list."
        set !STF_NCPA_FLUSH_COPYLIST = TRUE
        CopyFilesInCopyList
    endif

    exit



;*******************************************************************************
; Description:
;    
; Input:
;    None.
;
; Output:
;    $($R0): STATUS: STATUS_SUCCESSFUL
;    $($R1): Option Type (COMPUTER ...)
;    $($R2): Diskette description
;*******************************************************************************
[Identify]
    read-syms DebugControl
    debug-output "### Identify"

    read-syms Identification

    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media      = #("Source Media Descriptions", 1, 1)

    return $(Status) $(Identifier) $(Media)



;*******************************************************************************
; Description:
;
; Input:
;    $($0):  Language used.  (ENG|FRN|...)
;
; Output:
;    $($R0): STATUS: STATUS_SUCCESSFUL
;                    STATUS_NOLANGUAGE
;                    STATUS_FAILED
;                    STATUS_NOTSUPPORTED
;
;    $($R1): Option List
;    $($R2): Option Text List
;*******************************************************************************
[ReturnOptions]
    read-syms DebugControl
    debug-output "### ReturnOptions"

    set OptionList     = {}
    set OptionTextList = {}
    set LanguageList   = ^(LanguagesSupported, 1)

    ifcontains(i) $($0) in $(LanguageList)
        set Status         = STATUS_SUCCESSFUL
        set OptionList     = ^(Options, 1)
        set OptionTextList = ^(OptionsText$($0), 1)

        ifstr(i) $($1) != ""
            set PlatformList = ^(PlatformsSupported, 1)
            ifcontains(i) $($1) not-in $(PlatformList)
                debug-output "Unknown platform:  "$($1)
                set Status = STATUS_NOLANGUAGE
            endif
        endif
    else
        debug-output "Language not supported."
        set Status = STATUS_NOLANGUAGE
    endif

    return $(Status) $(OptionList) $(OptionTextList)



;*******************************************************************************
; Description:
;    This section performs the following tasks:
;       Copy files representing Options.
;       Configure the installed option.
;       Update the registry for the installed option
;
; Input:
;    $($0):  Language to use
;    $($1):  OptionID to install
;    $($2):  SourceDirectory
;    $($3):  AddCopy  (YES | NO)
;    $($4):  DoCopy   (YES | NO)
;    $($5):  DoConfig (YES | NO)
;
; Output:
;    $($R0): STATUS: STATUS_SUCCESSFUL |
;                    STATUS_NOLANGUAGE |
;                    STATUS_USERCANCEL |
;                    STATUS_FAILED
;*******************************************************************************
[InstallOption]
    read-syms DebugControl
    debug-output "### InstallOption"

    Set LanguageList = ^(LanguagesSupported, 1)
    ifcontains(i) $($0) not-in $(LanguageList)
        return STATUS_NOLANGUAGE
    endif

    set OptionId = $($1)
    set SrcDir = $($2)

    read-syms FileConstants$(!STF_LANGUAGE)
    read-syms FileConstants

    set-title $(Function$(OptionId)Title)

    ifstr(i) $(!NTN_InstallMode) == Deinstall
        shell "" RemoveSection $(OptionId)
    else-ifstr(i) $(!NTN_InstallMode) == Update
        shell "" UpdateSection $(OptionId) $(SrcDir)
    else-ifstr(i) $(!NTN_InstallMode) == Bind
        shell "" BindSection $(OptionId)
    else-ifstr(i) $(!NTN_InstallMode) == Configure
        shell "" ConfigureSection $(OptionId)
    else
        startwait
        shell "" InstallSection $($1) $($2) $($3) $($4) $($5)
        endwait

        ifstr(i) $($R0) != STATUS_SUCCESSFUL
            shell "" RemoveSection
            return STATUS_FAILED
        endif
    endif

    debug-output "Final status: "$($R0)

    return $($R0)



;*******************************************************************************
; Description:
;    
; Input:
;    $($0): OptionId
;
; Output:
;    $($R0) Status
;*******************************************************************************
[RemoveSection]
    read-syms DebugControl
    debug-output "### RemoveSection"

    set OptionId = $($0)

    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)

    ifstr(i) $(MiniportProductKeyName) == $(!NTN_RegBase)
        debug-output "Removing software component."
        shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(MiniportProductName)
    else
        debug-output "Removing hardware component."
        shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(MiniportProductName), $(!NTN_RegBase)
    endif

    return STATUS_SUCCESSFUL



;*******************************************************************************
; Description:
;    
; Input:
;    $($0):  OptionId
;    $($1):  SourceDirectory
;
; Output:
;    $($R0) Status
;*******************************************************************************
[UpdateSection]
    read-syms DebugControl
    debug-output "### UpdateSection"

    set OptionId = $($0)
    set SrcDir = $($1)

    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)

    openregkey $(!REG_H_LOCAL) "" $(MiniportProductKeyName) $(MAXIMUM_ALLOWED) +
        ProductKey
    ifstr $(ProductKey) == ""
        debug-output "Cannot get registry key."
        shell "" ShowErrorMessage "FATAL" $(MsgRegistryKeyDoesNotExist)
        return STATUS_FAILED
    endif

    getregvalue $(ProductKey), "MajorVersion", VersionInfo
    set MajorVersion = *($(VersionInfo), 4)
    debug-output "Major version: "$(MajorVersion)
    getregvalue $(ProductKey), "MinorVersion", VersionInfo
    set MinorVersion = *($(VersionInfo), 4)
    debug-output "Minor version: "$(MinorVersion)

    set-mul OldVersion = $(MajorVersion), 1000
    set-add OldVersion = $(OldVersion), $(MinorVersion)

    set-mul NewVersion = $(ProductMajorVersion), 1000
    set-add NewVersion = $(NewVersion), $(ProductMinorVersion)

    ifint $(OldVersion) > $(NewVersion)
        debug-output "Oldversion: "$(OldVersion)",   NewVersion: "$(NewVersion)
        shell "" ShowErrorMessage "FATAL" $(MsgDowngrade)
        return STATUS_USERCANCEL
    endif

    install "Install-Update"

    setregvalue $(ProductKey) { MajorVersion, $(NoTitle), $(!REG_VT_SZ), +
        $(ProductMajorVersion) }
    setregvalue $(ProductKey) { MinorVersion, $(NoTitle), $(!REG_VT_SZ), +
        $(ProductMinorVersion) }

    closeregkey $(ProductKey)

    ; Enumerate all netcards installed of this type and update them
    set iSearch = 1     ; start of search.

    nextnetcard = +
        shell $(UtilityInf), FindNextNetworkCard, $(MiniportProductName), +
            $(iSearch)
        set KeyNetcard = $($R0)
        set iSearch = $($R1)        ; next network card.

        ifstr $(KeyNetcard) != $(KeyNull)
            ; Get the service name so we can get the device location on the bus.
            getregvalue $(KeyNetcard), "ServiceName", ServiceNameInfo
            set ServiceName = *($(ServiceNameInfo), 4)
            debug-output "ServiceName: "$(ServiceName)

            ; get the bus, device, and function number before calling 
            ; "Install-ChangeDefaults".
            openregkey $(!REG_H_LOCAL) "" $(ServiceKeyName)"\"$(ServiceName)"\"+
                "Parameters" $(MAXIMUM_ALLOWED) ParameterKey

            getregvalue $(ParameterKey), "BusNumber", ValueInfo
            set BusNum = *($(ValueInfo), 4)
            getregvalue $(ParameterKey), "SlotNumber", ValueInfo
            set DeviceNum = *($(ValueInfo), 4)
            getregvalue $(ParameterKey), "FunctionNumber", ValueInfo
            set FunctionNum = *($(ValueInfo), 4)

            debug-output "bus: "$(BusNum)"   Dev: "$(DeviceNum)"   Funct: "+
                $(FunctionNum)


            install "Install-ChangeDefaults"

            ; Change the description.
            setregvalue $(KeyNetcard) { Description, $(NoTitle), +
                $(!REG_VT_SZ), $(Miniport$(OptionId)Description) }

            closeregkey $(KeyNetcard)

            ; Set BCMDID = 0x14e40000 + device ID
            set-hextodec BCMDID = $(DevID)
            debug-output "UpdateSection DevID: "$(DevID)" BCMDID: "$(BCMDID)
            set-add BCMDID = 350486528, $(BCMDID)
            debug-output "UpdateSection BCMDID: "$(BCMDID)

            setregvalue $(ParameterKey) { BCMDID, $(NoTitle), +
                $(!REG_VT_DWORD), $(BCMDID) }
            closeregkey $(ParameterKey)

            goto nextnetcard
        Endif
    
    ; shell "" ShowErrorMessage "NONFATAL" $(MsgUpdateDone)

    return STATUS_SUCCESSFUL



;*******************************************************************************
; Description:
;    
; Input:
;    $($0):  OptionId
;
; Output:
;    $($R0) Status
;*******************************************************************************
[BindSection]
    read-syms DebugControl
    debug-output "### BindSection"

    set OptionId = $($0)

    return STATUS_SUCCESSFUL



;*******************************************************************************
; Description:
;    
; Input:
;    None
;
; Output:
;    None
;*******************************************************************************
[Install-OTHER]
    set STF_VITAL = ""
    set STF_OVERWRITE = "ALWAYS"
    AddSectionFilesToCopyList Files-Other $(SrcDir) $(!STF_WINDOWSSYSPATH)
    set !STF_NCPA_FLUSH_COPYLIST = TRUE
    CopyFilesInCopyList
    Exit



;*******************************************************************************
; Description:
;    
; Input:
;    None
;
; Output:
;    None
;*******************************************************************************
[Install-ChangeDefaults]
    debug-output "### Install-ChangeDefaults"

    ; BusNum, DeviceNum, and FunctionNum must be initialized before calling
    ; this section.

    ; Load B57dtect dll so we can read PCI configuration registers mainly to
    ; get the PCI IDs.
    LoadLibrary $(MsgCannotFindB57dtectDll) $(!STF_WINDOWSSYSPATH)"\"+
        $(B57dtectDll) HwdtectDll

    ; Get device ID.
    LibraryProcedure DevID $(HwdtectDll) B57dtectPortIo "PciRd16" +
        $(BusNum) $(DeviceNum) $(FunctionNum) "0x02"
    debug-output "DevID: "$(DevID)

    ; Get subvendor ID.
    LibraryProcedure SVID $(HwdtectDll) B57dtectPortIo "PciRd16" +
        $(BusNum) $(DeviceNum) $(FunctionNum) "0x2c"
    debug-output "SVID: "$(SVID)

    ; Get the subsystem id.
    LibraryProcedure SSID $(HwdtectDll) B57dtectPortIo "PciRd16" +
        $(BusNum) $(DeviceNum) $(FunctionNum) "0x2e"
    debug-output "SSID: "$(SSID)

    FreeLibrary $(HwdtectDll)

    set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Ethernet"
    set MiniportB57NT4Description   = "Broadcom NetXtreme Gigabit Ethernet "+
        "NDIS 4.0 Driver Version "$(ProductVersion)"."

    ifstr(i) $(DevID) == "0x164d"
        set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Fast Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetXtreme Fast Ethernet "+
            "NDIS 4.0 Driver Version "$(ProductVersion)"."
    endif

    ifstr(i) $(DevID) == "0x169a"
        set MiniportB57NT4HardwareTitle = "Broadcom NetLink (TM) Gigabit Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetLink (TM) Gigabit Ethernet "+
            "NDIS 4.0 Driver Version "$(ProductVersion)"."
    endif

    ifstr(i) $(DevID) == "0x169c"
        set MiniportB57NT4HardwareTitle = "Broadcom NetLink (TM) Gigabit Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetLink (TM) Gigabit Ethernet "+
            "NDIS 4.0 Driver Version "$(ProductVersion)"."
    endif

    ifstr(i) $(DevID) == "0x169d"
        set MiniportB57NT4HardwareTitle = "Broadcom NetLink (TM) Gigabit Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetLink (TM) Gigabit Ethernet "+
            "NDIS 4.0 Driver Version "$(ProductVersion)"."
    endif

    ifstr(i) $(DevID) == "0x166e"
        set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Fast Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetXtreme Fast Ethernet "+
            "NDIS 4.0 Driver Version "$(ProductVersion)"."
    endif

    ifstr(i) $(DevID) == "0x1712"
        set MiniportB57NT4HardwareTitle = "Broadcom NetLink Fast Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetLink Fast Ethernet "+
            "NDIS 4.0 Driver Version "$(ProductVersion)"."
    endif

    ifstr(i) $(DevID) == "0x1713"
        set MiniportB57NT4HardwareTitle = "Broadcom NetLink Fast Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetLink Fast Ethernet "+
            "NDIS 4.0 Driver Version "$(ProductVersion)"."
    endif

    ifstr(i) $(DevID) == "0x1669"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Fiber"
            set MiniportB57NT4Description = "Broadcom NetXtreme Gigabit Fiber "+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
            set ConnectionList = { "Auto" }
            set ConnectionValueList = { 0 }
    endif

    ifstr(i) $(DevID) == "0x1679"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Fiber"
            set MiniportB57NT4Description = "Broadcom NetXtreme Gigabit Fiber "+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
            set ConnectionList = { "Auto" }
            set ConnectionValueList = { 0 }
    endif


    ; Change the title and description.
    ifstr(i) $(SVID) == "0x14e4"
        ifstr(i) $(SSID) == "0x16a8"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Fiber"
            set MiniportB57NT4Description = "Broadcom NetXtreme Gigabit Fiber "+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."

            set ConnectionList = { "Auto" }
            set ConnectionValueList = { 0 }
        endif

        ifstr(i) $(SSID) == "0x0002"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Fiber"
            set MiniportB57NT4Description = "Broadcom NetXtreme Gigabit Fiber "+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."

            set ConnectionList = { "Auto" }
            set ConnectionValueList = { 0 }
        endif

        ifstr(i) $(SSID) == "0x000a"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Fiber"
            set MiniportB57NT4Description = "Broadcom NetXtreme Gigabit Fiber "+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."

            set ConnectionList = { "Auto" }
            set ConnectionValueList = { 0 }
        endif

        ifstr(i) $(SSID) == "0x0003"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Fiber"
            set MiniportB57NT4Description = "Broadcom NetXtreme Gigabit Fiber "+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."

            set ConnectionList = { "Auto" }
            set ConnectionValueList = { 0 }
        endif

        ifstr(i) $(SSID) == "0x0007"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Gigabit Fiber"
            set MiniportB57NT4Description = "Broadcom NetXtreme Gigabit Fiber "+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."

            set ConnectionList = { "Auto" }
            set ConnectionValueList = { 0 }
        endif
    endif

    ; 3COM adapter description.
    ifstr(i) $(SVID) == "0x10b7"
        ifstr(i) $(SSID) == "0x1000"
            set MiniportB57NT4HardwareTitle = "3Com 3C996 10/100/1000 "+
                "Server NIC"
            set MiniportB57NT4Description = "3Com 3C996 10/100/1000 "+
                "Server NIC."
        endif

        ifstr(i) $(SSID) == "0x1004"
            set MiniportB57NT4HardwareTitle = "3Com 3C996 Gigabit Fiber-SX "+
                "Server NIC"
            set MiniportB57NT4Description = "3Com 3C996 Gigabit Fiber-SX "+
                "Server NIC."

            set ConnectionList = { "Auto" }
            set ConnectionValueList = { 0 }
        endif

        ifstr(i) $(SSID) == "0x1006"
            set MiniportB57NT4HardwareTitle = "3Com 3C996B Gigabit "+
                "Server NIC"
            set MiniportB57NT4Description = "3Com 3C996B Gigabit "+
                "Server NIC."
        endif

        ifstr(i) $(SSID) == "0x1007"
            set MiniportB57NT4HardwareTitle = "3Com 3C1000 Gigabit NIC"
            set MiniportB57NT4Description = "3Com 3C1000 Gigabit NIC."
        endif

        ifstr(i) $(SSID) == "0x1008"
            set MiniportB57NT4HardwareTitle = "3Com 3C940 Gigabit LOM "
            set MiniportB57NT4Description = "3Com 3C940 Gigabit LOM "
        endif

        ifstr(i) $(SSID) == "0x1100"
            set MiniportB57NT4HardwareTitle = "3Com 10/100/1000 PCI "
            set MiniportB57NT4Description = "3Com 10/100/1000 PCI "
        endif

        ifstr(i) $(SSID) == "0x2000"
            set MiniportB57NT4HardwareTitle = "3Com Dual Port 10/100/1000 PCI-X Server Nic"
            set MiniportB57NT4Description = "3Com Dual Port 10/100/1000 PCI-X Server Nic."
        endif

        ifstr(i) $(SSID) == "0x2001"
            set MiniportB57NT4HardwareTitle = "3Com Dual Port 1000-SX PCI-X Server Nic"
            set MiniportB57NT4Description = "3Com Dual Port 1000-SX PCI-X Server Nic."
        endif

        ifstr(i) $(SSID) == "0x3000"
            set MiniportB57NT4HardwareTitle = "3Com Quad Port 10/100/1000 PCI-X Server Nic"
            set MiniportB57NT4Description = "3Com Quad Port 10/100/1000 PCI-X Server Nic."
        endif
    endif





    ifstr(i) $(SVID) == "0x1028"
        ; rename devices for dell
        ifstr(i) $(SSID) == "0x0175"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Gigabit Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Gigabit Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x0176"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Gigabit Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Gigabit Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x0177"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Gigabit Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Gigabit Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x0178"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Gigabit Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Gigabit Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x0179"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Gigabit Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Gigabit Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x0182"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Gigabit Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Gigabit Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x0186"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Gigabit Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Gigabit Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x0187"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Fast Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Fast Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x0188"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Fast Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Fast Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
        ifstr(i) $(SSID) == "0x018f"
            set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme 57xx Fast Controller"
            set MiniportB57NT4Description   = "Broadcom NetXtreme 57xx Fast Controller"+
                "NDIS 4.0 Driver Version "$(ProductVersion)"."
        endif
    endif



    ; Dell
    ifstr(i) $(SVID) == "0x1028"
        ; Driver Information Entries
        ; These items will be set by IHV...
        Set DriverMfgr = "Broadcom"                   ; IHV name
        Set DriverVersionID = "4.00"                  ; The IHV driver package version
        Set BaseDriverFileVersion = $(ProductVersion) ; Version in Key file
        Set BaseDriverFileName = "b57nt4.sys"         ; Key file for version check

        ; These items will be set to VENDOR values, and then set to OEM-specific by OEM
        Set DriverOEM = "Dell"                                          ; name of the OEM
        Set DriverFamily = "NIC"                                        ; device family (NIC, Storage, Video...)
        Set DriverProduct = "BCM5700"                                   ; Specific Name of device (chipset, for example)
        Set DriverDescription = "Broadcom NetXtreme Gigabit Ethernet"  ; Description of device (product name, OS or system supported)
        Set DriverOEMVersion = "A00"                                    ; OEM-specified version

        ; This section is added to all INFs to add registry entries for Driver Info.
        set DriverInfoRegList = { "InstalledOptions",$(DriverOEM),$(DriverFamily),$(DriverMfgr),$(DriverProduct) }
        set DriverInfoKey = "SOFTWARE"
        OpenRegKey $(!REG_H_LOCAL) "" $(DriverInfoKey) $(!REG_KEY_CREATE_SUB_KEY) DriverInfoOldKeyHandle
        ifstr $(DriverInfoOldKeyHandle) == ""
            shell "subroutn.inf" SetupMessage $(!STF_LANGUAGE) "NONFATAL" "DriverInfo registry failed. Could not open HKLM\Software ("$(RegLastError)")"
            set DriverInfoFailed = "FAIL"
        else
            ForListDo $(DriverInfoRegList)
                Set NewDriverInfoKey = $(DriverInfoKey)"\"$($)
                OpenRegKey $(!REG_H_LOCAL) "" $(NewDriverInfoKey) $(!REG_KEY_ALL_ACCESS) DriverInfoKeyHandle
                ifstr(i) $(DriverInfoKeyHandle) == ""
                    CreateRegKey $(DriverInfoOldKeyHandle) {$($),0,GenericClass} "" $(!REG_KEY_ALL_ACCESS) "" DriverInfoKeyHandle
                    ifstr $(DriverInfoKeyHandle) == ""
                        shell "subroutn.inf" SetupMessage $(!STF_LANGUAGE) "NONFATAL" "DriverInfo registry failed. Could not create key:"$($)" ("$(RegLastError)")"
                        set DriverInfoFailed = "FAIL"
                    endif
                endif
                CloseRegKey $(DriverInfoOldKeyHandle)
                set DriverInfoOldKeyHandle = $(DriverInfoKeyHandle)
                set DriverInfoKey = $(NewDriverInfoKey)
            EndForListDo
        endif

        ifstr $(DriverInfoFailed) != "FAIL"
            SetRegValue $(DriverInfoKeyHandle) {"Description",0,$(!REG_VT_SZ),$(DriverDescription)}
            SetRegValue $(DriverInfoKeyHandle) {"CurrentVer",0,$(!REG_VT_SZ),$(DriverOEMVersion)}
            SetRegValue $(DriverInfoKeyHandle) {"Ver_"$(DriverOEMVersion),0,$(!REG_VT_SZ),$(DriverVersionID)}
            SetRegValue $(DriverInfoKeyHandle) {"BaseDriverFileName",0,$(!REG_VT_SZ),$( BaseDriverFileName)}
            SetRegValue $(DriverInfoKeyHandle) {"BaseDriverFileVersion",0,$(!REG_VT_SZ),$(BaseDriverFileVersion)}

            CloseRegKey $(DriverInfoKeyHandle)
        endif

        ifstr(i) $(SSID) == "0x8126"
            set MiniportB57NT4HardwareTitle = "Broadcom 570x Gigabit Integrated Controller"
            set MiniportB57NT4Description = "Broadcom 570x Gigabit Integrated Controller"
        endif
    endif

    ; Compaq adapter description.
    ifstr(i) $(SVID) == "0x0e11"
        ifstr(i) $(SSID) == "0x007c"
            set MiniportB57NT4HardwareTitle = "BCM5701 Gigabit Ethernet"
            set MiniportB57NT4Description = "BCM5701 Gigabit Ethernet."
        endif

        ifstr(i) $(SSID) == "0x00c1"
            set MiniportB57NT4HardwareTitle = "BCM5701 Gigabit Ethernet"
            set MiniportB57NT4Description = "BCM5701 Gigabit Ethernet."
        endif

        ifstr(i) $(SSID) == "0x0085"
            set MiniportB57NT4HardwareTitle = "BCM5701 Gigabit Ethernet"
            set MiniportB57NT4Description = "BCM5701 Gigabit Ethernet."
        endif

        ifstr(i) $(SSID) == "0x00bb"
            set MiniportB57NT4HardwareTitle = "BCM5702 Gigabit Ethernet"
            set MiniportB57NT4Description = "BCM5702 Gigabit Ethernet."
        endif

        ifstr(i) $(SSID) == "0x00ca"
            set MiniportB57NT4HardwareTitle = "BCM5703 Gigabit Ethernet"
            set MiniportB57NT4Description = "BCM5703 Gigabit Ethernet."
        endif

        ifstr(i) $(SSID) == "0x00cb"
            set MiniportB57NT4HardwareTitle = "BCM5703 Gigabit Ethernet"
            set MiniportB57NT4Description = "BCM5703 Gigabit Ethernet."
        endif
    endif


    ifstr(i) $(DevID) == "0x170d"
        set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Fast Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetXtreme Fast Ethernet NDIS 4.0 Driver."
    endif

    ifstr(i) $(DevID) == "0x170e"
        set MiniportB57NT4HardwareTitle = "Broadcom NetXtreme Fast Ethernet"
        set MiniportB57NT4Description   = "Broadcom NetXtreme Fast Ethernet NDIS 4.0 Driver."
    endif


    Exit



;*******************************************************************************
; Description:
;    
; Input:
;    $($0):  OptionId
;
; Output:
;    $($R0)  STATUS_FAILED or STATUS_SUCCESSFUL
;*******************************************************************************
[ConfigureSection]
    read-syms DebugControl
    debug-output "### ConfigureSection"

    set OptionId = $($0)

    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)

    openregkey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) ProductKey
    ifstr $(ProductKey) == ""
        debug-output "Component not installed."
        shell "" ShowRegistryErrorMessage "FATAL" CANNOT_FIND_COMPONENT_SERVICE
        return STATUS_FAILED
    Endif

    shell $(UtilityInf) FindService $(ProductKey)
    ifstr(i) $($R0) != NO_ERROR
        debug-output "Canot not find the component."
        closeregkey $(ProductKey)
        shell "" ShowRegistryErrorMessage "FATAL" $($R0)
        return STATUS_FAILED
    endif

    closeregkey $($R1)
    closeregkey $(ProductKey)

    set ParameterKey = $($R2)

    ifstr $(ParameterKey) == ""
        shell "" ShowRegistryErrorMessage "FATAL" CANNOT_FIND_COMPONENT_SERVICE
        return STATUS_FAILED
    endif

    EnumRegValue $(ParameterKey) ValueList

    set ConnectionIndex = 0
    set FlowControlCapIndex = 0
    set RxMtuIndex = 1500
    ForListDo $(ValueList)
        set ValueItem = $($)
        set ValueName = *($(ValueItem), 1)
        set ValueData = *($(ValueItem), 4)
        ifstr(i) $(ValueName) == "RequestedMediaType"
            set ConnectionIndex = $(ValueData)
        endif

        ifstr(i) $(ValueName) == "FlowControlCap"
            set FlowControlCapIndex = $(ValueData)
        endif

        ifstr(i) $(ValueName) == "RxMtu"
            set RxMtuIndex = $(ValueData)
        endif

        ifstr(i) $(ValueName) == "BusNumber"
            set BusNum = $(ValueData)
        endif

        ifstr(i) $(ValueName) == "SlotNumber"
            set DeviceNum = $(ValueData)
        endif

        ifstr(i) $(ValueName) == "FunctionNumber"
            set FunctionNum = $(ValueData)
        endif
    EndForListDo

    set OldConnectionValue = $(ConnectionIndex)
    set OldFlowControlCapValue = $(FlowControlCapIndex)
    set OldRxMtuValue = $(RxMtuIndex)

    set ConnectionList = ^(RequestedMediaType$(OptionId), 1)
    set ConnectionValueList = ^(RequestedMediaType$(OptionId), 2)
    debug-output "ConnectionList: "$(ConnectionList)
    debug-output "ConnectionValueList: "$(ConnectionValueList)

    set FlowControlCapList = ^(FlowControlCap$(OptionId), 1)
    set FlowControlCapValueList = ^(FlowControlCap$(OptionId), 2)
    debug-output "FlowControlCapList: "$(FlowControlCapList)
    debug-output "FlowControlCapValueList: "$(FlowControlCapValueList)

    set RxMtuList = ^(RxMtu$(OptionId), 1)
    set RxMtuValueList = ^(RxMtu$(OptionId), 2)
    debug-output "RxMtuList: "$(RxMtuList)
    debug-output "RxMtuValueList: "$(RxMtuValueList)

    ; Get the bus, device, and function number are initialized above.
    install "Install-ChangeDefaults"
    debug-output "New connection list: "$(ConnectionList)
    debug-output "New connection value list: "$(ConnectionValueList)

    set ConnectionValue = *($(ConnectionList), ~($(ConnectionValueList), +
        $(ConnectionIndex)))
    ifstr(i) $(ConnectionValue) == ""
        set ConnectionValue = *($(ConnectionList), 1)
    endif

    set FlowControlCapValue = *($(FlowControlCapList), ~($(FlowControlCapValueList), +
        $(FlowControlCapIndex)))
    ifstr(i) $(FlowControlCapValue) == ""
        set FlowControlCapValue = *($(FlowControlCapList), 1)
    endif

    set RxMtuValue = *($(RxMtuList), ~($(RxMtuValueList), $(RxMtuIndex)))
    ifstr(i) $(RxMtuValue) == ""
        set RxMtuValue = *($(RxMtuList), 1)
    endif

    read-syms DialogConstants$(!STF_LANGUAGE)

    ifstr(i) $(DevID) == "0x1653"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1654"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x165d"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x166e"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1696"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x169c"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x169d"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x170d"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x170e"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1658"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1659"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1676"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1677"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x167c"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x167d"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x16f7"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x16fd"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x16dd"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1600"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1601"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x167b"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1674"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1673"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x167a"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1672"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1693"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x167f"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x169b"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x169a"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1712"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else-ifstr(i) $(DevID) == "0x1713"
        read-syms RequestedMediaTypeADlg$(!STF_LANGUAGE)
    else
        read-syms RequestedMediaTypeDlg$(!STF_LANGUAGE)
    endif

    debug-output "HelpContext = "$(HelpContext)
    sethelpfile $(!STF_WINDOWSSYSPATH)"\"$($(OptionId)HelpFile) +
        $(MinHelpId) $(MaxHelpId) $($(OptionId)HelpId)

    set ConnectionIndex = *($(ConnectionList), 1)
    set FlowControlCapIndex = *($(FlowControlCapList), 1)
    set RxMtuIndex = *($(RxMtuList), 1)

    set RetStatus = STATUS_SUCCESSFUL

    ui start "Config"
    ifstr(i) $(DLGEVENT) == "CONTINUE"
        set ConnectionIndex = $(Combo1Out)
        set FlowControlCapIndex = $(Combo2Out)
        set RxMtuIndex = $(Combo3Out)
    else-ifstr(i) $(DLGEVENT) == "BACK"
        set RetStatus = STATUS_USERCANCEL
    endif
    ui pop 1

    set NewConnectionValue = *($(ConnectionValueList), +
        ~($(ConnectionList), $(ConnectionIndex)))
    set NewFlowControlCapValue = *($(FlowControlCapValueList), +
        ~($(FlowControlCapList), $(FlowControlCapIndex)))

    ifstr(i) $(DevID) == "0x1653"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x1654"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x165d"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x166e"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x1696"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x169d"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x169c"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x170d"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x1712"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x1713"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x1674"
        set NewRxMtuValue = 1500
    else-ifstr(i) $(DevID) == "0x170e"
        set NewRxMtuValue = 1500
    else
        set NewRxMtuValue = *($(RxMtuValueList), +
            ~($(RxMtuList), $(RxMtuIndex)))
    endif

    debug-output "New Connection value = "$(NewConnectionValue)
    debug-output "Old Connection value = "$(OldConnectionValue)
    debug-output "New FlowControlCap value = "$(NewFlowControlCapValue)
    debug-output "Old FlowControlCap value = "$(OldFlowControlCapValue)
    debug-output "New RxMtu value = "$(NewRxMtuValue)
    debug-output "Old RxMtu value = "$(OldRxMtuValue)

    ifstr(i) $(NewConnectionValue) == $(OldConnectionValue)
        ifstr(i) $(NewFlowControlCapValue) == $(OldFlowControlCapValue)
            ifstr(i) $(NewRxMtuValue) == $(OldRxMtuValue)
                set RetStatus = STATUS_USERCANCEL
            endif
        endif
    endif

    ifstr(i) $(RetStatus) == "STATUS_SUCCESSFUL"
        set NewValueList = {                                        +
            { RequestedMediaType, $(NoTitle), $(!REG_VT_DWORD),     +
                $(NewConnectionValue)},                             +
            { FlowControlCap, $(NoTitle), $(!REG_VT_DWORD),         +
                $(NewFlowControlCapValue)},                         +
            { RxMtu, $(NoTitle), $(!REG_VT_DWORD),                  +
                $(NewRxMtuValue)} }
        shell $(UtilityInf), AddValueList, $(ParameterKey), $(NewValueList)
    endif

    closeregkey $(ParameterKey)

    return $(RetStatus)



;*******************************************************************************
; Description:
;    
; Input:
;    $($0): PciIdList
;
; Output:
;    $($R0) Adapter list.
;*******************************************************************************
[BuildAdapterList]
    read-syms DebugControl
    read-syms FileConstants

    debug-output "### BuildAdapterList"

    set PciIdList = $($0)
    debug-output "PciIdList: "$(PciIdList)

    ; Load B57dtect dll so we can get the PCI sub vendor id.
    LoadLibrary $(MsgCannotFindB57dtectDll) $(!STF_WINDOWSSYSPATH)"\"+
        $(B57dtectDll) HwdtectDll

    set AllAdapterList = {}

    forlistdo $(PciIdList)
        set VID = *($($), 1)
        set DID = *($($), 2)
        debug-output "VID: "$(VID)"  DID: "$(DID)

        shell $(UtilityInf), GetPCIInformation, $(VID) $(DID)
        ifint $($ShellCode) == $(!SHELL_CODE_OK)
            set AdapterList = $($R0)
            debug-output "AdapterList: "$(AdapterList)

            forlistdo $(AdapterList)
                set Adapter = $($)
                set BusNum = *($(Adapter), 1)
                set DeviceNum = *($(Adapter), 2)
                set FunctionNum = *($(Adapter), 3)
                ifint $(FunctionNum) == 1
                    ; GHL It just so happens that the second function is at
                    ; device + 32 to make nt4 happy
                    set-add DeviceNum = $(DeviceNum),32
                    set Adapter = { $(BusNum), $(DeviceNum), $(FunctionNum) }
                endif
                ; Get subvendor ID.
                LibraryProcedure SVID $(HwdtectDll) B57dtectPortIo "PciRd16" +
                    $(BusNum) $(DeviceNum) $(FunctionNum) "0x2c"
                debug-output "SVID: "$(SVID)

                ; Get the subsystem id.
                LibraryProcedure SSID $(HwdtectDll) B57dtectPortIo "PciRd16" +
                    $(BusNum) $(DeviceNum) $(FunctionNum) "0x2e"
                debug-output "SSID: "$(SSID)

                set AllAdapterList = >($(AllAdapterList), $(Adapter))
            endforlistdo
        endif
    endforlistdo

    FreeLibrary $(HwdtectDll)

    debug-output "AllAdapterList: "$(AllAdapterList)

    return $(AllAdapterList)



;*******************************************************************************
; Description:
;    
; Input:
;    None.
;
; Output:
;    $($R0)  STATUS_FAILED or STATUS_SUCCESSFUL
;*******************************************************************************
[CheckServicePack]
    read-syms DebugControl
    debug-output "### CheckServicePack"

    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)

    ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
        return STATUS_SUCCESSFUL
    endif

    ; Load B57dtect.dll so we can get the service pack info.
    LoadLibrary $(MsgCannotFindB57dtectDll) $(!STF_WINDOWSSYSPATH)"\"+
        $(B57dtectDll) HwdtectDll

    LibraryProcedure OsVersionInfo $(HwdtectDll) B57GetOsVersion
    debug-output "OsVersionInfo: "$(OsVersionInfo)

    FreeLibrary $(HwdtectDll)

    split-string $(OsVersionInfo) "," OsVersionInfoList
    debug-output "OsVersionInfoList: "$(OsVersionInfoList)

    set ServicePack = *($(OsVersionInfoList), 9)
    debug-output "Service Pack: "$(ServicePack)

    set UnsupportedServicePacks = { "Service Pack 0", "Service Pack 1", +
        "Service Pack 2", "Service Pack 3" }

    ifcontains(i) $(ServicePack) in $(UnsupportedServicePacks)
        set DlgType = "MessageBox"
        set STF_MB_TITLE = $(MessageBoxTitle)
        set STF_MB_TEXT  = $(MsgUntestedServicePack)
        set STF_MB_TYPE  = 3    ; YES or NO buttons.
        set STF_MB_ICON  = 2    ; Info icon.
        set STF_MB_DEF   = 1    ; Default button YES.

        ui start "Message"

        ifstr(i) $(DLGEVENT) == "YES"
            debug-output "Continue with installation."
            set RetStatus = STATUS_SUCCESSFUL
        else
            debug-output "Quit installation."
            set RetStatus = STATUS_FAILED
        endif
    else
        debug-output "Supported service pack."
        set RetStatus = STATUS_SUCCESSFUL
    endif

    return $(RetStatus)



;*******************************************************************************
; Description:
;    Determine if the driver has been installed for a network card get the
;    give bus and slot number.
;    
; Input:
;    $($0): Bus number.
;    $($1): Slot number.
;
; Output:
;    $($R0): STATUS_FAILED or STATUS_SUCCESSFUL.
;    $($R1): "NO" or "YES"
;*******************************************************************************
[IsDriverAlreadyInstalled]
    read-syms DebugControl
    debug-output "### IsDriverAlreadyInstalled"

    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)

    set BusNum  = $($0)
    set SlotNum = $($1)
    set FunctionNum = $($2)

    ; Open the NetworkCards registry hive.
    OpenRegKey $(!REG_H_LOCAL) "" $(NetworkCardKeyName) $(MAXIMUM_ALLOWED) +
        IE_KeyNetcards
    Ifstr $(IE_KeyNetcards) == ""
        debug-output "Unable to open registry key: "$(NetworkCardKeyName)
        shell "" ShowRegistryErrorMessage "FATAL" +
            UNABLE_OPEN_NETWORKCARD_SECTION
        return STATUS_FAILED
    endif

    ; Get a list of installed network cards.
    EnumRegKey $(IE_KeyNetcards) IE_KeyNameList

    ; Compare the product name, bus number, and slot number.  If all the
    ; the comparisions matched, then the driver was installed for this adapter.
    ForListDo  $(IE_KeyNameList)
        set IE_KeyName = *($($),1)

        ; Open the key that contains the driver information.
        OpenRegKey $(IE_KeyNetcards) "" $(IE_KeyName) $(MAXIMUM_ALLOWED) IE_Card
        Ifstr $(IE_Card) == ""
            debug-output "Unable to open the adapter instance key."
            shell "" ShowRegistryErrorMessage "FATAL" +
                UNABLE_OPEN_NETWORKCARD_SECTION
            return STATUS_FAILED
        endif

        ; Get the product name.
        GetRegValue $(IE_Card), "ProductName", ProductNameInfo

        set CardProductName = *($(ProductNameInfo), 4)
        debug-output "Found product name: "$(CardProductName)

        ifcontains(i) $(CardProductName) in { B57NT4, Q57NT4 }
            ; Get the service name so we can get the bus and slot number later.
            GetRegValue $(IE_Card), "ServiceName", ServiceNameInfo
            set ServiceName = *($(ServiceNameInfo), 4)
            debug-output "Found service name: "$(ServiceName)

            ; Open the driver parameter key to get the bus and slot number.
            OpenRegKey $(!REG_H_LOCAL) "" $(ServiceKeyName)"\"$(ServiceName)+
                "\Parameters" $(MAXIMUM_ALLOWED) IE_KeyService
            Ifstr $(IE_KeyService) == ""
                debug-output "Unable to open service key."
                shell "" ShowRegistryErrorMessage "FATAL" +
                    UNABLE_OPEN_NETWORKCARD_SECTION
                return STATUS_FAILED
            endif

            GetRegValue $(IE_KeyService), "BusNumber", BusInfo
            GetRegValue $(IE_KeyService), "SlotNumber", SlotInfo
            GetRegValue $(IE_KeyService), "FunctionNumber", FunctionInfo

            set CardBusNum = *($(BusInfo), 4)
            set CardSlotNum = *($(SlotInfo), 4)
            set CardFunctionNum = *($(FunctionInfo), 4)

            ifint $(CardBusNum) == $(BusNum)
                ifint $(CardSlotNum) == $(SlotNum)
                    ifint $(CardFunctionNum) == $(FunctionNum)
                        debug-output "Adapter already installed"
                        return STATUS_SUCCESSFUL "YES"
                    endif
                endif
            endif
        endif
    EndForListDo

    debug-output "Adapter not previously installed"

    return STATUS_SUCCESSFUL "NO"



;*******************************************************************************
; Description:
;    
; Input:
;    $($0):  OptionId
;    $($1):  SourceDirectory
;    $($2):  AddCopy  (YES | NO)
;    $($3):  DoCopy   (YES | NO)
;    $($4):  DoConfig (YES | NO)
;
; Output:
;    $($R0)  STATUS_FAILED or STATUS_SUCCESSFUL
;*******************************************************************************
[InstallSection]
    read-syms DebugControl
    debug-output "### InstallSection"

    set OptionId = $($0)
    set SrcDir   = $($1)
    set AddCopy  = $($2)
    set DoCopy   = $($3)
    set DoConfig = $($4)

    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)

    detect CurrentDate

    ; Get installation source directory.
    ifstr(i) $(DoCopy) == "YES"
        debug-output "DoCopy"

        shell $(UtilityInf) DoAskSource $(!STF_CWDDIR) $(SrcDir) YES
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            shell "" ShowShellErrorMessage
            return STATUS_FAILED
        else-ifstr(i) $($R0) == STATUS_FAILED
            shell "" ShowRegistryErrorMessage "FATAL" ASK_SOURCE_FAIL
            return STATUS_FAILED
        else-ifstr(i) $($R0) == STATUS_USERCANCEL
            debug-output "User cancelled."
            return STATUS_USERCANCEL
        endif

        set SrcDir = $($R1)
    endif

    install "Install-Help"
    install "Install-OTHER"
    install "Install-Option"

    ; First time installation -- we need to install the software component.
    openregkey $(!REG_H_LOCAL) "" $(MiniportProductKeyName) $(MAXIMUM_ALLOWED) +
        ProductKey
    ifstr $(ProductKey) == ""
        debug-output "First time installation"

        ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
            debug-output "Copy file failed."
            shell "" ShowRegistryErrorMessage "FATAL" UNABLE_COPY_FILE
            return STATUS_FAILED
        endif

        debug-output "Create the software component."

        shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
            $(MiniportProductName), $(MiniportProductName), +
            $(MiniportProductSoftwareDisplayName), $(STF_CONTEXTINFNAME), +
            $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "", +
            $(NetEventDll)
        ifstr(i) $($R0) != NO_ERROR
            debug-output "Add miniport software component failed."

            closeregkey $($R1)
            closeregkey $($R2)
            closeregkey $($R3)
            closeregkey $($R4)
            closeregkey $($R5)

            shell "" ShowRegistryErrorMessage "FATAL" $($R0)
            return STATUS_FAILED
        endif

        ; $R1 contains handle to "SOFTWARE\[Manufacturer]\CurrentVersion".
        ; $R2 contains handle to "SOFTWARE\[Manufacturer]\CurrentVersion\NetRules".
        ; $R3 contains handle to "SYSTEM\CurrentControlSet\[Service]".
        ; $R4 contains handle to "SYSTEM\CurrentControlSet\[Service]\Parameters".
        ; $R5 contains handle to "SYSTEM\CurrentControlSet\[Service]\Linkage".

        set ProductKey   = $($R1)
        set NetRuleKey   = $($R2)
        set ServiceKey   = $($R3)
        set ParameterKey = $($R4)
        set LinkageKey   = $($R5)

        set NewValueList = {                                +
            { SoftwareType, $(NoTitle), $(!REG_VT_SZ),      +
                $(MiniportSoftwareType) },                  +
            { MajorVersion, $(NoTitle), $(!REG_VT_DWORD),   +
                $(ProductMajorVersion) },                   +
            { MinorVersion, $(NoTitle), $(!REG_VT_DWORD),   +
                $(ProductMinorVersion) },                   +
            { Title,        $(NoTitle), $(!REG_VT_SZ),      +
                $(MiniportProductSoftwareTitle) },          +
            { Description,  $(NoTitle), $(!REG_VT_SZ),      +
                $(MiniportProductDescription) },            +
            { ServiceName,  $(NoTitle), $(!REG_VT_SZ),      +
                $(MiniportProductName) },                   +
            { InstallDate,  $(NoTitle), $(!REG_VT_DWORD),   +
                *($(Now),1) } }

        shell $(UtilityInf), AddValueList, $(ProductKey), $(NewValueList)
        ifstr(i) $($R0) != NO_ERROR
            debug-output "Cannot create miniport software key."

            closeregkey $(ProductKey)
            closeregkey $(NetRuleKey)
            closeregkey $(ServiceKey)
            closeregkey $(ParameterKey)
            closeregkey $(LinkageKey)

            shell "" ShowRegistryErrorMessage "FATAL" $($R0)
            return STATUS_FAILED
        endif

        set NewValueList = {                                                +
            { type,         $(NoTitle), $(!REG_VT_SZ),                      +
                $(MiniportNetRuleSoftwareType) },                           +
            { use,          $(NoTitle), $(!REG_VT_SZ),                      +
                $(MiniportNetRuleSoftwareUse) },                            +
            { bindform,     $(NoTitle), $(!REG_VT_SZ),                      +
                $(MiniportNetRuleSoftwareBindForm) },                       +
            { class,        $(NoTitle), $(!REG_VT_MULTI_SZ),                +
                $(MiniportNetRuleSoftwareClass) },                          +
            { bindable,     $(NoTitle), $(!REG_VT_MULTI_SZ),                +
                $(MiniportNetRuleSoftwareBindable) },                       +
            { InfOption,    $(NoTitle), $(!REG_VT_SZ), $(OptionId) } }

        shell $(UtilityInf), AddValueList, $(NetRuleKey), $(NewValueList)
        ifstr(i) $($R0) != NO_ERROR
            debug-output "### Cannot create the miniport netrules."

            closeregkey $(ProductKey)
            closeregkey $(NetRuleKey)
            closeregkey $(ServiceKey)
            closeregkey $(ParameterKey)
            closeregkey $(LinkageKey)

            shell "" ShowRegistryErrorMessage "FATAL" $($R0)
            return STATUS_FAILED
        endif

        closeregkey $(NetRuleKey)
        closeregkey $(ServiceKey)
        closeregkey $(ParameterKey)
        closeregkey $(LinkageKey)
    endif
    closeregkey $(ProductKey)

    ; Check OS version. - Disabled for now.
    ;shell "" CheckServicePack
    ;ifstr(i) $($R0) != STATUS_SUCCESSFUL
    ;    return STATUS_USERCANCEL
    ;endif

    ; Get the adapter list.
    set PciIdList = { { 5348, 5700 }, { 5348, 5701 }, { 5348, 5702 }, { 5348, 5798 }, { 5348, 5709 }, { 5348, 5703 }, { 5348, 5799 }, { 5348, 5704 } , { 5348, 5725 } , { 5348, 5715 } , { 5348, 5901 } , { 5348, 5902 }, { 5348, 5830 } , { 5348, 5831} , { 5348, 5782 } , { 5348, 5800} , { 5348, 5788 } , { 5348, 5789 } , { 5348, 5742 } , { 5348, 5716}  , { 5348, 5750 } , { 5348 , 5756 } , { 5348 , 5751 } , { 5348 , 5757 } , { 5348 , 5758 } , { 5348 , 5720 } , { 5348 , 5721 } , { 5348 , 5726 } , { 5348 ,  5789 }, { 5348 , 5879 }, { 5348 , 5885 } ,  { 5348 , 5853 }, { 5348 , 5632 }, { 5348 , 5633 } , { 5348 , 5636 } , { 5348 , 5637 } , { 5348 , 5638 } , { 5348 , 5639 }  , { 5348 , 5376 }  , { 5348 , 5677 }  , { 5348 , 5752 }  , { 5348 , 5753 } , { 5348 , 5736 } , { 5348 , 5737 } , { 5348 , 5887 } , {5348 , 5754} , {5348 , 5746} , {5348 , 5755} , {5348 , 5747} , {5348 , 5786}, {5348 , 5787} , {5348 , 5779} , {5348 , 5759} , {5348 , 5746}  , {5348 , 5747}  , {5348 , 5906} , {5348 , 5907}}  
    shell "" BuildAdapterList $(PciIdList)
    set AdapterList = $($R0)

    ifstr(i) $(AdapterList) == {}
        shell "" ShowErrorMessage "NONFATAL" $(MsgNoAdapterFound)
        return STATUS_FAILED
    endif

    ; Load B57dtect dll so we can get the PCI sub vendor id.
    LoadLibrary $(MsgCannotFindB57dtectDll) $(!STF_WINDOWSSYSPATH)"\"+
        $(B57dtectDll) HwdtectDll

    ; HotPlug PCI port number.  This number is only valid for 5701 device
    ; with 0x0e110085 subsystem id.
    set HppPortNum = 0

    debug-output "======== Install adapters: "$(AdapterList)
    forlistdo $(AdapterList)
        debug-output "***** Installing adapter "$($)"."
        set BusNum = *($($), 1)
        set DeviceNum = *($($), 2)
        set FunctionNum = *($($), 3)

        ; Change the default parameters according to the subsystem id.
        install "Install-ChangeDefaults"

        shell "" IsDriverAlreadyInstalled $(BusNum) $(DeviceNum) $(FunctionNum)
        ifstr $($R0) != STATUS_SUCCESSFUL
            return STATUS_FAILED
        endif

        ifstr(i) $($R1) != "YES"
            debug-output "add hardware component."

            shell $(UtilityInf), AddHardwareComponent, $(MiniportProductName), +
                $(STF_CONTEXTINFNAME), $(MiniportProductKeyName)
            ifstr(i) $($R0) != NO_ERROR
                debug-output "### Add hardware component error."

                closeregkey $($R1)
                closeregkey $($R2)
                closeregkey $($R3)

                shell "" ShowRegistryErrorMessage "FATAL" $($R0)
                return STATUS_FAILED
            endif

            set HardNetCardKey   = $($R1)
            set HardNetRuleKey   = $($R2)
            set HardParameterKey = $($R3)

            set AdapterNumber    = $($R4)

            set NewValueList = { +
                { Manufacturer, $(NoTitle), $(!REG_VT_SZ), $(Manufacturer) }, +
                { Title, $(NoTitle), $(!REG_VT_SZ), +
                    "["$($R4)"] "$(Miniport$(OptionId)HardwareTitle)" "+
                    "(Bus "$(BusNum)", Slot "$(DeviceNum)")." }, +
                { Description, $(NoTitle), $(!REG_VT_SZ), +
                    $(Miniport$(OptionId)Description) }, +
                { ProductName, $(NoTitle), $(!REG_VT_SZ), +
                    $(MiniportProductName) }, +
                { ServiceName, $(NoTitle), $(!REG_VT_SZ), $($R5) }, +
                { InstallDate, $(NoTitle), $(!REG_VT_DWORD), *($(Now), 1) } }

            shell $(UtilityInf), AddValueList, $(HardNetCardKey), +
                $(NewValueList)
            ifstr(i) $($R0) != NO_ERROR
                closeregkey $(HardNetCardKey)
                closeregkey $(HardNetRuleKey)
                closeregkey $(HardParameterKey)

                shell "" ShowRegistryErrorMessage "FATAL" $($R0)

                return STATUS_FAILED
            endif

            set DeviceId = ""
            LibraryProcedure DeviceId $(HwdtectDll) B57dtectPortIo "PciRd16" +
                $(BusNum) $(DeviceNum) $(FunctionNum) "0x02"
            debug-output "Device Id: "$(DeviceId)

            ; Get subvendor ID.
            LibraryProcedure SubVenId $(HwdtectDll) B57dtectPortIo "PciRd16" +
                $(BusNum) $(DeviceNum) $(FunctionNum) "0x2c"
            debug-output "Subvendor Id: "$(SubVenId)

            ; Get the subsystem id.
            LibraryProcedure SubSysId $(HwdtectDll) B57dtectPortIo "PciRd16" +
                $(BusNum) $(DeviceNum) $(FunctionNum) "0x2e"
            debug-output "Subsystem Id: "$(SubSysId)

            ; Increment the Hpp port number.
            ifstr(i) $(DeviceId) == "0x1645"
                ifstr(i) $(SubVenId) == "0x0e11"
                    ifstr(i) $(SubSysId) == "0x0085"
                        set-add HppPortNum = $(HppPortNum), 1
                    endif
                endif
            endif

            ; Set BCMDID = 0x14e40000 + device ID
            set-hextodec BCMDID = $(DeviceId)
            debug-output "UpdateSection BCMDID: "$(BCMDID)
            set-add BCMDID = 350486528, $(BCMDID)
            debug-output "UpdateSection BCMDID: "$(BCMDID)

            ifstr(i) $(DeviceId) == "0x1645"
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 10  }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 30 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { HppPortNum,           $(NoTitle), $(!REG_VT_DWORD), $(HppPortNum) } +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            else-ifstr(i) $(DeviceId) == "0x1646"
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 10  }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 30 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { WireSpeed,            $(NoTitle), $(!REG_VT_DWORD), 1 } +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            else-ifstr(i) $(DeviceId) == "0x164d"
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 10  }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 30 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { WireSpeed,            $(NoTitle), $(!REG_VT_DWORD), 1 } +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            else-ifstr(i) $(DeviceId) == "0x16a6"
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 10  }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 30 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { WireSpeed,            $(NoTitle), $(!REG_VT_DWORD), 1 } +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            else-ifstr(i) $(DeviceId) == "0x1647"
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 10  }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 30 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { WireSpeed,            $(NoTitle), $(!REG_VT_DWORD), 1 } +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            else-ifstr(i) $(DeviceId) == "0x16a7"
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 10  }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 30 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            else-ifstr(i) $(DeviceId) == "0x1648"
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 10  }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 30 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { WireSpeed,            $(NoTitle), $(!REG_VT_DWORD), 1 } +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            else-ifstr(i) $(DeviceId) == "0x170D"
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 10  }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 30 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { WireSpeed,            $(NoTitle), $(!REG_VT_DWORD), 1 } +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            else
                set NewValueList = { +
                    { BCMDID,               $(NoTitle), $(!REG_VT_DWORD), $(BCMDID) }, +
                    { BusType,              $(NoTitle), $(!REG_VT_DWORD), 5   }, +
                    { BusNumber,            $(NoTitle), $(!REG_VT_DWORD), $(BusNum) }, +
                    { SlotNumber,           $(NoTitle), $(!REG_VT_DWORD), $(DeviceNum) }, +
                    { FunctionNumber,       $(NoTitle), $(!REG_VT_DWORD), $(FunctionNum) }, +
                    { MediaType,            $(NoTitle), $(!REG_VT_DWORD), 1   }, +
                    { TxPacketDescCnt,      $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxStdDescCnt,         $(NoTitle), $(!REG_VT_DWORD), 200 }, +
                    { RxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 360 }, +
                    { TxCoalescingTicks,    $(NoTitle), $(!REG_VT_DWORD), 360 }, +
                    { RxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 15  }, +
                    { TxMaxCoalescedFrames, $(NoTitle), $(!REG_VT_DWORD), 75  }, +
                    { FlowControlCap,       $(NoTitle), $(!REG_VT_DWORD), 0 }, +
                    { RxMtu,                $(NoTitle), $(!REG_VT_DWORD), 1500} +
                    { WireSpeed,            $(NoTitle), $(!REG_VT_DWORD), 1 } +
                    { RequestedMediaType,   $(NoTitle), $(!REG_VT_DWORD), 0 } }
            endif

            debug-output "Write driver params."
            shell $(UtilityInf), AddValueList, $(HardParameterKey), +
                $(NewValueList)
            ifstr(i) $($R0) != NO_ERROR
                debug-output "### Add parameter shell error."

                closeregkey $(HardNetCardKey)
                closeregkey $(HardNetRuleKey)
                closeregkey $(HardParameterKey)

                shell "" ShowRegistryErrorMessage "FATAL" $($R0)

                return STATUS_FAILED
            endif

            set TempProdName = """"$(MiniportProductName)$(AdapterNumber)""""
            set TempBindForm = $(TempProdName)$(MiniportNetRuleHardwareBindForm)

            debug-output "updating netrules."
            set NewValueList = {                                           +
                { type,      $(NoTitle), $(!REG_VT_SZ),                    +
                    $(MiniportNetRuleHardwareType) },                      +
                { bindform,  $(NoTitle), $(!REG_VT_SZ), $(TempBindForm) }, +
                { class,     $(NoTitle), $(!REG_VT_MULTI_SZ),              +
                    $(MiniportNetRuleHardwareClass) },                     +
                { InfOption, $(NoTitle), $(!REG_VT_SZ), $(OptionId)} }

            shell $(UtilityInf), AddValueList, $(HardNetRuleKey), +
                $(NewValueList)
            ifstr(i) $($R0) != NO_ERROR
                debug-output "### Add hardware component error."

                closeregkey $(HardNetCardKey)
                closeregkey $(HardNetRuleKey)
                closeregkey $(HardParameterKey)

                shell "" ShowRegistryErrorMessage "FATAL" $($R0)

                return STATUS_FAILED
            endif

            closeregkey $(HardNetCardKey)
            closeregkey $(HardNetRuleKey)

            ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
                Shell $(UtilityInf), AddDefaultNetCardParameters, +
                    $(HardParameterKey)
            endif

            closeregkey $(HardParameterKey)
        endif

        debug-output ""
    endforlistdo

    FreeLibrary $(HwdtectDll)

    ; Create IBM hot plug PCI service key.
    createregkey $(!REG_H_LOCAL) { $(IBM_HPP_ServiceKey), $(NoTitle), +
        GenericClass } "" $(MAXIMUM_ALLOWED) "" HppKey 
    ifstr(i) $(HppKey) != ""
        set NewValueList = {                                            +
            { DriverServices, $(NoTitle), $(!REG_VT_SZ),                +
                $(MiniportProductName) },                               +
            { FriendlyName,   $(NoTitle), $(!REG_VT_SZ),                +
                $(MiniportProductSoftwareDisplayName) } }

        shell $(UtilityInf), AddValueList, $(HppKey), $(NewValueList)

        closeregkey $(HppKey)
    endif

    ; Create Compaq hot plug PCI key.
    openregkey $(!REG_H_LOCAL) "" $(CPQ_HPP_Key) $(MAXIMUM_ALLOWED) HppKey
    ifstr $(HppKey) == ""
        createregkey $(!REG_H_LOCAL) { $(CPQ_HPP_Key), $(NoTitle), +
            GenericClass } "" $(MAXIMUM_ALLOWED) "" HppKey 

        set NewValueList = {                                            +
            { ClassID, $(NoTitle), $(!REG_VT_SZ), 0 },                  +
            { DLLName,   $(NoTitle), $(!REG_VT_SZ), "CQRNICMN.DLL" } }

        shell $(UtilityInf), AddValueList, $(HppKey), $(NewValueList)
    endif
    closeregkey $(HppKey)

    createregkey $(!REG_H_LOCAL) { $(CPQ_HPP_Key)"\"$(MiniportProductName), +
        $(NoTitle), GenericClass } "" $(MAXIMUM_ALLOWED) "" HppKey 

    set NewValueList = {                                                +
        { BaseOIDAddress, $(NoTitle), $(!REG_VT_DWORD), 4278322176 },   +
        { SetOIDAddress,  $(NoTitle), $(!REG_VT_DWORD), 4278321933 } }

    shell $(UtilityInf), AddValueList, $(HppKey), $(NewValueList)

    closeregkey $(HppKey)

    return STATUS_SUCCESSFUL

