;-----------------------------------
;   VERSION
;-----------------------------------
[VERSION]
Ver=0038

;-----------------------------------
;   PRINTERINFO
;-----------------------------------
[PRINTERINFO]

True1200=NO                         ;YES:1200 DPI machine         NO: 600 DPI machine
ResidentFont=YES                    ;YES:Resident font            NO:No Resident font
Japan=NO                            ;YES:for Japan                NO:Except Japan
A3Printer=NO                        ;YES:A3 printer               NO:A4 printer
NoWatermark=NO                      ;YES:Watermark Setting        NO:No Watermark setting
Duplex=YES                          ;YES:Duplex(possible)         NO:Duplex(impossible)
DirectRaster=NO                     ;YES:Direct Raster Mode       NO:Not direct Raster mode
EnvRotate=YES                       ;YES:Rotation of an envelop   NO:Not Rotation of an envelop
Collate=YES                         ;YES:Support(Collation)       NO:Not support(Collation)
FontSubstitution=YES                ;YES:Font substitution        NO:Font non-substitution
Monochrome=NO                       ;YES:Monochrome fix           NO:Not monochrome fix
ReversePortrait=NO                  ;YES:Default(reverse portrait NO:Default(Not reverse portrait)
MKK=YES                             ;YES:Support MKK              NO:Not support MKK
GL2=YES                             ;YES:Support character rotation(GL2)
                                    ;NO :Not support character rotation(GL2)
Finisher=NO                         ;YES:Support(Finisher)        NO:Not support(Finisher)
WideUserDefinePaper=NO              ;YES:Support(oblong user define)
                                    ;NO :Not support(oblong user define)
MPT_Duplex=YES                      ;YES:Support duplex(MPT)      NO:Not support duplex(MPT)

iLogoBmpID=1
dwDefAvlMemory="3696"
wPPM=12                             ;Color printing speed(PPM)
wModelID=0
Measure=0

wFinisherType="PUNCH.___ + TRAY._____ "     ;Setting for Finisher type
;; EXPLAIN
;;  Please describe '_', when intact.
;;  PUNCH.234
;;        2 ------- Finisher Punch 2Holes
;;         3 ------ Finisher Punch 3Holes
;;          4 ----- Finisher Punch 4Holes
;;
;;  TRAY.12345
;;       1 -------- A setup using a 1st Tray
;;        2 ------- A setup using a 2nd Tray
;;         3 ------ A setup using a 3rd Tray
;;          4 ----- A setup using a 4th Tray
;;           5 ---- A setup using a 5th Tray

;Paper size (for Japan)
PaperOrder=1                        ;Default
PaperSize="23, 0, 1, 2,24, 3, 5, 6,26, 7, 8,27,28,22,25,9,10,11,12,13,30,15,16,20,17,18,19"      ;iPaperOrderPX711

;Paper size (for ODA,for A3 machine,for inch)
PaperOrder_inch=0                   ;Default
PaperSize_inch="5, 6,26, 7, 8,27,28,23, 0, 1, 2,24, 3,22,25,15,16,20,17,18,19"

;Paper size (for OEL,for A3 machine,for mm)
PaperOrder_mm=1                     ;Default
PaperSize_mm="23, 0, 1, 2,24, 3, 5, 6,26, 7, 8,27,28,22,25,15,16,20,17,18,19"

;Paper Source
SourceOrder=0                           ; When a Paper type is set as a default(SourceOrder=-1)
Source="0,7,1,2"                  ; (Paper type and a mix display
                            ;0:DMBIN_AUTO
                            ;1:DMBIN_UPPER
                            ;2:DMBIN_2ND
                            ;3:DMBIN_3RD
                            ;4:DMBIN_4TH
                            ;5:DMBIN_5TH
                            ;6:DMBIN_MMF
                            ;7:DMBIN_MANUAL

;Paper type
PaperTypeOrder=0                        ; Default(for SourceOrder=-1)
PaperType="0,5,1,4,6,7,3,2"             ; (Paper source and a mix display)
                            ;0:PLAIN
                            ;1:LETTERHEAD
                            ;2:TRANSPARENCY
                            ;3:LABELS
                            ;4:BOND
                            ;5:RECYCLED
                            ;6:CARDSTOCK
                            ;7:ROUGH
                            ;8:GLOSSY

;Paper weight
MediatypeOrder=0                        ;Default
MediaType="0,1,3,5,6,9,10,7"
                            ;00:PRINTERSETTING
                            ;01:LIGHT
                            ;02:MEDIUMLIGHT
                            ;03:MEDIUM
                            ;04:MEDIUMHEAVY
                            ;05:HEAVY
                            ;06:ULTRAHEAVY
                            ;07:TRANSPARENCY
                            ;08:CARDSTOCK
                            ;09:LABELS
                            ;10:LABELS2
                            ;11:GLOSSY

;Quality(Job options)
QualityType="2,1,0,-1"  ;Turn to put in order (7 -> 0)
                        ;In the case of three kinds, the 4th is set to -1.
                            ;   DPI         ResolutionOption
                            ;0: DMRES_300,  DMRESOPT_QUICK600x600   //Fast 600x600
                            ;1: DMRES_600,  0                       //600x600
                            ;2: DMRES_600,  DMRESOPT_V1200          //600x1200
                            ;3: DMRES_600,  DMRESOPT_V2400          //600x2400
                            ;4: DMRES_600,  DMRESOPT_QUICK1200x1200 //Fast 1200x1200
                            ;5: DMRES_1200, 0                       //1200x1200
                            ;6: DMRES_600,  DMRESOPT_QUICK1200x2400 //Fast 1200x2400
                            ;7: DMRES_1200, DMRESOPT_V2400          //1200x2400

IntrayType="TRAY.________"

;-----------------------------------
;   PaperSourceType
;-----------------------------------
[PaperSourceType]       ;A4 machine
1 =TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____
2 =TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____
3 =TRAY.1____AM__ + STK.UD + FIN.__ + EJS__L____
4 =TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____
5 =TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
6 =TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____
7 =TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____
8 =TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____
9 =TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____
10=TRAY.1____AM__ + STK.UD + FIN.__ + EJS__L____
11=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
12=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
13=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
14=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
15=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
16=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
17=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
18=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
19=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
20=TRAY.12___AM__ + STK.UD + FIN.__ + EJS__L____
21=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
22=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
23=TRAY.12___AMDF + STK.UD + FIN.__ + EJS__L____
24=TRAY.12___AMDF + STK.UD + FIN.U_ + EJS__L____
25=TRAY.12___AMDF + STK.UD + FIN.U_ + EJS__L____
26=TRAY.12___AMDF + STK.UD + FIN.__ + EJS__L____
27=TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____
28=TRAY.12___AMDF + STK.UD + FIN.U_ + EJS__L____
29=TRAY.12___AMDF + STK.UD + FIN.__ + EJS__L____
30=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
31=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
32=TRAY._____AM__ + STK.UD + FIN.__ + EJS__L____
33=TRAY.12___AM__ + STK.UD + FIN.__ + EJS__L____

;; EXPLAIN
;;  Please describe '_', when intact.
;;  TRAY.12345AMD
;;       1 -------- A setup using a 1st Tray
;;        2 ------- A setup using a 2nd Tray
;;         3 ------ A setup using a 3rd Tray
;;          4 ----- A setup using a 4th Tray
;;           5 ---- A setup using a 5th Tray
;;            A --- A setup using a Automatic Tray Selection
;;             M -- A setup using a MPF and MANUAL Insert
;;              D - A setup using a Duplex Printing
;;
;;  STK.UD
;;      U --------- Upface at the Stacker Eject
;;       D -------- Downface at the Stacker Eject
;;
;;  FIN.UD
;;      U --------- Upface at the Finisher Eject
;;       D -------- Downface at the Finisher Eject
;;
;;  EJS23L23PS
;;     2 ---------- Short Edge Feed 2Punch Holes (UP Face)
;;      3 --------- Short Edge Feed 3Punch Holes (UP Face)
;;        2 ------- Long Edge Feed 2Punch Holes (UP Face)
;;         3 ------ Long Edge Feed 3Punch Holes (UP Face)
;;          P ----- Punch Holes (Down Face)
;;           S ---- Staple (Down Face)

;---------------------------------
;   Font substitution table
;---------------------------------
[SUBSTTABLE]
1=""Arial","Arial",-1"
2=""Times New Roman","Times New",-1"
3=""Symbol","Symbol",-1"
4=""Wingdings","Wingdings",-1"
5=""Courier New","Courier",-1"


;---------------------------------
;   Dither table
;---------------------------------
[DITHER]    ;600dpi machine
UDlpgrayEntryMesh="3,3,2,3,3,2,3,3,2,3,3,2,3,3,2"       ;1:grayM12High,2:grayM16High,3:grayM16Low
UDlpgrayEntryLine="3,3,2,3,3,2,3,3,2,3,3,2,3,3,2"       ;1:grayM12High,2:grayM16High,3:grayM16Low


;---------------------------------
;   Custum size paper
;---------------------------------
[USERFREESIZE]      ;         MAX mm       MAX dot       MIN mm       MIN dot       ;A4 machine
                    ;       x      y      x      y       x     y      x      y
UDDPIChange_Portrait    =" 2159,  3556,  2550,  4200,    640, 1480,   756,  1748"
UDDPIChange_Landscape   =" 3556,  2159,  4200,  2550,   1480,  640,  1748,   756"
UDFreeSize_Portrait     =" 2159, 12000,  2550, 14173,    640, 1480,   756,  1748"
UDFreeSize_Landscape    ="12000,  2159, 14173,  2550,   1480,  640,  1748,   756"
UDFinisherSize_Portrait =" 2970, 12000,  3508, 14173,    640, 1480,   756,  1748"       ;for Finisher
UDFinisherSize_Landscape="12000,  2970, 14173,  3508,   1480,  640,  1748,   756"       ;for Finisher


;-----------------------------------
;   Paper weight(Rebellion)
;-----------------------------------
[AllMediatype]      ;(MediatypePN37)
1 ="TRAY.12___AMD_ + STK.UD + FIN.U_ + EJS__L____"      ;
2 ="TRAY.12_____D_ + STK.UD + FIN.U_ + EJS__L____"      ;
3 ="TRAY.12_____D_ + STK.UD + FIN.U_ + EJS__L____"      ;
4 ="TRAY.12____MD_ + STK.UD + FIN.U_ + EJS__L____"      ;
5 ="TRAY.12____MD_ + STK.UD + FIN.U_ + EJS__L____"      ;
6 ="TRAY.12____MD_ + STK.UD + FIN.U_ + EJS__L____"      ;
7 ="TRAY._2____M__ + STK.UD + FIN.U_ + EJS__L____"      ;
8 ="TRAY.______M__ + STK.UD + FIN.__ + EJS__L____"      ;
9 ="TRAY.______M__ + STK.UD + FIN.__ + EJS__L____"      ;
10="TRAY.______M__ + STK.UD + FIN.__ + EJS__L____"      ;
11="TRAY.______M__ + STK.UD + FIN.__ + EJS__L____"      ;
12="TRAY.______M__ + STK.UD + FIN.__ + EJS__L____"      ;

                            ;1 :PRINTERSETTING
                            ;2 :LIGHT
                            ;3 :MEDIUMLIGHT
                            ;4 :MEDIUM
                            ;5 :MEDIUMHEAVY
                            ;6 :HEAVY
                            ;7 :ULTRAHEAVY
                            ;8 :TRANSPARENCY
                            ;9 :CARDSTOCK
                            ;10:LABELS
                            ;11:LABELS2
                            ;12:GLOSSY

;; EXPLAIN
;;  Please describe '_', when intact.
;;  TRAY.12345AMD
;;       1 -------- A setup using a 1st Tray
;;        2 ------- A setup using a 2nd Tray
;;         3 ------ A setup using a 3rd Tray
;;          4 ----- A setup using a 4th Tray
;;           5 ---- A setup using a 5th Tray
;;            A --- A setup using a Automatic Tray Selection
;;             M -- A setup using a MPF and MANUAL Insert
;;              D - A setup using a Duplex Printing
;;
;;  STK.UD
;;      U --------- Upface at the Stacker Eject
;;       D -------- Downface at the Stacker Eject
;;
;;  FIN.UD
;;      U --------- Upface at the Finisher Eject
;;       D -------- Downface at the Finisher Eject
;;
;;  EJS23L23PS
;;     2 ---------- Short Edge Feed 2Punch Holes (UP Face)
;;      3 --------- Short Edge Feed 3Punch Holes (UP Face)
;;        2 ------- Long Edge Feed 2Punch Holes (UP Face)
;;         3 ------ Long Edge Feed 3Punch Holes (UP Face)
;;          P ----- Punch Holes (Down Face)
;;           S ---- Staple (Down Face)
;;


;-----------------------------------
;   Paper feed option
;-----------------------------------
[PAPER]
UDfitpage=0             ; Fit to Page     0:OFF        1:ON
UDCoverPrint=0          ; Cover printing  0:OFF        1:ON
UDSource_Cover=0        ; Paper source(Cover print)
                        ; (Paper type and a mix display) When a Paper type is set as a default(UDSource_Cover=-1)
UDPaperType_Cover=0     ; Paper type(Cover print)(Paper source and a mix display)
UDCoverPrintThick=0     ; Paper weight(Cover print)
UDDriverSetting_Pinfof=1; Paper information   0:not saved    1:saved


;-----------------------------------
;   Options
;-----------------------------------
[OPTION]
UDSouceOption=0         ; Tray number(0-2,0:1,1:2,2:3)
UDautotray=1            ; Auto tray change     0:NO      1:YES
UDsizechk=1             ; Paper check
UDDuplex=0              ; Duplex Option Unit  0:NO      1:YES
UDHdd=0                 ; Printer Hard Disk   O:Not Hard Disk  1:Hard Disk
UDJobSpool=0            ; Job Spool           0:No Job Spool   1:Job Spool
UDFinisher=0            ; Finisher            0:NO      1:YES


;-----------------------------------
;   Orientation
;-----------------------------------
[ORIENTAION]
UDOrientation=1         ; 1:Portrait    2:Landscape
UDPortDirect=0          ; Portrait rotate     0:NO    1:YES
UDLandDirect=0          ; Landscape rotate    0:NO    1:YES
UDLongEdge=1            ; Long Edge Feed      0:NO    1:YES
UDMPFisManual=0         ; MPT is Manual feed  0:NO    1:YES


;-----------------------------------
;   Copies
;-----------------------------------
[COPIES]
UDCopies=1              ; Copies (1-999)
UDwJobType=0            ; Job type     0:Normal(default),1:Proof and Print,2:Secure Print,3:Spooled Job
UDfCollate=0            ; Collate    0:NO   1:YES


;-----------------------------------
;   Job PIN
;-----------------------------------
[REQUESTEVERY]
UDdwJobTypeOption=0     ;1:Request Job Name for each print job


;-----------------------------------
;   Finisher Mode
;-----------------------------------
[LAYOUTTYPE]
UDdwFinishingMode=0             ; Finishing Mode 0:Standard/N-up,1:booklet,2:Poster Print
UDmultipage=0                   ; 0:1up 1:2up 3:4up 4:8up 5:9up 6:16up
UDdwPageBorder=1                ; Page Borders 0-5 Page Borders 0-5
UDmultiPort=0                   ; Standard/N-up Page layout Portrait 0-3
UDmultiLand=1                   ; Standard/N-up Page layout Landscape 0-3
UDdwSignature=-1                ; Booklet Signature -1:No Limit,1:4 2:8 3:12 4:16
UD2UP=0                         ; Booklet 2pages 0:Not setup  1:setup
UDRightToLeft=0                 ; Booklet Right to Left 0:Left to Right  1:Right to Left
UDEnlarge=0                     ; Poster Print Enlarge 0:2,1:4,2:9,3:Custom
UDRegistMarks=1                 ; Poster Print Add RegstrationMarks 0:No,1:YES
UDdwRegistColor="0x00C0C0C0"    ; Poster Print RegstrationMarks Color 0-7:R,8-15:G,16-23:B,24-31:non
UDOverlap=1                     ; Poster Print Add Overlap 0:No,1:Yes
UDOverlapWidth=100              ; Poster Print Overlap width 0-200 (1/10mm)
UDCstmX=2                       ; Poster Print (Custom)Nimber of Enlarge X (1-4)
UDCstmY=2                       ; Poster Print (Custom)Nimber of Enlarge Y (1-4)
UDDirectionPort=1               ; Poster Print (Custom)Orientation 0:landscape,1:portrait
UDDirectionAuto=1               ; Poster Print (Custom)setup Auto 0:No 1:Yes


;-----------------------------------
;   Other
;-----------------------------------
[ETC]
UDdmScale=100           ; Miscellaneous 25-400
UDBandArea_Nup=0x01     ; Bind margin (for Standard/N-up)
                        ; Not set:0x01 set Left:0x11 set upper:0x12 set Right:0x13 set Lower:0x14
UDBandArea_BookLet=0    ; Bind margin(for BookLet)
                        ; Not set :0   set:0x10
UDBandWidth_Nup=0       ; Bind margin width (for Standard/N-up) 0-300 (1/10mm)
UDBandWidth_BookLet=0   ; Bind margin width (for BookLet) 0-300 (1/10mm)
UDTonerSave=0           ; Job Options-Toner save 0:NO  1:YES


;-----------------------------------
;   Finisher
;-----------------------------------
[FINISHING]
UDOutputBin=0           ; Output Bin 0:Printer Face Down,1:Printer Face Up
UDfFinishingAction=0    ; Staple  0:None  1:Staple  2:Staple+Punch(Across long Edge)  3:Punch(Across Long Edge)  4:Punch(Across Short Edge)


;-----------------------------------
;   2-Sided Printing
;-----------------------------------
[DUPLEX]
UDdmDuplex=1            ; Duplex 1:None  2:Long Edge  3:Short Edge


;-----------------------------------
;   Color
;-----------------------------------
[COLORMODE]
UDcolormode=0           ; Color Mode (0:Auto Color  1:Manual Color  2:Monochrome


;-----------------------------------
;   Color Mode
;-----------------------------------
[COLORMODECOLOR]
UDcoloradjust=0         ; Manual Color(0:Auto  1:Natural  2:Unadjusted)
UDcoloradjustOpt=0      ; Manual Color-Natural(0:Standard Monitor  1:High Brightmess Monitor  2:Digital Camera  3:sRGB  4:Vivid Color)


;-----------------------------------
;   Quality
;-----------------------------------
[RESOLUTION]
UDPrintQuality=-4           ;
                            ; -4 : DMRES_HIGH   (Quality)
                            ; -3 : DMRES_MEDIUM (Normal)
                            ; -2 : DMRES_LOW    (Fast)
                            ; -1 : DMRES_DRAFT  (Intact)


;-----------------------------------
;   Black Finish
;-----------------------------------
[BLACKFINISH]
UDBlackFinish=0             ;Black Finish (0:Auto  1:Gloss  2:Matte)


;-----------------------------------
;   Image Quality
;-----------------------------------
[IMAGEQUALITY]
UDImageThinOut=100      ;Image Quality 100:Hi Quality  66:  50:  33:Hi Speed


;-----------------------------------
;   Advanced
;-----------------------------------
[DETAILSETTING]
UDfDriverExpand=0           ;Advanced Keep Page Layout with Scale Change
UDSpoolEMF=1                ;Advanced Reduce size if spool file
UDTIFF=1                    ;Advanced Compression is done TIFF three bytes (FIX 0)
UDAdjLine=1                 ;Advanced Adjust ultra fine lines
UDRop_MultiColor=0          ;Advanced Express Correcty Drawing of Combine
UDAlMatte=0                 ;Advanced Always create 100% Black(K) Toner
UDfOverPrint=0              ;Advanced Black character is printing over background
UDAP_Collate=1              ;Advanced Priority is given to AP Collation
UDMaintenanceCycle=0        ;Advanced Run maintenance cycle before printing


;-----------------------------------
;   The response of the color function to AP
;-----------------------------------
[APCOLOR]
UDfColor=1                  ;  1:Color  2:Monochrome


;-----------------------------------
;   Print process mode
;-----------------------------------
[PROCESSMODE]
UDColorProcessMode=0        ;0:Printer setting  1:depp(Type1),2:thin(Type2)


;-----------------------------------
;   Watermark
;-----------------------------------
[WATERMARK]
UDwFontSize=72              ; Watermark  size
UDwAngle=45                 ; Watermark  Angle
UDszFont="Arial"            ; Watermark  Font name
UDlfWeight=0                ; Watermark  Font style (bold)
UDlfItalic=0                ; Watermark  Font style (Italics)
UDdwColor="0x00C0C0C0"      ; Watermark  Color  0-7:R,8-15:G,16-23:B,24-31:non
UDxOffset=0                 ; Watermark  Adjustment  x
UDyOffset=0                 ; Watermark  Adjustment  y
UDBasePos=3                 ; Watermark  Position (0:Upper Left  1:Upper Center  2:Upper Right  3:Center  4:Lower Left  5:Lower Center  6:Lower Right
UDWM_XOffset=118            ; Watermark  x base offset
UDWM_YOffset=118            ; Watermark  y base offset
UDTrim=0                    ; Watermark  Trim (0:None  1:Circle  2:Single Frame  3:Duouble Frame)


;-----------------------------------
;   True Type Font Output Type
;-----------------------------------
[FONT]
UDOUTorBIT=1            ;Dounload (0:Outline Font   1:Bitmap Font)
;                       ;Setup by PRTYPE_FONT_SUB in prtype(0x00000080L)


;-----------------------------------
;   Enviroment( for Japan only)
;-----------------------------------
[PCENV]
UDDocContents=0             ; Printing Contents(0:Geberal Document   1:DTP)
UDEnvWarningDlg=0           ; Show Message Box when Enviroment check error(0:NO  1:YES)
UDFreeHdd_General32=6       ; HDD Free Space(MB)(32bit Geberal Document)
UDFreeMem_General32=6       ; Memorry Available(MB)(32bit Geberal Document)
UDFreeHdd_DTP32=20          ; HDD Free Space(MB)(32bit DTP)
UDFreeMem_DTP32=20          ; Memorry Available(MB)(32bit DTP)
UDFreeHdd_General16=6       ; HDD Free Space(MB)(16bit Geberal Document)
UDFreeMem_General16=6       ; Memorry Available(MB)(16bit Geberal Document)
UDFreeHdd_DTP16=20          ; HDD Free Space(MB)(16bit DTP)
UDFreeMem_DTP16=20          ; Memorry Available(MB)(16bit DTP)
UDEnableEnv=0               ; Display Enviroment Button (0:Not Display  1:Display)

;-----------------------------------
;   Color matching
;-----------------------------------
[COLORMATCHING]
Auto_NT=
Auto_NV=
StdMonitor_NT=Natural
StdMonitor_NV=Natural
HighBrightness_NT=Light
HighBrightness_NV=Light
DigitalCamera_NT=DigitalCamera
DigitalCamera_NV=Light
sRGB_NT=sRGB
sRGB_NV=sRGB
Vivid_NT=Vivid
Vivid_NV=Vivid

[COLORMATCHING_FILE]
Natural=OVCCM011.BIN
Vivid=OVCCM012.BIN
Light=OVCCM013.BIN
DigitalCamera=OVCCM014.BIN
sRGB=OVCCM015.BIN

